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For the last decade, Condominiums were constructed and also in the process of construction in different parts of Addis Ababa. The city is going through condominium booms which partly alleviate the housing problem. Most of these condominiums are constructed at the periphery part of the city, further from the city centers, where most of the jobs and services are located. Yet, the public transportation, that many residents depend on to access their jobs is not available in abundance in those suburban locations. Nowadays updated level of public transit coverage in the city of Addis Ababa is not known. As a result, any intervention in this sector cannot be fruitful unless the level of the gap is known scientifically. The purpose of this research is therefore to evaluate the intensity of transit service availability in relationship to neighborhood socio-economic and demographic characteristics in all parts of the city specifically the suburban condominiums of Addis Ababa. Two methods were used in this study. The first method was Addis Ababa bus and LRT service index (ABLSI), this method analyzed Anbessa, Sheger and LRT transit service availability in terms of transit capacity, frequency and coverage score. After standardizing each capacity, frequency and coverage score the results were summed together to produce transit availability index in each 99 transit analysis zones (Woredas) of the city. The second method was simple regression analysis, using this analysis the magnitude of correlation between transit availability index and socio-economic characteristics were identified. Based on the analysis the first method result were identified, it showed that Low and almost no transit service has been available in the periphery condominium residential Woredas whereas in the inner part of the city Woredas low to high public transit service intensity was identified. The second method result also showed that the intensity of transit service availability index has positive relationship with the socio-economic and demographic characteristics of periphery condominium neighborhoods. The study definitely answered regarding to the intensity of public transit availability difference between inner city and periphery Woredas with condominium residential neighborhoods. It also answered the relationship between public transit availability index and socio-economic characteristics of the periphery condominium residential neighborhoods. Further studies are needed for Woredas that have low and almost no transit availability index route design.
Key words: public transit availability index, condominium development, public transit mismatch, socio-economic characteristics

For the last decade, Condominiums were constructed and also in the process of construction in different parts of Addis Ababa. The city is going through condominium booms which partly alleviate the housing problem in the city. Currently large numbers of communities are living in these condominium sites. Most of these condominiums are constructed at the periphery part of the city, further from the city centers, where most of the jobs and services are located. Yet, the public transportation, that many residents depend on to access their jobs is not available in abundance in those suburban locations.
This research, therefore, evaluates condominium development and the intensity of public transit service availability mismatch in Addis Ababa city specifically the periphery condominium residential neighborhoods. The three specific objectives that has been developed to assess the identified problems were; objective one evaluating the availability of transit service in suburban condominium neighborhoods, objective two evaluating the intensity of public transit service difference between the city center and periphery condominium residential areas and objective three evaluating the socio-economic impact of public transit availability at the periphery condominium residential areas. 
In order to achieve the objectives methodologies were developed. The analysis methods used were ABLIA (Addis Ababa bus and LRT index availability) for objective one and two and simple regression analysis method for objective three.
The result of objective one and two were Low and almost no transit service is available in the periphery condominium residential Woredas whereas in the inner part of the city Woredas low to high transit service is identified. The result of the third objective shows that the intensity of transit service availability has strong positive relationship with the socio-economic and demographic characteristics. 
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[bookmark: _Toc11760125][bookmark: _Toc13425731]: IINTRODUCTION
1.1. [bookmark: _Toc11760126][bookmark: _Toc13425732]Background 
 	Ethiopian government outlined an ambitious vision for low-income urban and housing development, formulated as the Integrated Housing Development Program (IHDP), since 2005 (Dejen, 2017). Addis Ababa was the first city which applies this national program. Ingwan et al. (2010) referred that Addis Ababa City Administration launched ambitious low cost condominium housing projects through the Integrated Housing Development Program (IHDP) in 2006. According to Ingwan and others the aim of IHDP was to minimize housing shortage, clear slums and provide decent shelter to middle and low income groups.  Based on Krems (2017) study 180,000 Addis Ababa condominium housing units are transferred to their owners. Addis Ababa city condominium map (2018) shows that; these numbers of housing units are located from 101 condominium sites with around a total of 1806.94hec coverage. According to Ministry of Urban Development and Housing 2019 report, starting from 2006 to 2018 the city administration of Addis Ababa provided the condominium housing units for 176,721 winners of the city dwellers; among the winners 52% are women which are the highest proportion. These communities make trip for different purpose to other part of the city specifically to inner city.
The trip from condominium residential areas to other parts of the city has beenis for social, economic and recreation purpose. To facilitate the trip; public transit services shall should be available in condominium areas with well coverage of transit routes, accessible stops/stations, acceptable frequency and adequate quantity of the service. 
Different public transit services are available in the city of Addis Ababa. According to Addis Ababa city Transport Authority (AACTA) 2018/19 public transport distribution report; Public transit services in the city includes; Anbessa City Bus, Sheger City Bus, Alliance City Bus, Public Service Bus (for civil servant), LRT, Taxi, Minibus and Midi-Bus (Higer & Isuzu). However, this study will focused on only LRT, Anbessa and Sheger city Bus transit services. Because these public transits are financed and administered by the city government which are not profit based transits. In addition, the three transit services are regularly assigned in the provided routes and relatively stick to their schedules than other privately owned public transits that are flexible in their schedules which lacks reliability by the passengers. As a result, for the city of Addis Ababa public transit availability spatial analysis, the three chosen transit services are appropriate to show the intensity of transit service availability at periphery condominiums neighborhoods. These public transit services have their own history, service quality and quantity within city as discussed below.
Among the existing public transit Anbessa bus is the old transit service in the history of the city.  Based on Abreha (2007) study Anbessa Bus Organization started in 1935 (1942 G.C.) by the Ministry of work and communication. Abraha stated that in 1994 the company was renamed as Anbessa City Bus Service following the proclamation number 187/1986 E.C.  According to Anbessa city bus enterprise 2018 annual report; Anbessa had 441 daily City Buses distribution and transported 107,064,171293,326 passengers through the yearper day which is 13 times larger than Sheger bus. It has 124 routes, 1644 stops, 29 stations and 4 depots (Anbessa City Bus enterprise, 2019).
Like Anbessa City Bus, Sheger Mass Transport service is also government financed public transport service. It was started its operation in 2016 (AACTA, 2016). This city Bus has 51 routes and 240 buses (AACTA, 2019). According to AACTA average frequency of public transport and number of passengers’ information from December 15-20/2011E.C. Sheger City Bus transported 21,518 average passengers per day. 
In addition to Anbessa and Sheger bus, currently LRT is one of the dominant public transit services in Addis Ababa. The service was started operation in 2016 with 41 trains and transports 120,000 passengers per day in both N-S and E-W direction (AACTA, 2016). The service has 39 stations with 5 common interchanging stations and two main depots in Hayat and Kality ends. 
Public transit services can be a sound solution for cities with increasing private cars (congestion) and mass residential neighborhoods located at the periphery of the city. According to Kenyon et al. (2002), Benefits of Public transport in comparison to individual transport have more effective energy consumption, reduced traffic accident rates, less traffic congestion and less space demand. Public transport also positively contributes to social integration. The spatial distribution of public transport has importance to link spaces with different activities like that of residence and job opportunity areas. The distribution of public transports cross urban spaces will be characterized by quality and quantity of its service provision. The quality and quantity of service also depended on balance of demand and supply related with street infrastructures (route and station or stops) and numbers of public bus availability. The networks of routes across different spaces (route coverage) will play great role for accessibility of public transport by the passengers. Therefore, provision of the public transport route at the required level, will will help to bring well coverage of public transport service. The study by George and John (2015) support the idea that transport network has a significant role in the development of sustainable, resilient and livable cities. 
Availability of public transport stations or stops within acceptable distance and their spatial locations will also becould be factors for public transport accessibility. Based on Stanislav (2016), accessibility may be characterized as the number of facilities (traffic terminals, stops etc.) available in a certain time or within certain walking distance or for a certain charge. Stanislav also said accessibility of public transport stops may primarily be monitored with consideration of their distribution and location. The availability of adequate public transit on the provided routes will increaseincreases the frequency of getting public transit service from each stations or stops.
Availability of public transportation at the periphery part of Addis Ababa condominium site communities is vital in getting employment, facilitating social interaction, getting better social services and recreational activities at different part of the city. Overall it will helps to facilitate socio-economic and spatial integration of the city. 
The study of this research will focused on identifying the gaps of availability of public transportation service in the periphery part of Addis Ababa condominium residential areas. The study will figured-out the intensity of integration among condominium sites and the availability of public transit by taking into considerations the whole city public transport coverage at woreda level which was the lowest administrative level of the city based on 2007 Addis Ababa city census data. Analyzing the city as whole will helped to show where the service gap has been will be availableavailable and at what level of intensity (high, medium and low service coverage). The intensity of the service can be displayed in maps using GIS from LRT, Anbessa and Sheger transit indexes by correlating with demographic and socio-economic characteristics of woredas. This will will help to make informed decisions and interventions in the public transportation sector of the city either by the government or the private sectors.  


 






	
Figure 1: Anbessa , Sheger and LRT public transit services
	Source: site survey, 2019


[bookmark: _Toc11653940][bookmark: _Toc13246191]Figure 21: condominium sites and public transit routes
[bookmark: _Toc11653941]Source: Addis Ababa city transport authority, 2019.


1.2. [bookmark: _Toc11651253][bookmark: _Toc11651745][bookmark: _Toc11651901][bookmark: _Toc11652468][bookmark: _Toc11652595][bookmark: _Toc11652787][bookmark: _Toc11653444][bookmark: _Toc11653825][bookmark: _Toc11653942][bookmark: _Toc11755844][bookmark: _Toc11755970][bookmark: _Toc11756281][bookmark: _Toc11756697][bookmark: _Toc11756836][bookmark: _Toc11756919][bookmark: _Toc11757138][bookmark: _Toc11757499][bookmark: _Toc11757669][bookmark: _Toc11757841][bookmark: _Toc11757937][bookmark: _Toc11758099][bookmark: _Toc11758245][bookmark: _Toc11758360][bookmark: _Toc11758522][bookmark: _Toc11758604][bookmark: _Toc11758692][bookmark: _Toc11758934][bookmark: _Toc11759019][bookmark: _Toc11760127][bookmark: _Toc11760782][bookmark: _Toc11823799][bookmark: _Toc11831505][bookmark: _Toc11831776][bookmark: _Toc11850630][bookmark: _Toc11851748][bookmark: _Toc11915123][bookmark: _Toc11916348][bookmark: _Toc11922715][bookmark: _Toc13078597][bookmark: _Toc13121367][bookmark: _Toc13121590][bookmark: _Toc13124603][bookmark: _Toc13124851][bookmark: _Toc13125102][bookmark: _Toc13228729][bookmark: _Toc13241026][bookmark: _Toc13241126][bookmark: _Toc13245272][bookmark: _Toc13246823][bookmark: _Toc13425491][bookmark: _Toc13425733]
1.3. [bookmark: _Toc11651254][bookmark: _Toc11651746][bookmark: _Toc11651902][bookmark: _Toc11652469][bookmark: _Toc11652596][bookmark: _Toc11652788][bookmark: _Toc11653445][bookmark: _Toc11653826][bookmark: _Toc11653943][bookmark: _Toc11755845][bookmark: _Toc11755971][bookmark: _Toc11756282][bookmark: _Toc11756698][bookmark: _Toc11756837][bookmark: _Toc11756920][bookmark: _Toc11757139][bookmark: _Toc11757500][bookmark: _Toc11757670][bookmark: _Toc11757842][bookmark: _Toc11757938][bookmark: _Toc11758100][bookmark: _Toc11758246][bookmark: _Toc11758361][bookmark: _Toc11758523][bookmark: _Toc11758605][bookmark: _Toc11758693][bookmark: _Toc11758935][bookmark: _Toc11759020][bookmark: _Toc11760128][bookmark: _Toc11760783][bookmark: _Toc11823800][bookmark: _Toc11831506][bookmark: _Toc11831777][bookmark: _Toc11850631][bookmark: _Toc11851749][bookmark: _Toc11915124][bookmark: _Toc11916349][bookmark: _Toc11922716][bookmark: _Toc13078598][bookmark: _Toc13121368][bookmark: _Toc13121591][bookmark: _Toc13124604][bookmark: _Toc13124852][bookmark: _Toc13125103][bookmark: _Toc13228730][bookmark: _Toc13241027][bookmark: _Toc13241127][bookmark: _Toc13245273][bookmark: _Toc13246824][bookmark: _Toc13425492][bookmark: _Toc13425734]
1.4. [bookmark: _Toc11651255][bookmark: _Toc11651747][bookmark: _Toc11651903][bookmark: _Toc11652470][bookmark: _Toc11652597][bookmark: _Toc11652789][bookmark: _Toc11653446][bookmark: _Toc11653827][bookmark: _Toc11653944][bookmark: _Toc11755846][bookmark: _Toc11755972][bookmark: _Toc11756283][bookmark: _Toc11756699][bookmark: _Toc11756838][bookmark: _Toc11756921][bookmark: _Toc11757140][bookmark: _Toc11757501][bookmark: _Toc11757671][bookmark: _Toc11757843][bookmark: _Toc11757939][bookmark: _Toc11758101][bookmark: _Toc11758247][bookmark: _Toc11758362][bookmark: _Toc11758524][bookmark: _Toc11758606][bookmark: _Toc11758694][bookmark: _Toc11758936][bookmark: _Toc11759021][bookmark: _Toc11760129][bookmark: _Toc11760784][bookmark: _Toc11823801][bookmark: _Toc11831507][bookmark: _Toc11831778][bookmark: _Toc11850632][bookmark: _Toc11851750][bookmark: _Toc11915125][bookmark: _Toc11916350][bookmark: _Toc11922717][bookmark: _Toc13078599][bookmark: _Toc13121369][bookmark: _Toc13121592][bookmark: _Toc13124605][bookmark: _Toc13124853][bookmark: _Toc13125104][bookmark: _Toc13228731][bookmark: _Toc13241028][bookmark: _Toc13241128][bookmark: _Toc13245274][bookmark: _Toc13246825][bookmark: _Toc13425493][bookmark: _Toc13425735]
1.5. [bookmark: _Toc11651256][bookmark: _Toc11651748][bookmark: _Toc11651904][bookmark: _Toc11652471][bookmark: _Toc11652598][bookmark: _Toc11652790][bookmark: _Toc11653447][bookmark: _Toc11653828][bookmark: _Toc11653945][bookmark: _Toc11755847][bookmark: _Toc11755973][bookmark: _Toc11756284][bookmark: _Toc11756700][bookmark: _Toc11756839][bookmark: _Toc11756922][bookmark: _Toc11757141][bookmark: _Toc11757502][bookmark: _Toc11757672][bookmark: _Toc11757844][bookmark: _Toc11757940][bookmark: _Toc11758102][bookmark: _Toc11758248][bookmark: _Toc11758363][bookmark: _Toc11758525][bookmark: _Toc11758607][bookmark: _Toc11758695][bookmark: _Toc11758937][bookmark: _Toc11759022][bookmark: _Toc11760130][bookmark: _Toc11760785][bookmark: _Toc11823802][bookmark: _Toc11831508][bookmark: _Toc11831779][bookmark: _Toc11850633][bookmark: _Toc11851751][bookmark: _Toc11915126][bookmark: _Toc11916351][bookmark: _Toc11922718][bookmark: _Toc13078600][bookmark: _Toc13121370][bookmark: _Toc13121593][bookmark: _Toc13124606][bookmark: _Toc13124854][bookmark: _Toc13125105][bookmark: _Toc13228732][bookmark: _Toc13241029][bookmark: _Toc13241129][bookmark: _Toc13245275][bookmark: _Toc13246826][bookmark: _Toc13425494][bookmark: _Toc13425736]
1.6. [bookmark: _Toc11651257][bookmark: _Toc11651749][bookmark: _Toc11651905][bookmark: _Toc11652472][bookmark: _Toc11652599][bookmark: _Toc11652791][bookmark: _Toc11653448][bookmark: _Toc11653829][bookmark: _Toc11653946][bookmark: _Toc11755848][bookmark: _Toc11755974][bookmark: _Toc11756285][bookmark: _Toc11756701][bookmark: _Toc11756840][bookmark: _Toc11756923][bookmark: _Toc11757142][bookmark: _Toc11757503][bookmark: _Toc11757673][bookmark: _Toc11757845][bookmark: _Toc11757941][bookmark: _Toc11758103][bookmark: _Toc11758249][bookmark: _Toc11758364][bookmark: _Toc11758526][bookmark: _Toc11758608][bookmark: _Toc11758696][bookmark: _Toc11758938][bookmark: _Toc11759023][bookmark: _Toc11760131][bookmark: _Toc11760786][bookmark: _Toc11823803][bookmark: _Toc11831509][bookmark: _Toc11831780][bookmark: _Toc11850634][bookmark: _Toc11851752][bookmark: _Toc11915127][bookmark: _Toc11916352][bookmark: _Toc11922719][bookmark: _Toc13078601][bookmark: _Toc13121371][bookmark: _Toc13121594][bookmark: _Toc13124607][bookmark: _Toc13124855][bookmark: _Toc13125106][bookmark: _Toc13228733][bookmark: _Toc13241030][bookmark: _Toc13241130][bookmark: _Toc13245276][bookmark: _Toc13246827][bookmark: _Toc13425495][bookmark: _Toc13425737]
1.7. [bookmark: _Toc11651258][bookmark: _Toc11651750][bookmark: _Toc11651906][bookmark: _Toc11652473][bookmark: _Toc11652600][bookmark: _Toc11652792][bookmark: _Toc11653449][bookmark: _Toc11653830][bookmark: _Toc11653947][bookmark: _Toc11755849][bookmark: _Toc11755975][bookmark: _Toc11756286][bookmark: _Toc11756702][bookmark: _Toc11756841][bookmark: _Toc11756924][bookmark: _Toc11757143][bookmark: _Toc11757504][bookmark: _Toc11757674][bookmark: _Toc11757846][bookmark: _Toc11757942][bookmark: _Toc11758104][bookmark: _Toc11758250][bookmark: _Toc11758365][bookmark: _Toc11758527][bookmark: _Toc11758609][bookmark: _Toc11758697][bookmark: _Toc11758939][bookmark: _Toc11759024][bookmark: _Toc11760132][bookmark: _Toc11760787][bookmark: _Toc11823804][bookmark: _Toc11831510][bookmark: _Toc11831781][bookmark: _Toc11850635][bookmark: _Toc11851753][bookmark: _Toc11915128][bookmark: _Toc11916353][bookmark: _Toc11922720][bookmark: _Toc13078602][bookmark: _Toc13121372][bookmark: _Toc13121595][bookmark: _Toc13124608][bookmark: _Toc13124856][bookmark: _Toc13125107][bookmark: _Toc13228734][bookmark: _Toc13241031][bookmark: _Toc13241131][bookmark: _Toc13245277][bookmark: _Toc13246828][bookmark: _Toc13425496][bookmark: _Toc13425738]
1.8. [bookmark: _Toc11651259][bookmark: _Toc11651751][bookmark: _Toc11651907][bookmark: _Toc11652474][bookmark: _Toc11652601][bookmark: _Toc11652793][bookmark: _Toc11653450][bookmark: _Toc11653831][bookmark: _Toc11653948][bookmark: _Toc11755850][bookmark: _Toc11755976][bookmark: _Toc11756287][bookmark: _Toc11756703][bookmark: _Toc11756842][bookmark: _Toc11756925][bookmark: _Toc11757144][bookmark: _Toc11757505][bookmark: _Toc11757675][bookmark: _Toc11757847][bookmark: _Toc11757943][bookmark: _Toc11758105][bookmark: _Toc11758251][bookmark: _Toc11758366][bookmark: _Toc11758528][bookmark: _Toc11758610][bookmark: _Toc11758698][bookmark: _Toc11758940][bookmark: _Toc11759025][bookmark: _Toc11760133][bookmark: _Toc11760788][bookmark: _Toc11823805][bookmark: _Toc11831511][bookmark: _Toc11831782][bookmark: _Toc11850636][bookmark: _Toc11851754][bookmark: _Toc11915129][bookmark: _Toc11916354][bookmark: _Toc11922721][bookmark: _Toc13078603][bookmark: _Toc13121373][bookmark: _Toc13121596][bookmark: _Toc13124609][bookmark: _Toc13124857][bookmark: _Toc13125108][bookmark: _Toc13228735][bookmark: _Toc13241032][bookmark: _Toc13241132][bookmark: _Toc13245278][bookmark: _Toc13246829][bookmark: _Toc13425497][bookmark: _Toc13425739]
1.9. [bookmark: _Toc11651260][bookmark: _Toc11651752][bookmark: _Toc11651908][bookmark: _Toc11652475][bookmark: _Toc11652602][bookmark: _Toc11652794][bookmark: _Toc11653451][bookmark: _Toc11653832][bookmark: _Toc11653949][bookmark: _Toc11755851][bookmark: _Toc11755977][bookmark: _Toc11756288][bookmark: _Toc11756704][bookmark: _Toc11756843][bookmark: _Toc11756926][bookmark: _Toc11757145][bookmark: _Toc11757506][bookmark: _Toc11757676][bookmark: _Toc11757848][bookmark: _Toc11757944][bookmark: _Toc11758106][bookmark: _Toc11758252][bookmark: _Toc11758367][bookmark: _Toc11758529][bookmark: _Toc11758611][bookmark: _Toc11758699][bookmark: _Toc11758941][bookmark: _Toc11759026][bookmark: _Toc11760134][bookmark: _Toc11760789][bookmark: _Toc11823806][bookmark: _Toc11831512][bookmark: _Toc11831783][bookmark: _Toc11850637][bookmark: _Toc11851755][bookmark: _Toc11915130][bookmark: _Toc11916355][bookmark: _Toc11922722][bookmark: _Toc13078604][bookmark: _Toc13121374][bookmark: _Toc13121597][bookmark: _Toc13124610][bookmark: _Toc13124858][bookmark: _Toc13125109][bookmark: _Toc13228736][bookmark: _Toc13241033][bookmark: _Toc13241133][bookmark: _Toc13245279][bookmark: _Toc13246830][bookmark: _Toc13425498][bookmark: _Toc13425740]
1.10. [bookmark: _Toc11651261][bookmark: _Toc11651753][bookmark: _Toc11651909][bookmark: _Toc11652476][bookmark: _Toc11652603][bookmark: _Toc11652795][bookmark: _Toc11653452][bookmark: _Toc11653833][bookmark: _Toc11653950][bookmark: _Toc11755852][bookmark: _Toc11755978][bookmark: _Toc11756289][bookmark: _Toc11756705][bookmark: _Toc11756844][bookmark: _Toc11756927][bookmark: _Toc11757146][bookmark: _Toc11757507][bookmark: _Toc11757677][bookmark: _Toc11757849][bookmark: _Toc11757945][bookmark: _Toc11758107][bookmark: _Toc11758253][bookmark: _Toc11758368][bookmark: _Toc11758530][bookmark: _Toc11758612][bookmark: _Toc11758700][bookmark: _Toc11758942][bookmark: _Toc11759027][bookmark: _Toc11760135][bookmark: _Toc11760790][bookmark: _Toc11823807][bookmark: _Toc11831513][bookmark: _Toc11831784][bookmark: _Toc11850638][bookmark: _Toc11851756][bookmark: _Toc11915131][bookmark: _Toc11916356][bookmark: _Toc11922723][bookmark: _Toc13078605][bookmark: _Toc13121375][bookmark: _Toc13121598][bookmark: _Toc13124611][bookmark: _Toc13124859][bookmark: _Toc13125110][bookmark: _Toc13228737][bookmark: _Toc13241034][bookmark: _Toc13241134][bookmark: _Toc13245280][bookmark: _Toc13246831][bookmark: _Toc13425499][bookmark: _Toc13425741]
1.11. [bookmark: _Toc11651262][bookmark: _Toc11651754][bookmark: _Toc11651910][bookmark: _Toc11652477][bookmark: _Toc11652604][bookmark: _Toc11652796][bookmark: _Toc11653453][bookmark: _Toc11653834][bookmark: _Toc11653951][bookmark: _Toc11755853][bookmark: _Toc11755979][bookmark: _Toc11756290][bookmark: _Toc11756706][bookmark: _Toc11756845][bookmark: _Toc11756928][bookmark: _Toc11757147][bookmark: _Toc11757508][bookmark: _Toc11757678][bookmark: _Toc11757850][bookmark: _Toc11757946][bookmark: _Toc11758108][bookmark: _Toc11758254][bookmark: _Toc11758369][bookmark: _Toc11758531][bookmark: _Toc11758613][bookmark: _Toc11758701][bookmark: _Toc11758943][bookmark: _Toc11759028][bookmark: _Toc11760136][bookmark: _Toc11760791][bookmark: _Toc11823808][bookmark: _Toc11831514][bookmark: _Toc11831785][bookmark: _Toc11850639][bookmark: _Toc11851757][bookmark: _Toc11915132][bookmark: _Toc11916357][bookmark: _Toc11922724][bookmark: _Toc13078606][bookmark: _Toc13121376][bookmark: _Toc13121599][bookmark: _Toc13124612][bookmark: _Toc13124860][bookmark: _Toc13125111][bookmark: _Toc13228738][bookmark: _Toc13241035][bookmark: _Toc13241135][bookmark: _Toc13245281][bookmark: _Toc13246832][bookmark: _Toc13425500][bookmark: _Toc13425742]
1.12. [bookmark: _Toc11651263][bookmark: _Toc11651755][bookmark: _Toc11651911][bookmark: _Toc11652478][bookmark: _Toc11652605][bookmark: _Toc11652797][bookmark: _Toc11653454][bookmark: _Toc11653835][bookmark: _Toc11653952][bookmark: _Toc11755854][bookmark: _Toc11755980][bookmark: _Toc11756291][bookmark: _Toc11756707][bookmark: _Toc11756846][bookmark: _Toc11756929][bookmark: _Toc11757148][bookmark: _Toc11757509][bookmark: _Toc11757679][bookmark: _Toc11757851][bookmark: _Toc11757947][bookmark: _Toc11758109][bookmark: _Toc11758255][bookmark: _Toc11758370][bookmark: _Toc11758532][bookmark: _Toc11758614][bookmark: _Toc11758702][bookmark: _Toc11758944][bookmark: _Toc11759029][bookmark: _Toc11760137][bookmark: _Toc11760792][bookmark: _Toc11823809][bookmark: _Toc11831515][bookmark: _Toc11831786][bookmark: _Toc11850640][bookmark: _Toc11851758][bookmark: _Toc11915133][bookmark: _Toc11916358][bookmark: _Toc11922725][bookmark: _Toc13078607][bookmark: _Toc13121377][bookmark: _Toc13121600][bookmark: _Toc13124613][bookmark: _Toc13124861][bookmark: _Toc13125112][bookmark: _Toc13228739][bookmark: _Toc13241036][bookmark: _Toc13241136][bookmark: _Toc13245282][bookmark: _Toc13246833][bookmark: _Toc13425501][bookmark: _Toc13425743]
1.13. [bookmark: _Toc11651264][bookmark: _Toc11651756][bookmark: _Toc11651912][bookmark: _Toc11652479][bookmark: _Toc11652606][bookmark: _Toc11652798][bookmark: _Toc11653455][bookmark: _Toc11653836][bookmark: _Toc11653953][bookmark: _Toc11755855][bookmark: _Toc11755981][bookmark: _Toc11756292][bookmark: _Toc11756708][bookmark: _Toc11756847][bookmark: _Toc11756930][bookmark: _Toc11757149][bookmark: _Toc11757510][bookmark: _Toc11757680][bookmark: _Toc11757852][bookmark: _Toc11757948][bookmark: _Toc11758110][bookmark: _Toc11758256][bookmark: _Toc11758371][bookmark: _Toc11758533][bookmark: _Toc11758615][bookmark: _Toc11758703][bookmark: _Toc11758945][bookmark: _Toc11759030][bookmark: _Toc11760138][bookmark: _Toc11760793][bookmark: _Toc11823810][bookmark: _Toc11831516][bookmark: _Toc11831787][bookmark: _Toc11850641][bookmark: _Toc11851759][bookmark: _Toc11915134][bookmark: _Toc11916359][bookmark: _Toc11922726][bookmark: _Toc13078608][bookmark: _Toc13121378][bookmark: _Toc13121601][bookmark: _Toc13124614][bookmark: _Toc13124862][bookmark: _Toc13125113][bookmark: _Toc13228740][bookmark: _Toc13241037][bookmark: _Toc13241137][bookmark: _Toc13245283][bookmark: _Toc13246834][bookmark: _Toc13425502][bookmark: _Toc13425744]
1.14. [bookmark: _Toc11651265][bookmark: _Toc11651757][bookmark: _Toc11651913][bookmark: _Toc11652480][bookmark: _Toc11652607][bookmark: _Toc11652799][bookmark: _Toc11653456][bookmark: _Toc11653837][bookmark: _Toc11653954][bookmark: _Toc11755856][bookmark: _Toc11755982][bookmark: _Toc11756293][bookmark: _Toc11756709][bookmark: _Toc11756848][bookmark: _Toc11756931][bookmark: _Toc11757150][bookmark: _Toc11757511][bookmark: _Toc11757681][bookmark: _Toc11757853][bookmark: _Toc11757949][bookmark: _Toc11758111][bookmark: _Toc11758257][bookmark: _Toc11758372][bookmark: _Toc11758534][bookmark: _Toc11758616][bookmark: _Toc11758704][bookmark: _Toc11758946][bookmark: _Toc11759031][bookmark: _Toc11760139][bookmark: _Toc11760794][bookmark: _Toc11823811][bookmark: _Toc11831517][bookmark: _Toc11831788][bookmark: _Toc11850642][bookmark: _Toc11851760][bookmark: _Toc11915135][bookmark: _Toc11916360][bookmark: _Toc11922727][bookmark: _Toc13078609][bookmark: _Toc13121379][bookmark: _Toc13121602][bookmark: _Toc13124615][bookmark: _Toc13124863][bookmark: _Toc13125114][bookmark: _Toc13228741][bookmark: _Toc13241038][bookmark: _Toc13241138][bookmark: _Toc13245284][bookmark: _Toc13246835][bookmark: _Toc13425503][bookmark: _Toc13425745]
1.15. [bookmark: _Toc11651266][bookmark: _Toc11651758][bookmark: _Toc11651914][bookmark: _Toc11652481][bookmark: _Toc11652608][bookmark: _Toc11652800][bookmark: _Toc11653457][bookmark: _Toc11653838][bookmark: _Toc11653955][bookmark: _Toc11755857][bookmark: _Toc11755983][bookmark: _Toc11756294][bookmark: _Toc11756710][bookmark: _Toc11756849][bookmark: _Toc11756932][bookmark: _Toc11757151][bookmark: _Toc11757512][bookmark: _Toc11757682][bookmark: _Toc11757854][bookmark: _Toc11757950][bookmark: _Toc11758112][bookmark: _Toc11758258][bookmark: _Toc11758373][bookmark: _Toc11758535][bookmark: _Toc11758617][bookmark: _Toc11758705][bookmark: _Toc11758947][bookmark: _Toc11759032][bookmark: _Toc11760140][bookmark: _Toc11760795][bookmark: _Toc11823812][bookmark: _Toc11831518][bookmark: _Toc11831789][bookmark: _Toc11850643][bookmark: _Toc11851761][bookmark: _Toc11915136][bookmark: _Toc11916361][bookmark: _Toc11922728][bookmark: _Toc13078610][bookmark: _Toc13121380][bookmark: _Toc13121603][bookmark: _Toc13124616][bookmark: _Toc13124864][bookmark: _Toc13125115][bookmark: _Toc13228742][bookmark: _Toc13241039][bookmark: _Toc13241139][bookmark: _Toc13245285][bookmark: _Toc13246836][bookmark: _Toc13425504][bookmark: _Toc13425746]
1.16. [bookmark: _Toc11651267][bookmark: _Toc11651759][bookmark: _Toc11651915][bookmark: _Toc11652482][bookmark: _Toc11652609][bookmark: _Toc11652801][bookmark: _Toc11653458][bookmark: _Toc11653839][bookmark: _Toc11653956][bookmark: _Toc11755858][bookmark: _Toc11755984][bookmark: _Toc11756295][bookmark: _Toc11756711][bookmark: _Toc11756850][bookmark: _Toc11756933][bookmark: _Toc11757152][bookmark: _Toc11757513][bookmark: _Toc11757683][bookmark: _Toc11757855][bookmark: _Toc11757951][bookmark: _Toc11758113][bookmark: _Toc11758259][bookmark: _Toc11758374][bookmark: _Toc11758536][bookmark: _Toc11758618][bookmark: _Toc11758706][bookmark: _Toc11758948][bookmark: _Toc11759033][bookmark: _Toc11760141][bookmark: _Toc11760796][bookmark: _Toc11823813][bookmark: _Toc11831519][bookmark: _Toc11831790][bookmark: _Toc11850644][bookmark: _Toc11851762][bookmark: _Toc11915137][bookmark: _Toc11916362][bookmark: _Toc11922729][bookmark: _Toc13078611][bookmark: _Toc13121381][bookmark: _Toc13121604][bookmark: _Toc13124617][bookmark: _Toc13124865][bookmark: _Toc13125116][bookmark: _Toc13228743][bookmark: _Toc13241040][bookmark: _Toc13241140][bookmark: _Toc13245286][bookmark: _Toc13246837][bookmark: _Toc13425505][bookmark: _Toc13425747]
1.17. [bookmark: _Toc11651268][bookmark: _Toc11651760][bookmark: _Toc11651916][bookmark: _Toc11652483][bookmark: _Toc11652610][bookmark: _Toc11652802][bookmark: _Toc11653459][bookmark: _Toc11653840][bookmark: _Toc11653957][bookmark: _Toc11755859][bookmark: _Toc11755985][bookmark: _Toc11756296][bookmark: _Toc11756712][bookmark: _Toc11756851][bookmark: _Toc11756934][bookmark: _Toc11757153][bookmark: _Toc11757514][bookmark: _Toc11757684][bookmark: _Toc11757856][bookmark: _Toc11757952][bookmark: _Toc11758114][bookmark: _Toc11758260][bookmark: _Toc11758375][bookmark: _Toc11758537][bookmark: _Toc11758619][bookmark: _Toc11758707][bookmark: _Toc11758949][bookmark: _Toc11759034][bookmark: _Toc11760142][bookmark: _Toc11760797][bookmark: _Toc11823814][bookmark: _Toc11831520][bookmark: _Toc11831791][bookmark: _Toc11850645][bookmark: _Toc11851763][bookmark: _Toc11915138][bookmark: _Toc11916363][bookmark: _Toc11922730][bookmark: _Toc13078612][bookmark: _Toc13121382][bookmark: _Toc13121605][bookmark: _Toc13124618][bookmark: _Toc13124866][bookmark: _Toc13125117][bookmark: _Toc13228744][bookmark: _Toc13241041][bookmark: _Toc13241141][bookmark: _Toc13245287][bookmark: _Toc13246838][bookmark: _Toc13425506][bookmark: _Toc13425748]
1.18. [bookmark: _Toc11651269][bookmark: _Toc11651761][bookmark: _Toc11651917][bookmark: _Toc11652484][bookmark: _Toc11652611][bookmark: _Toc11652803][bookmark: _Toc11653460][bookmark: _Toc11653841][bookmark: _Toc11653958][bookmark: _Toc11755860][bookmark: _Toc11755986][bookmark: _Toc11756297][bookmark: _Toc11756713][bookmark: _Toc11756852][bookmark: _Toc11756935][bookmark: _Toc11757154][bookmark: _Toc11757515][bookmark: _Toc11757685][bookmark: _Toc11757857][bookmark: _Toc11757953][bookmark: _Toc11758115][bookmark: _Toc11758261][bookmark: _Toc11758376][bookmark: _Toc11758538][bookmark: _Toc11758620][bookmark: _Toc11758708][bookmark: _Toc11758950][bookmark: _Toc11759035][bookmark: _Toc11760143][bookmark: _Toc11760798][bookmark: _Toc11823815][bookmark: _Toc11831521][bookmark: _Toc11831792][bookmark: _Toc11850646][bookmark: _Toc11851764][bookmark: _Toc11915139][bookmark: _Toc11916364][bookmark: _Toc11922731][bookmark: _Toc13078613][bookmark: _Toc13121383][bookmark: _Toc13121606][bookmark: _Toc13124619][bookmark: _Toc13124867][bookmark: _Toc13125118][bookmark: _Toc13228745][bookmark: _Toc13241042][bookmark: _Toc13241142][bookmark: _Toc13245288][bookmark: _Toc13246839][bookmark: _Toc13425507][bookmark: _Toc13425749]
1.19. [bookmark: _Toc11651270][bookmark: _Toc11651762][bookmark: _Toc11651918][bookmark: _Toc11652485][bookmark: _Toc11652612][bookmark: _Toc11652804][bookmark: _Toc11653461][bookmark: _Toc11653842][bookmark: _Toc11653959][bookmark: _Toc11755861][bookmark: _Toc11755987][bookmark: _Toc11756298][bookmark: _Toc11756714][bookmark: _Toc11756853][bookmark: _Toc11756936][bookmark: _Toc11757155][bookmark: _Toc11757516][bookmark: _Toc11757686][bookmark: _Toc11757858][bookmark: _Toc11757954][bookmark: _Toc11758116][bookmark: _Toc11758262][bookmark: _Toc11758377][bookmark: _Toc11758539][bookmark: _Toc11758621][bookmark: _Toc11758709][bookmark: _Toc11758951][bookmark: _Toc11759036][bookmark: _Toc11760144][bookmark: _Toc11760799][bookmark: _Toc11823816][bookmark: _Toc11831522][bookmark: _Toc11831793][bookmark: _Toc11850647][bookmark: _Toc11851765][bookmark: _Toc11915140][bookmark: _Toc11916365][bookmark: _Toc11922732][bookmark: _Toc13078614][bookmark: _Toc13121384][bookmark: _Toc13121607][bookmark: _Toc13124620][bookmark: _Toc13124868][bookmark: _Toc13125119][bookmark: _Toc13228746][bookmark: _Toc13241043][bookmark: _Toc13241143][bookmark: _Toc13245289][bookmark: _Toc13246840][bookmark: _Toc13425508][bookmark: _Toc13425750]
1.20. [bookmark: _Toc11651271][bookmark: _Toc11651763][bookmark: _Toc11651919][bookmark: _Toc11652486][bookmark: _Toc11652613][bookmark: _Toc11652805][bookmark: _Toc11653462][bookmark: _Toc11653843][bookmark: _Toc11653960][bookmark: _Toc11755862][bookmark: _Toc11755988][bookmark: _Toc11756299][bookmark: _Toc11756715][bookmark: _Toc11756854][bookmark: _Toc11756937][bookmark: _Toc11757156][bookmark: _Toc11757517][bookmark: _Toc11757687][bookmark: _Toc11757859][bookmark: _Toc11757955][bookmark: _Toc11758117][bookmark: _Toc11758263][bookmark: _Toc11758378][bookmark: _Toc11758540][bookmark: _Toc11758622][bookmark: _Toc11758710][bookmark: _Toc11758952][bookmark: _Toc11759037][bookmark: _Toc11760145][bookmark: _Toc11760800][bookmark: _Toc11823817][bookmark: _Toc11831523][bookmark: _Toc11831794][bookmark: _Toc11850648][bookmark: _Toc11851766][bookmark: _Toc11915141][bookmark: _Toc11916366][bookmark: _Toc11922733][bookmark: _Toc13078615][bookmark: _Toc13121385][bookmark: _Toc13121608][bookmark: _Toc13124621][bookmark: _Toc13124869][bookmark: _Toc13125120][bookmark: _Toc13228747][bookmark: _Toc13241044][bookmark: _Toc13241144][bookmark: _Toc13245290][bookmark: _Toc13246841][bookmark: _Toc13425509][bookmark: _Toc13425751]
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1.25. [bookmark: _Toc11760150][bookmark: _Toc13425756]Pproblem statement 
For the last decade, Condominiums were constructed and also in the process of construction in different parts of Addis Ababa. The city is going through condominium booms which partly alleviate the housing problem in the city. Currently large numbers of communities are living in these condominium sites. Most of the condominiums are constructed at the periphery part of the city, further from the city centers, where most of the jobs are located. According to Hassan et al. (2018) in Addis Ababa, some of the new government-built condominium housing is located near the city center, but much of it has been built on the geographical margins of the city. Yet, the public transportation, that many residents depend on to access their jobs is not available in abundance in those suburban locations.
Communities who are living in the condominium areas are working in the inner part of the city. There were also communities relocated to the periphery condominium sites in due to urban renewal programs whose livelihood is directly depend on inner city.  The renewal took place in the sub-cities of Lideta, Kirkos, Arada, and Addis Ketema which are part of the inner city (UN- Habitat, 2017). The relocated communities’ livelihoods were dependent on these inner city areas (Hassan et al., 2018). When these communities resettled in the periphery part of the city condominiums they lost their social and economic activities because mostly these condominium sites provide dormitory function. As a result, to do their job they move to inner part of the city during the day time and back to home during night time. However, to accomplish their daily task transportation is a great challenge because these residential sites are not well provided with public transportation (Fenta, 2014). According to Hassan and others (2018) study, the periphery condominium residents monthly expenses is rising without secured income and they cannot afford the costs of privately administered transportation services from the condominium to work in the city center. As a result, there is public transportation demand at the periphery part of the city but the demand and supply of the public transport service is not balanced.  According to Fenta (2014) “Addis Ababa faces various problems including insufficient and poor quality of public transport. That means the existing public transport system in Addis Ababa is critically inadequate to provide service for the increasing travel demand of the city, because the number of cars providing the service is not sufficient”. As a result, there is less integration of public transit and condominium development with less accessible and reliable service provision. From the reliability perspective the transit is not available any time, regularity is not satisfactory because of long waiting time at transit stops, operational speed or trip time is long because of congestion and the public transportations not having segregated lane. 
This indicates the city has been developed with unplanned housing and transportation service balance that links residents to job, school and shopping area which results spatial mismatch between these different activity spaces. This also has its own negative social and economic influences on condominium dwellers in the suburban area of the city.
1.26. [bookmark: _Toc11760151][bookmark: _Toc13425757]General objective 
The purpose of this research is to evaluate the gaps of the availability of transit service in relationship to neighborhood socio-economic and demographic characteristics in the city of Addis Ababa specifically in the suburban condominiums parts of Addis Ababa. Nowadays updated level of public transit coverage in the city of Addis Ababa is not known. As a result, any intervention in this sector could not been fruitful unless the level of the gap is known scientifically. Therefore, this study  shows which part of the city has high, medium and low level of public transit. It also shows which demographic (population size, age and gender) and socio-economic (labor force and income level) characteristics lies in high, medium and low level of intensity of public transit service. At the end the purpose of this study is to show which condominium sites are well covered or not by the public transit service in comparison. with the whole part of the city.
1.26.1. [bookmark: _Toc11757694][bookmark: _Toc11757866][bookmark: _Toc11757962][bookmark: _Toc11758124][bookmark: _Toc11758270][bookmark: _Toc11758385][bookmark: _Toc11758547][bookmark: _Toc11758629][bookmark: _Toc11758717][bookmark: _Toc11758959][bookmark: _Toc11759044][bookmark: _Toc11760152][bookmark: _Toc11760807][bookmark: _Toc11823824][bookmark: _Toc11831530][bookmark: _Toc11831801][bookmark: _Toc11850655][bookmark: _Toc11851773][bookmark: _Toc11915148][bookmark: _Toc11916373][bookmark: _Toc11922740][bookmark: _Toc13078622][bookmark: _Toc13121392][bookmark: _Toc13121615][bookmark: _Toc13124628][bookmark: _Toc13124876][bookmark: _Toc13125127][bookmark: _Toc13228754][bookmark: _Toc13241051][bookmark: _Toc13241151][bookmark: _Toc13245297][bookmark: _Toc13246848][bookmark: _Toc13425516][bookmark: _Toc13425758]
1.26.2. [bookmark: _Toc11760153][bookmark: _Toc13425759]SpecificSpecific objectives
· To eEvaluateing the availability of transit service in suburban condominium neighborhoods.
· To eEvaluatinge the intensity of public transit service difference between the city center and periphery condominium residential areas.
· To Evaluating identify the socio-economic and demographic impact of public transit availability at the periphery condominium residential areas.
1.27. 1.4. Hypothesis 
When there is adequate number of public transit services, routes and stations or stops distributed across the city, then it brings more employed labor force, better income level for the community, more aged people and women in social and economic activity in condominium residential neighborhoods.
1.28. [bookmark: _Toc11760155][bookmark: _Toc13425762] 1.5. Research question
· How public transits (services, route and stops) are spatially distributed and connected to periphery condominium residential areas?
· Are there major differences between the city centers and the suburban condominium neighborhoods related with availability of transit service?
· In what way does the public transit availability benefit affect the socio-economic and demographic aspect of the study area?
1.29. [bookmark: _Toc11760156][bookmark: _Toc13425763] 1.6. Significance of study
The study shows the public transport service gap intensity in periphery condominium residential areas in map, charts and tables. This helps for the city administration, policy makers and private investors to make informed decisions and interventions in the public transportation sector. Therefore, for the city administration the study gives clear image about the availability of spatial coverage of public transit route and the provided service quality and quantity at each transit analysis zone. As discussed on the above the study would also help private sectors to invest in transportation sector to fill the available service gap without hesitation. It also helps policy makers to update the current policy related with existing reality of public transportation based on the recommendation of the study. 
1.30. [bookmark: _Toc11760157][bookmark: _Toc13425764]1.7.  Scope of the study
The study evaluateds the whole Addis Ababaentire city Anbessa, Sheger and LRT public transport spatial coverage at the woreda level which was the smallest administrative unit of the city based on 2007 census data of Addis Ababa. Much more it focuses on condominium areas specifically the periphery part of the city. These periphery condominiums are Asco, Mikelely Land, Jemo, Mekanissa Kotari, KaraKore, Tulu Dimtu, Gelan, Kilinto, Bole Bulbula, Yeka Abado, Yeka Ayat, Bole Ayat, Bole Arabsa, Bole Lemi,etc. Moreover, it assesseds availability of number of buses and LRT trams, stops, carrying capacity, route coverage and frequency of buses and LRT trams at each stop within each woreda traffic analysis zones. In addition, tThe transit availability wasis assessed in comparison with the number of population (socio-economic & demographic characteristics) and area coverage of the woreda which is was taken as a traffic analysis zone.
1.31. [bookmark: _Toc11760158][bookmark: _Toc13425765] 1.8. LimitationLimitation of the study
The traffic analysis zone which is in our case woreda  limits(Woreda) limits the study. Because this woreda was based on 2007 census data and there wasis no recent census data after 2007 that considers the recent woreda administrative level. There is also 2016 socio-economic data limitation because this data was collected at sub-city level by CSA.  Therefore, census data is also a major limiting factor in this study. Time is another limiting factor for this research to deal with primary data. As a result, the research used only secondary data.
1.32. [bookmark: _Toc11760159][bookmark: _Toc13425766] 1.9. Organization of the research
The study contains five chapters. Chapter one provides with an introduction part of the paper. The chapter highlights background of the study, the research problems and questions, purpose of the study, objectives, significance, scope, limitation and organization of the paper. The second chapter provides a literature review which is based on a survey of previous studies in this research field. It mainly focuses on condominium development, public transit availability, spatial coverage and connectivity of transit route as well as transit service in urban areas. ; it also tries to focus on condominium developments and public transport integration mismatch. This chapter also presents theories and principles that are relevant to the present study. Chapter three discusediscusseds about backgrounds of the study area. Chapter four focus on research methodology that was used to collect and analyze the data. Chapter five discusses about result and discussion. Chapter six discusses about conclusion and recommendation. 
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[bookmark: _Toc11760161][bookmark: _Toc13425768]LITRATURE REVIEW
2.1. [bookmark: _Toc1579186][bookmark: _Toc11760162][bookmark: _Toc13425769]2.1. General description
The literature review discussed issues that are related with housing (condominium) development and public transit service (transit service availability, spatial coverage and transit mismatch) as well as socio economic and demographic impact of availability of public transit. Important words are defined based on the contextual meaning accordingly.

Condominium: it means a building for residential or other purpose with five or more separately owned units and common elements (all that are part of the condominium except the units), in a high-rise building or in a row of houses, and includes the land holding of the building  
(FederaL Negarit Gazeta, 2003).
Public transit: it is a motorized mode of transport which includes trains, trams and buses operating on fixed linear routes connecting a number of stops in series that together form a network of transport systems. The size and the capacity of transit system differsdiffer according to the particular mode and context (Tesfaye, 2012).
Public transit spatial coverage: is public transit service within reasonable physical proximity to traveler’s home/destination (Al Mamun & Lownes, 2011).
Public transit availability: it is how easily passengers can access and use transit service service(TCQSM, 2003).. It is the measure of public transportation service intensity at the local level (Woldeamanuel & Covington, 2010).
Armstrong and Thiriez (1987) stated that, public transportation is a key component of a sustainable transportation system that helps mobility (movement of people, goods and services)  without harming the economy and environment. As a result, public transport in urban areas has gained greater attention in recent years for improving sustainability and the quality of urban life (Bok, 2016).  The economic and environmental performance of cities can be enhanced by connecting resources to destinations effectively and facilitating mass mobility (Bok, 2016). According to Armstrong and Thiriez public transportation also decreases the increased auto ownership and insures long term sustainability in terms of resource consumption by relieving highway congestion and provides a very efficient means of moving large numbers of people.
Bok (2016) study shows that, public transport in urban areas has gained greater attention in recent years for improving sustainability and the quality of urban life. The economic and environmental performance of cities can be enhanced by connecting resources to destinations effectively and facilitating mass mobility (Bok, 2016). Based on Ross (2012) study public transit is a key component of the economic and social fabric of metropolitan areas. According to Armstrong and Thiriez (1987)  public transportation also decreases the increased auto ownership and insures long term sustainability in terms of resource consumption by relieving highway congestion and provides a very efficient means of moving large numbers of people. Ross also said Therefore, commuting to work is one purpose of trip residents may use a transit system (Ross, 2012). According to this scholarRoss study commuters make up the largest share of transit trips nationwide. However, to transport people, goods and services without adequate infrastructure is unthinkable. 
As Moreno (2016) discussed in his study that, public transportation cannot be functional without transport infrastructure. Based on Yatskiv et al. (2017) study availability of public transport infrastructure is a vital factor in providing an attractive public transport with door to door access as well as the long-distance travel. Moreno also saidHowever, in developing countries the demand of public transport infrastructure has not kept up with the demands of growing populations in cities (Moreno, 2016). According to Woldeamanuel and Covington (2014) study, transportation service may not be constant because of change in service demand as a result of population growth through time. Nowadays in developing countries huge population growth has been recorded (Buhaug & Urdal, 2013). Hence, the Increase in population has caused an increase in the demand for mobility (Samek & Torchio, 2015). Nevertheless, public transport infrastructure is not provided based on the riders demand in developing countries specifically for less affluent areas. As Moreno (2016) discussed in his study “Infrastructure provision has historically been biased against less affluent areas, so access to formal jobs is often difficult and costly for a large part of the lower income population. As a result, low-income workers may be discouraged from commuting to formal jobs, lack information on job opportunities, and face discrimination.” (Moreno, 2016).
As Buhaug and Urdal (2013) study indicates, through time huge population growth is recorded in developing countries. The Increase in population has caused an increase in the demand for mobility (Samek & Torchio, 2015). Therefore, development of transportation services is an important factor for social wellbeing (Yatskiv et al., 2017). Based on Yatskiv et al. (2017) study availability of public transport infrastructure is a vital factor in providing an attractive public transport with door to door access as well as the long-distance travel.
According to Woldeamanuel and Covington (2010) study, transportation service may not be constant because of change in service demand as a result of population growth through time.  As Based on Woldeamanuel and Covington (2014) study  this phenomenadevelopment of public transit infrastructure  requires planning for the future, especially forecasting the effects of demographic changes of both people and jobs. Therefore,Hence, based on Woldeamanuel and Covington study, it is essential for transit agencies, transportation planners and local government officials to should undertake periodic evaluations of the socio-spatial distribution of transit service across neighborhoods (Woldeamanuel & Covington (2014). 
2.2. [bookmark: _Toc11760163][bookmark: _Toc13425770]Urbanization and 2.2. CondominiumHousing development 
Condominium housing is a form of housing tenure where each resident household owns their individual unit, but equally shares ownership and responsibility for the communal areas and facilities of the building (Bewunetu, 2016).  It was introduced in the late 1960s in British (Rosen & Walks, 2015). Based on Rosen and Alan (2013) study during the post war period both in US and Canada low-rise single family homes were delivered. However, starting from 1970 population growth, demographic change, regressive rental housing policies and consumer preference change contributed for higher-density condo-living in metropolitan area downtowns (Rosen & Alan, 2013).  As a result, Rosen and Walks (2015) stated that, condominiums make up a fast growing form of housing ownership in cities and suburbs across the globe. According to Rosen and Walks condominium was introduced in the late 1960s, first in British Columbia with the Strata Title Act (1966). As Rosen and Walks described based on this Strata Title Act; condominiums facilitate double ownership, where specific individual units are owned and registered in the name of buyers, coupled with shared ownership over residential common property. This fast growing Rosen and Walks also stated condominium development brought spatial shift from suburbanization and urban dispersion towards concentration, gentrification, and intensification , which in turn brought profound changes in urban social life (Rosen & Walks, 2015). The spatial shift happened mainly because of high rise condominium development at the center (Rosen & Alan, 2013). Therefore, Condo-ism is a force that is countering long trends towards dispersion; it is also important factor in the production and reproduction of the contemporary city (Rosen & Alan, 2013).
 
Rosen and Alan (2013) study shows, condo development were seen as an important ingredient in governments’ attempts to re-urbanize existing built up areas, intensify them and regulate suburban sprawl.  Rosen and Walks (2015) study shows in cities like Toronto such shifts are tightly intertwined with the rise of condo-ism. Based on Rosen and Alan (2013) study during the post war period both in US and Canada low-rise single family homes were delivered. However, starting from 1970 population growth, demographic change, regressive rental housing policies and consumer preference change contributed for higher-density condo-living in metropolitan area downtowns (Rosen & Alan, 2013). Rosen and Alan (2013) study shows North American cities rental apartment buildings, cooperative housing and offices were built in most large city downtowns. Nonetheless, Aaccording to Rosen and Alan urban restructuring and the extensive development of condominium high-rises are dramatically altering the physical environment of many large cities (Toronto, London and New York) and have been an image of a city of towers. However, other studies shows that rather than densification, centralization and intensification of housing units, suburbanization is promoted because of  government  housing related policies.Rosen and Alan also discussed competitive urban policies in global cities such as Toronto, London and New York encourage high-density condominium developments. Based on the policy these cities were successful in facilitating inner-city renewal and boosting economic activity which exacerbates urban problems in hindering gentrification, increasing spatial inequalities, displacement and social exclusion. 
	Rosen and Alan (2013) study stated that, North America’s cities have begun to shift from physical development at the edge to the center. This shift happened because of high rise condominium development at the center. Therefore, Condo-ism is a force that is countering long trends toward dispersion; it is also associated with changing social attitudes and values of city residents, and cultural meanings of urbanism. Rosen and Alan generalized that condo-ism is an important factor in the production and reproduction of the contemporary city.
Wang et al. (2011) study indicates, in 1980s, housing units in major Chinese cities were bonded to jobs as they were located together with or very close to places of employment. However, from the 1990s, accelerated suburbanization of population in major Chinese cities driven by urban redevelopment, urban land reform and urban housing reform has fundamentally altered the jobs-housing spatial relation (Wang et al., 2011). It is the urban poor that suffer most from such housing misallocations (Bewunetu, 2016).  
Wang et al. (2011) discussed that, the spatial bond that existed between urban jobs and urban housing has dissolved and replaced by spatial mismatch when the jobs-housing relationship becomes increasingly imbalanced or separated in space. T.herefore, Housing is not adequate if it is cut off from employment opportunities, health care services, schools, child care centers and other social facilities, or if located in polluted or dangerous areas (UNHCHR & UN-HABITAT, 2014) . However, this phenomenon is clearly observed in African cities.
Africa is the most rapidly urbanizing yet economically poorest region of the world, where almost every country experiences housing shortage (Bewunetu, 2016). According to UN-HABITAT (2010) report housing deficit in Ethiopia lies between 900,000 and 1,000,000 units (UN-HABITAT, 2010). Among this deficit Addis Ababa shares 300,000 housing units (UN-HABITAT, 2010). According to Tiumelissan and Pankhurst (2013) the urban landscape in Ethiopia is undergoing a fundamental transformation, with whole neighborhoods in the center of major cities being cleared for urban development. As Dejen (2017) study indicates that Ethiopian government outlined an ambitious vision for low-income urban and housing development, formulated as the Integrated Housing Development Program (IHDP), since 2005. Addis Ababa is the first city which applies this national program in Ethiopia.
The city of Addis Ababa shares what is studied by Rosen and Alan (2013) (re-urbanize existing built up areas and regulating suburban sprawl) and Wang et al. .(2011) (change from spatial bond to spatial mismatch between jobs and housing). 
	According to Tiumelissan & Pankhurst (2013) the urban landscape in Ethiopia is currently undergoing a fundamental transformation, with whole neighborhoods in the center of major cities being cleared for urban development . As Tiumelissan and Pankhurst study indicates the urban renewal programs have twin objectives of promoting urban growth and providing improved housing for the urban poor. Dejen (2017) study indicates that Ethiopian government outlined an ambitious vision for low-income urban and housing development, formulated as the Integrated Housing Development Program (IHDP), since 2005. Addis Ababa is the first city which applies this national program in Ethiopia. Ingwan et al. (2010) referred that, Addis Ababa City Administration launched ambitious low-cost condominium housing projects through the Integrated Housing Development Program (IHDP) in 2006 to minimize housing shortage, clear slums, and provide decent shelter to middle and low income groups. Particularly 20% to 30% of housing units allocated to female headed households; and youth also have equal opportunity to participate in the programme (MoWUD, 2007).   Based on Krems (2017) up-to their study time around 180,000 Addis Ababa condominium housing units are transferred to their owners. But according to Ministry of Urban Development and Housing (2019) starting from 1998 to 2010E.C. the city administration of Addis Ababa provided the condominium housing units for 176,721 lottery winners of the city dwellers; among the winners 52% are women which is the highest proportion. Based on Tiumelissan and Pankhurst (2013) study low-cost housing condominium apartments are being constructed by the government and offered to urban residents who were living in the areas that are being demolished and who can afford the down-payment and subsequent monthly payments. Some of these condominiums are close to central areas that are being redeveloped and a larger number are being constructed on the outskirts of the city (Tiumelissan & Pankhurst, 2013). 
Related with periphery condominium residential neighborhoods distance from the city center; there is limitation of formal and informal jobs availability although the stated intention of the government was to relocate the poor to new government-built condominium housing, receiving a condominium is not a realistic option for the majority of the low-income inhabitants in the inner city related with the livelihood activity (Hassen et al., 2018).; There is limitation of formal and informal jobs availability notably women who were preparing and selling food and beverages in central part of the city could not do from condominium housing (Tiumelissan & Pankhurst, 2013). 
Based on Hassen et al. (2018) study new government housing, targeted at low- and middle-income inhabitants of the city, has rapidly filled with new residents. Although the stated intention of the government was to relocate the poor to new government-built condominium housing, receiving a condominium is not a realistic option for the majority of the low-income inhabitants in the inner city related with the livelihood activity (Hassen et al., 2018). Hassen et al.and others also discussed that many relocates lifestyle is forced to change, their monthly expenses rise and they cannot afford the costs of transportation from the condominium to work in the city center. 
In addition, these scholars found out that “within the condominiums, home-based enterprises are difficult to establish and maintain. The reasons for this are: potential customers are not willing to walk up flights of stairs to buy the products; neighbors complain about cooking food for commercial purposes or small-scale manufacturing within apartments.” According toit is also proven by World Bank (2017) study, condominium living forced the community into different lifestyles which were formerly dependent on house rent could not regain this source of income and these households are now in Poverty unable to meet their basic needs. Based on this fact Hassen et al. (2018) pointed out that transportation channels are vitally important for the well-being and survival of the poor in cities to get jobs. According to Addis Ababa city planning project office (2016) study residential development in expansion areas are not adequately provided with mass transport to city core. Centers, market areas, working places are not well connected with residential areas by public transport (Addis Ababa city planning project office, 2016). 
2.3. [bookmark: _Toc13425771]Housing policy in Ethiopia
[bookmark: _Toc11760164]Ethiopian Constitution article 41(3) states that every Ethiopian national has the right to equal access to publicly funded social services while article 41(4) imposes obligation on the state to allocate its ever increasing resources to provide to the public social services. Based on these articles the MUDHCo has issued a National Housing Development Policy and Strategic Framework in 2014. The policy has identified key problems and their manifestations along with causal factors and pin pointed policy directions to deal with the problems. The following summarizes the key challenges in enhancing access to housing in urban areas along with policy options devised by government to overcome the key challenges (Tesfalem , 2017). 
Factors for condominium housing development
· proliferation of squatter and informal settlements
· high proportion of slum dwellers
· homelessness limited supply of houses by the public and private developers
· high cost of construction
· low income levels of urban households
· limited serviced land supply
· lack of clarity in taxes and levies
· shortage of public housing finance
· high rate mortgage interest rates
Policy directions
· improving the income of urban households through various income generating programs and packages
· enhancing and improving the supply and production of construction materials
· boosting production of high quality and low cost local construction materials by
· enhancing housing and construction research and development;
· improving construction materials through technology transfer
· construction of additional houses by
· ensuring access of law income households to public condominium houses;
· devising a dynamic organizational system that facilitates housing credit and efficient land supply that will support private saving societies so as to expand production of new houses;
· supporting high income private and real estate developers to construct increased
· numbers of houses with improved land management procedures;
· supporting banks and financial institutions to enhance their capacity of availing mortgage facilities to house builders through enhancement of housing finance schemes and sources;
· effecting a systematic transfer of publicly owned houses to private owners
· Enhancing the implementation capacity of urban administrations to enable them to efficiently deliver serviced urban land for housing development;
· Improving the implementation capacity of urban administrations to enable them deliver improved land registration and management systems, efficient implementation of the lease hold system and to withstand illegal and informal land development.
Therefore, based on the above factors and policy direction of the national housing development; Addis Ababa was the first city which applies this national program in 2006.
2.4. [bookmark: _Toc13425772]Urbanization and  Public transit servicetransportation
Transportation system is the engine of social and economic activities (Tesfaye, 2012). 	Aljoufie (2014) stated that, rapid urban growth causes enormous and continued challenges to many cities in both developing and developed countries. As Tesfaye (2012) referred, provision of competent and efficient transportation system is important for the cities in the modern era of globalization where cities are the centers of urbanization and propellers of national and global economies. Transportation system is also the engine of social and economic activities (Tesfaye, 2012). 
Aljoufie (2014) stated that, rapid urban growth causes enormous and continued challenges to many cities in both developing and developed countries. UrbanHowever, urban sprawl, lack of integrated planning framework and dramatic land use changes have caused a significant impact on the daily share of travel modes that add burden on the transportation system (Aljoufie, 2014). To confront these challenges encouragement of effective public transport is vital. In fact, public transport is becoming a more acceptable alternative to the private automobile and experiencing greater use by a wider socioeconomic range of people, due to higher personal transport costs, environmental concerns, and a solution for increasing congestion in urban areas (Aljoufie, 2014).
Based on Kumar and Barrett (2008) study access to public transport services in Africa’s cities can be assessed on several levels. Kumar and Barrett stated that the low density of paved roads, coupled with unplanned growth, poor road surfaces, and narrow streets suggests that the geographic reach of bus services is seriously restricted. In Africa cities on average, passengers walk for around 10 minutes to reach a bus and typically waiting around 30 minutes at the bus stop before being able to start their trip (Kumar & Barrett, 2008). Kumar & Barrett discussed that, “a strategy for improving urban public transport in African cities consists of stepped measures to improve infrastructure, traffic management and service quality. Short-term steps include increasing road funding, enforcing existing regulations, controlling overcrowding, and strengthening vehicle inspections. Medium-term measures include rehabilitating roads, improving traffic management, setting and enforcing service standards (fares, schedules) and developing a new route structure. The long-term goal is to consolidate gains in all these areas through the creation of a metropolitan transport authority with jurisdiction over roadways and vehicles.”
According to Addis Ababa city planning project office (2016) Addis Ababa transport policy give emphasis on issues such as s:iIntegration between urban transport and land use, promoting mass transit facilities and transport infrastructures which includes non-motorized transport facility ,traffic safety and management to reduce congestion and traffic accidents are the major ones.
Addisu (2010) stated that, the public transport of Addis Ababa is composed of three main systems: 
1. Anbessa City Bus Enterprise which is owned and subsided by the city government. 
2. Privately owned taxis, with fixed tariff rates and partially defined paths and stops. 
3. Midi bus transport service, with fixed paths and stops.
Based on Addis Ababa city Transport Authority (AACTA) (2018/19) public transport distribution report; currently public transit in the city of Addis Ababa includes Anbessa City Bus, Sheger City Bus, Alliance City Bus, Public Service Employees Transport Service Enterprise (PSETSE), LRT, Taxi, Minibus and Midi-Bus (Higer & Isuzu ktkt). 
Tesfaye (2012) referred that, there are around 2.25million public transport trips per day in the city of Addis Ababa which is more 85% are carried out by the informal sector. Minibuses account for 1.4million trips/day, midi-buses and other taxis 0.55million trips and city buses 0.3million trips/day (Tesfaye, 2012). These trips include work, school, shopping, recreational and social activities and trips to social services (medical visits and worship center). From these trips work and education are the dominant purposes of urban trips in Addis Ababa (Abreha, 2007).
This study focused on only three mass transportation systems that are scheduled, administered and financed by the city government of Addis Ababa; LRT, Anbessa and Sheger city Buses. 
Based on Abreha (2007) study Anbessa Bus Organization started in 1935(1942 G.C.) by the Ministry of work and communication. Abraha stated that in 1994 the company was renamed as Anbessa City Bus Service following the proclamation number 187/1986 E.C. In his study Abreha found out that, “Anbessa bus provides its services to only 71% of the total population within a walking distance of 500m. The average number of buss was 4 in each rout line. Average headway time is 30min with crowdedness, long waiting time and absence of seating. The modal share of walking takes 60% to 70%. Among vehicle transport private car take 2%, 72% by taxi, 26 % by city bus.” Addisu (2010) discussed that, Anbessa was serving up to 700,000 passengers per day within 93 routes of the city. In 2016, Anbessa bus transported a total of 396,000 passengers per day with 650 busses in 123 different lines in the city (Addis Ababa City Planning Project Office, 2016; Tagagne, 2018). According to ACBE 2018 annual report; Anbessa had 441 daily City Buses distribution and transported 107,064,171 passengers which means it transported 242,776 passenger per day.  As Tagagne (2018) mentioned, ACBE in 2018 the service is provided with a total of 440 active buses which is almost closest to the enterprise report. A single Anbessa bus passenger carrying capacity ranges to 100-150 persons (Addis Ababa City Planning Project Office, 2016). The Anbassa bus service has 124 routes, 1644 stops, 29 stations and 4 depots (Anbessa City Bus enterprise, 2019).  Addisu (2010), Addis Ababa city planning project office (2016), Tegegne (2018) and Anbessa City Bus enterprise (2019) studies and reports shows, the spatial coverage of Anbessa city bus routes are increasing but the number of buses distributed and the number of passengers transported are decreasing time to time. Kenea (2017) study indicates, Anbessa city bus has only four depots (Piassa, Legehar, Mercato and Bole Anbessa garage) projecting from the city to the sub-cities and the Oromia towns within a 40 km radius. As Kenea explained, compared with the size of the city and surrounding Oromia towns, the number of existing bus terminals, planning and operation are inadequate.
Sheger Mass Transport service started its operation in 2016 (AACTA, 2016). This city Bus has 51 routes and 240 buses (AACTA, 2019). According to Addis Ababa City Transport Authority (AACTA) average frequency of public transport and number of passengers’ information from December 15-20/2011E.C. Sheger City Bus transported 21,518 average passengers per day. 
AACTA (2016) stated that, Addis Ababa Light Rail Transit (LRT) service started operation in 2015 with 41 trains and transports 120,000 passengers per day in both N-S and E-W direction. The service has 39 stations with 5 common interchanging stations and two main depots in Hayat and Kality ends (AACTA, 2016). According to Tagagne (2018) study, the AALRT serves an average of 97,002 passengers per day. Abdlemalik (2017) stated that, Major residential and real estate development locations at Ayat, CMC, Gurdshola and the transportation center Torhailoch are accessed through the east west LRT route. Abdlemalik (2017) discussed that, the North-South corridor is a heavily-used route; it access Africa’s largest open market Merkato. This route starts from Giorgis (Piazza) in the north and heads a little distance to the west to access Merkato and Autobus Tera (the Intercity Bus Terminal) (Abdlemalik, 2017).
 Tagagne found the average waiting time to get AALRT service is 17 minutes. As Tagagne said in his study during peak hour, the average waiting time is 15 minutes. The AALRT administration has a plan to decrease the average waiting time to 10-12 minutes (Tagagne, 2018).
Tagagne referred that at the beginning AALRT office had a plan of 6-minute headway. However, due to a number of problems the headway extended up to 16-18 minutes due to lack of spare parts; shortage of electric supply; very high passenger loadings. Continuous rail crossing of vehicle and pedestrian; lack of skilled personnel and shortage of supply decreases the frequency of the service availability in the stations (Tagagne, 2018). 
Fenta (2014) explained that, Addis Ababa faces various problems including insufficient and poor quality of public transport. Fenta found that existing public transport system in Addis Ababa is critically inadequate to provide service for the increasing travel demand of the city, because the number of cars providing the service is not sufficient. 
Addis Ababa City Planning Project Office (2016) study indicates, the total travel demand of the city has reached 3.2 million person trips per day in the year 2010. From this travel demand only 73 percent is covered by public transport. However, this could not meet the present transport demand of the city, as the city’s population is increasing and its surface area has been stretched out to about 54,000ha (Addis Ababa City Planning Project office, 2016).
According to Addis Ababa city planning project office (2016) study, despite the increase in number and quality of roads and number of passenger vehicles, the transport problem of the city has not yet been alleviated because of lack of integration between land use and transport plan and delay in the installation of mass transit. As a result, according the project office study 55% from the total modes of mobility is covered by walking due to low income level of urban dwellers and inaccessibility of public transport. 
2.5. [bookmark: _Toc11760165][bookmark: _Toc13425773]Public transportation availability for low income and commuters 
Transit availability and accessibility is the measure of public transportation service intensity at the local level (Woldeamanuel & Covington, 2014 ; Pulugurtha et al, 2011). As Al Mamun and Lownes (2011) referred that, “the Local Index of Transit Availability (LITA), developed by Rood (1998), measures the transit service intensity or transit accessibility in an area by integrating three aspects of transit services: route coverage (spatial availability), frequency (temporal availability), and capacity (comfort and convenience).” According to Woldeamanuel and Covington (2014) study the spatial distribution of transit services availability, particularly, transit capacity, coverage, and frequency of service are essential to determine transit service availability and quality. McKenzie (2013) stated that, “as the nation’s low-income population has become more sub-urban in recent decades; transit access may become an increasingly valuable, yet scarcer link to opportunity for those with the fewest resources and housing options.”
Based on Woldeamanuel and Covington (2014) study a portion of Americans relies on various modes of public transit for commuting. As they discussed great portion of members in low-income, elderly and minority households are depend on public transit. According to Moreno (2016) stated that, employers are not confident to higher lower-income workers residing in areas with poor transport accessibility. As Moreno discussed it is because of formal employers may be concerned about the consequences of long commutes on workers performance. This can be happen when there are no large employment centers absorbing low-skilled workers in urban peripheral areas and availability of poor public transport accessibility (Moreno, 2016). 
[bookmark: _Toc1576176]According to McKenzie (2013) the changing socio demographic makeup of suburbs present new planning opportunities and challenges, including associated with transportation and mobility. As a result, public transit service provides a positive social benefit in transportation of low-income residents (Scott, 2014).  Compared to compact urban centers or inner cities, transit availability in suburb communities is relatively poor in most metropolitan areas (McKenzie, 2013). As a result, sSuburbs developed around inadequate public transit Service, placing a burden on low-income residents relies heavily on public transportation (Scott, 2014).
Figure 1: How poor public transport can lead to high job informality rates
[image: ]Source: Moreno (2016)

Public transit service provides a positive social benefit by reducing automobile pollution, reducing automobile vehicle long distance travelled, and providing accessible transportation to low-income residents (Scott, 2014). According to Scott (2014) study public investment in additional transit service can reduce commuting times, relieve the transportation burden on low-income suburban residents and help alleviate poverty. Therefore, as Woldeamanuel and Covington (2014) study indicates in order to develop convenient transportation service expansion plans and policies for an area; transit accessibility, availability and intensity measures should be properly identified. Woldeamanuel and Covington (2014) found that, neighborhood transit availability index can be created from transit capacity, frequency and service coverage to determine the level of intensity of service (high, medium and low) in the study area. 
2.6. [bookmark: _Toc11760166][bookmark: _Toc13425774]Spatial coverage and mismatch of public transportation in urban areas
The distribution of land uses such as residential, industrial or commercial over the urban area determines the locations of human activities such as living, working, shopping, education or leisure. The distribution of human activities in space requires spatial interactions or trips in the transport system to overcome the distance between the locations of activities. The distribution of infrastructure in the transport system creates opportunities for spatial interactions (Michael, 1993). But if the distributed transport infrastructure not integrated with well public transit system then activity spaces cannot be linked which results spatial mismatch. Spatial mismatch is an old problem that still impacts workers in metropolitan areas (Woldeamanuel & Covington, 2014). As Moreno (2016) referred thatdiscussed in his study, the spatial mismatch hypothesis (SMH) was inspired by the rapid residential suburbanization around metropolitan areas of the US in the second half of the 20th century. Moreno stated that, as people moved from the cities to the suburbs, firms also dispersed from central areas to suburban areas. According to Moreno because of housing market discrimination and zoning regulations low income communities were not able to move to the suburb residential areas. As a result, there was an increase in the concentration of minorities in inner-city areas, where low-skilled job creation was slow (Moreno, 2016). The SMH is supported by the fact that many of the jobs created in the large metropolitan areas were in suburbs with poor or non-existent public transit service; these jobs are practically inaccessible to city residents who either do not own vehicles or own vehicles that demands long commute to the suburbs (Alam, 2005). 
In the other way as Scott (2014) referred, spatial mismatch research has found that transportation access has a positive relationship with employment outcomes whereas housing and employment discrimination have a negative relationship with the spatial mismatch of jobs and housing (Scott, 2014).Therefore, Woldeamanuel and Covington (2014) found that effective public transportation is important in solving the gap between the residence and job locations. Considering residence in designing routes could not be the only solution but the transit systems should also consider transit accessibility from job locations (Woldeamanuel & Covington, 2014). Therefore, the accessibility factor is important in designing the public transport infrastructures (Ross & Svajlenka, 2012).
According to Abreha (2007) study when the transit accessibility is increased then the spatial coverage also will increase. The higher the spatial coverage of the service the shorter will be the walking distance to the service (Abreha, 2007). Transit coverage varies by neighborhood characteristics; including proximity to the urban core and neighborhood income levels (Ross, 2012). Tomer (2012) finds that, across large metropolitan areas job is accessible by public transit and accessibility is even lower in the suburbs, where transit coverage is typically poor. In contrast, peripheral areas of large cities in developing countries are the locus of dense housing settlements, with a predominance of informal employment and low availability of formal jobs (Moreno, 2016). According to Moreno study low-income workers are particularly dependent on public transport; better access to public transport can reduce inequality by improving labor market outcomes (Moreno, 2016).
According to Kraft (2016) accessibility is characterized as the number of facilities (terminals, stops etc.) available in a certain time or within a certain walking distance or for a certain charge. Based on Kraft study spatial accessibility of public transport stops with the distance of 400 meters and 5minutes travel time represents a comfortably accessible walking distance. Accessibility of public transit stops are also considered with their distribution and locations (Kraft, (2016).
2.7. [bookmark: _Toc13425775]Public Transit Spatial Mismatch in Los Angeles Suburbs (Empirical literature) 
The spatial distribution of transit services, particularly, transit capacity, coverage, and frequency of service were used to determine transit service availability and quality. Major inconsistencies in the spatial distribution of available transit services were a great challenge. The aim of the study was to evaluate the spatial distribution and essential characteristics of transit service within the San Fernando Valley, the northern suburbs of the Los Angeles metropolitan area. This area was approximately 30 to 40 miles from the center of Los Angeles City. The neighborhoods were examples of second and third rings of suburbs and
 overall, the development had a suburban character in terms of density and type of housing. Using Geographical Information System (GIS) and multivariate statistical models for the analysis, a comprehensive neighborhood level transit availability index was created as a function of transit capacity, frequency and service coverage (Woldeamanuel & Covington, 2014).
[image: ][image: ][image: ][image: ][image: ][image: ][bookmark: _Toc13246192]Figure 3: Transit Intensity Maps and Population Density
                   
  Source: Woldeamanuel and Covington, 2014

The index results showed that a significant portion of the study area has low transit availability. At the tract level, an aging population and minority population characteristics were negatively related to transit availability; indicating that on average, there are slight inconsistencies in the demand and the supply of transit services.
2.8. [bookmark: _Toc13425776]Summary of the literature 
Public transportation helps for mass mobility of passengers. It gains attention in recent years as a result of its role decreasing auto ownership, relieving highway congestion and transporting mass population (Armstrong & Thiriez ,1987)). Among different purpose of trips commuting takes the largest share worldwide. To facilitate this tripe adequate infrastructure is a big constraint in developing world. Infrastructure provision is biased in less affluent or low income communities (Moreno, 2016). As a result, low income communities are discouraged to get jobs (Yatskiv et al., 2017). In addition to provision of adequate infrastructure; transportation service may not be constant related with population dynamics. Therefore, periodic evaluation of socio spatial distribution of transit service is needed (Woldeamanuel & Covington, 2014).
High density condominium residential neighborhoods were contributed by population growth, demographic change, and regressive rental housing policies. Fast growing of housing ownership in cities and suburbs brought spatial shift. The shift is from sub-urbanization and dispersion towards concentration, gentrification and intensification in America and Europe cities (Rosen & Alan, 2013). Other studies also promote from densification, centralization and intensification of housing units to suburbanization because of policies change (Wang et al., 2011). This shift was happened in Chinese cities because of urban redevelopment, urban land reform and urban housing reform. As a result of the spatial shift, the spatial bond that existed between urban jobs and urban housing is decreasing.
In Africa this thing is clearly observed. Ethiopia is one of the countries which condominium housing development is existed (Bewunetu, 2016). The aim of IHDP of the city administration was to minimize housing shortage, clear slums and provide decent shelter to middle and low income groups.  Addis Ababa which is the capital of Ethiopia constructed mass residential condominium housing specifically at the periphery part of the city. Most of condominium housing units are located at the periphery part of the city. City centers, market areas, working places are not well connected with residential areas by public transport. Transportation system is engines of social and economic activities. In order to confront these challenges encouragement of effective public transport is vital (Scott, 2014).
Lack of integration between land use, transport and delay in the installation of mass transit creates mismatch. Transit availability is a measure of public transportation service intensity. The transit availability is measured by integrating three aspects transit services route coverage (spatial availability), frequency (temporal availability) and capacity (comfort and convenience) (Woldeamanuel & Covington, 2014). Low income population has become more sub-urban residents in recent decades. Therefore, the public transit service availability should be known in these areas in order identify the level of intensity of the service and to intervene accordingly.
2.9. [bookmark: _Toc13425777]Conceptual framework 
The following conceptual framework illustrates the interrelated entities in which one can feed the other to evaluate public transit availability in the core and periphery of Addis Ababa city.
Typical issues of the study that of intensity of public transit availability, socio-economic and demographic characteristics are identified. Based on the issues inner and periphery areas of the city are evaluated. The result of the evaluation anticipated either high intensity or low intensity of the public transit service with its negative or positive socio-economic characteristics. As a result, Low intensity of the public transit service with negative socio-economic areas are recommended for possible solutions
Typical issues
Intensity of public transit availability
Socio-economic & demographic characteristics
Condominium residential neighborhoods
Population dynamics 
Public transit service and infrastructure availability  
Inner city
Periphery areas
Evaluation of findings
High transit service intensity
Low transit service intensity
Negative socio-economic & demographic characteristics
Positive socio-economic & demographic characteristics
Public transit mismatch
















 
[bookmark: _Toc13246193]                         Figure 4: Conceptual Framework of the Study
                        Source: Computed by Author, 2019
2.10. [bookmark: _Toc11760167][bookmark: _Toc13425778] Research gap
According to the literature review which is was done on the above international experience shows that spatial mismatch (specifically segregation of jobs and residence) is happening in metropolitan areas. Because of the segregation low incomes, aged people and women are affected. This experience (spatial mismatch) is clearly observed in the city of Addis Ababa because of the spatial segregation between suburb condominium residences and the city center where more of formal and informal jobs are available. Based on the above literature review studies are were done related with public transit and residential neighborhoods mismatch in US metropolitans. In Ethiopia specifically in Addis Ababa transportation studies are were done related with measuring and evaluating the performance, accessibility, efficiency and quality of public transit service and the transit route. But no studies are done yet in Addis Ababa to show the extent (transit availability) and impact (socio-economic) of mismatch among city periphery condominium neighborhoods and the city public transit service.  
[bookmark: _Toc11652827][bookmark: _Toc11653982]This study fsfill the gap through analyzing the demographic characteristics and spatial coverage of public transit availability by taking into account caring capacity, frequency and transit coverage of the service within Addis Ababa city specifically in the city periphery condominium areas. The result displayed graphically using GIS to show the extent of service gap in each study woredas. This also enables the city transport authority to act on the public transit service gap based on tangible fact. 










[bookmark: _Toc11760168][bookmark: _Toc11916390][bookmark: _Toc11922757][bookmark: _Toc13124897][bookmark: _Toc13125148][bookmark: _Toc13241172][bookmark: _Toc13245318][bookmark: _Toc13246869][bookmark: _Toc13425779]CHAPTER THREE: 
[bookmark: _Toc11760169][bookmark: _Toc13425780]BACKGROUND OF THE STUDY AREA
3.1. [bookmark: _Toc11760170][bookmark: _Toc13425781]Introduction 
The study of this research evaluates public transit availability (carrying capacity, frequency and coverage of the service) at the periphery residential condominium neighborhoods of Addis Ababa city. This section focuses on general description of the city, condominium development, transport infrastructure, public transportation service and challenges of integration between public transportation service and periphery condominiums.
Addis Ababa
Addis Ababa is the capital city of Ethiopia which is located in the center of the country. It was emerged in 1886 as a military camp in the strategic area of Entoto hills. In 1888, it was moved to the hot springs (Ffilwoha) located near the present day city Centre (Hassan et al., 2018). According to Hassen and others, the early primary historical elements of the formation of the city were the palace, the churches, the marketplace (Arada) and the houses of the nobility. Currently the city extends over 540 square kilometres at an altitude of 2,500 meters above the level of the Mediterranean Sea. The city is also the seat of government, center for education, industry and service. It is a chartered city with status of a city and state, the current governance structure of the city has three administration tiers, city level (central), sub city level and woreda (district) level (AACPPO, 2016). The three tiers of the city administration includes; one city administration, 10 sub-cities and 116 woredas. As the Federal Ministry of Transport (2011) referred that, the 2007 national census data, having a growth rate of 2.1%, the population of Addis Ababa was 2,738,248 which accounted for 32.27% of the total urban population of the Country. Recently Different studies indicated that the population size of Addis Ababa is growing fast. Based on the 2007 census data, the city population growth in 2016 with 3.8 growth rate is indicated 4.6 million (UN-habitat, 2017). As result of population increase the city demands sufficient infrastructures such as that of transportation system and housing provision. The city government tries to alleviate these challenges by providing public transits (such as Buses & LRT) and condominium housing.  
3.2. [bookmark: _Toc11760171][bookmark: _Toc13425782]Condominium development in Addis Ababa
The city of Addis Ababa encompass a complex combination of planned and unplanned elements of the city, it can be viewed as the original old city, the industrial city, the informal city, the market city, the condominium city, and so forth (Hassan et al., 2018). As a condominium city; these communal housings are the result of population growth, space constraint and redevelopment strategies which are promoted by the federal government. The Federal Democratic Republic of Ethiopia enacted the condominium law under the proclamation No.370/2003 (FEDERAL Negarit Gazeta, 2003). Based on this proclamation number the Ministry of Urban Development, Housing and Construction has been providing the policy framework and detail norms for government initiated and implemented housing program since 2004. In addition to the housing program policy framework WUB Consult (2015) stated that, the 2005 urban development policy brought radical change to the way housing is to be developed; government took the lead to develop houses in mass and transfer it to owner-occupiers.
The condominium housing program was launched first in Addis Ababa in 2004 and then scaled up in other major urban centers of the country. In Addis Ababa the housing program was expanded from the 20/80 financing ratio to 10/90 and 40/60 of housing productions (Hassan et al., 2018). According to WUB Consult (2015) total housing demand in Addis Ababa based on registered households is about 994,344. If we assume all registrants are able to pay, the serviced land demand would be over 7,500 hectares (WUB Consult, 2015). Since 2004 to 2014 a total of more than 2486 ha of land were used for the construction of low and middle rise condominium housing, including social services and other investment activities (WUB Consult, 2015). The land was produced both in the expansion and inner city redevelopment areas of Addis Ababa. The expansion areas of Addis Ababa are primarily being filled with government sponsored condominium apartment housing neighborhoods (Hassan et al., 2018).  Recent studies revealed that more than 160,000 housing units have been transferred to beneficiaries since 2004, the year the program started and more than 100,000 housing units are under construction (Hassan et al., 2018). According to Ministry of Urban Development and Housing 2019 report, starting from 2006 to 2018 the city administration of Addis Ababa provided the condominium housing units for 176,721 winners of the city dwellers. Therefore, condominium housing provision is increasing through time. 
3.3. [bookmark: _Toc11760172][bookmark: _Toc13425783]Public transport service in Addis Ababa
The expansion of the city, increasing population size coupled with the economic growth has required respective transport service supply for the increasing mobility needs of the People. (FDREMT,  2011). As a result, the city administration developed Transport Policy of Addis Ababa in 2011 that upgrades Anbessa City Bus Enterprise, introduce Bus Rapid Transit /Light Rail Transit System along major corridors, and promote Minibus Taxi Services (Fenta, 2014).
In order to introduce viable transportation service transport infrastructures should be developed. The existing Addis Ababa street network is composed of four different types of streets; principal Arterial Street, Sub Arterial Street, Collector Street and Local Street. At present, existing road density is below the universally accepted standard of 25% which is 18% of the built-up area (29,000ha.) and 10% of the total urban space (54,000ha.) (AACPPO, 2016). Therefore, the road infrastructure is insufficient for carrying the transit of the city. 
Based on Addis Ababa city Transport Authority (AACTA) (2018/19) public transport distribution report; public transit in the city of Addis Ababa includes Anbessa City Bus, Sheger City Bus, Alliance City Bus, Public Service Employees Transport Service Enterprise (PSETSE), LRT, Taxi, Minibus and Midi-Bus (Higer & Isuzu ktkt). These public transit services facilitate trips in the city. According to Abreha (2007) study the modal share of vehicle transport; private car takes 2%, 72% by taxi, 26 % by city bus. Tesfaye (2012) referred that, there are around 2.25million public transport trips per day in the city of Addis Ababa which is more 85% are carried out by the informal sector. Minibuses account for 1.4million trips/day, midi-buses and other taxis 0.55million trips and city buses 0.3million trips/day.
This study focused on only three mass transportation systems that are scheduled, administered and financed by the city government of Addis Ababa; LRT, Anbessa and Sheger city Buses. 
Based on Abreha (2007) study Anbessa Bus Organization started in 1935(1942G.C.) by the Ministry of work and communication. Abraha stated that in 1994 the company was renamed as Anbessa City Bus Service following the proclamation number 187/1986E.C. Addisu (2010) discussed that, Anbessa was serving up to 700,000 passengers per day within 93 routes of the city. In 2016, Anbessa bus transported a total of 396,000 passengers per day with 650 busses in 123 different lines in the city (Addis Ababa City Planning Project Office, 2016; Tagagne, 2018). According to ACBE 2018 annual report; Anbessa had 441 daily City Buses distribution and transported 107,064,171 passengers throughout the year which means it transported 242,776 passengers per day.  As Tagagne (2018) mentioned, ACBE in 2018 the service is provided with a total of 440 active buses which is almost closest to the enterprise report. A single Anbessa bus passenger carrying capacity ranges to 100-150 persons (Addis Ababa City Planning Project Office, 2016). The Anbassa bus service has 124 routes, 1644 stops, 29 stations and 4 depots (Anbessa City Bus enterprise, 2019).  Addisu (2010), Addis Ababa city planning project office (2016), Tegegne (2018) and Anbessa City Bus enterprise (2019) studies and reports shows, the spatial coverage of Anbessa city bus routes are increasing but the number of buses distributed and the number of passengers transported are decreasing time to time. Kenea (2017) study indicates, Anbessa city bus has only four depots (Piassa, Legehar, Mercato and Bole Anbessa garage) projecting from the city to the sub-cities and the Oromia towns within a 40 km radius. As Kenea explained, compared with the size of the city and surrounding Oromia towns, the number of existing bus terminals, planning and operation are inadequate.
Sheger Mass Transport service started its operation in 2016 (AACTA, 2016). This city Bus has 51 routes and 240 buses (AACTA, 2019). According to Addis Ababa City Transport Authority (AACTA) average frequency of public transport and number of passengers’ information from December 15-20/2011E.C. Sheger City Bus transported 21,518 average passengers per day.
AACTA (2016) stated that, Addis Ababa Light Rail Transit (LRT) service started operation in 2015 with 41 trains and transports 120,000 passengers per day in both N-S and E-W direction. The service has 39 stations with 5 common interchanging stations and two main depots in Hayat and Kality ends (AACTA, 2016). According to Tagagne (2018) study, the AALRT serves an average of 97,002 passengers per day. Abdlemalik (2017) stated that, Major residential and real estate development locations at Ayat, CMC, Gurdshola and the transportation center Torhailoch are accessed through the east west LRT route. Abdlemalik (2017) discussed that, the North-South corridor is a heavily-used route; it access Africa’s largest open market Merkato. This route starts from Giorgis (Piazza) in the north and heads a little distance to the west to access Merkato and Autobus Tera (the Intercity Bus Terminal) (Abdlemalik, 2017).  Tagagne (2018) referred that; at the beginning AALRT office had a plan of 6-minute headway. However, due to a number of problems the headway extended up to 16-18 minutes due to lack of spare parts; shortage of electric supply; very high passenger loadings. Continuous rail crossing of vehicle and pedestrian; lack of skilled personnel and shortage of supply decreases the frequency of the service availability in the stations (Tagagne, 2018).
3.4. [bookmark: _Toc13425784][bookmark: _Toc11760173]Challenges of public transport service at the periphery condominium residential areas 

Different challenges of the urban transport are observed in the city of Addis Ababa. Insufficient public transport service provision and limited coverage of the service are major public transport service constraints which results poor access to residence and work place, education, health and other services (FDREMT, 2011). The city has been undergoing horizontal expansion as the major form of development throughout its history including condominium residential areas (Fenta, 2014). Residential development in expansion areas are not adequately provided with mass transport to city core (AACPPO, 2016). This is due to lack of integration between expansion areas and urban transport which is the result of poor transport planning and implementation (Hassan et al., 2018; FDREMT, 2011). In addition to lack of integration, lack of provision of appropriate road infrastructure is also a challenge for the periphery residents not access the public transport (Fenta, 2014). 
According to FDREMT,(,  2011(2011) the Transport Policy of Addis Ababa has outlined eleven key policy issues to address the transportation service challenges. Among these key issues which related with developments in expansion areas and transport service are; 
· Integration of Land-use and Transport Plan: according to this issue expansion of residential land use development without considering the necessary transport infrastructure and services resulted inefficiencies in the transport system.
· Expansion of transport infrastructure: the coverage of transport network is inadequate compared to international standard and the existing road network is not properly utilized.
· 
· [bookmark: _Toc11653989]Enhance transport service provision: the service is limited to major roads and its coverage is very low. These trends indicate that the government gives emphasis for transportation challenges which are seen at the periphery part of the city. But to provide functional solutions for the challenges by the government, there has to be detail scientific studies to identify the intensity of the gap and to intervene accordingly. This study contributes by identifying the gabs of transit availability across the city specifically at periphery part of condominium areas using GIS as a spatial analysis tool. Enhance transport service provision: the service is limited to major roads and its coverage is very low. 
· [bookmark: _Toc11653990]These trends indicate that the government gives emphasis for transportation challenges which are seen at the periphery part of the city. But to provide functional solutions for the challenges by the government, there has to be detail scientific studies to identify the intensity of the gap and to intervene accordingly. This study contributes by identifying the gabs of transit availability across the city specifically at periphery part of condominium areas using GIS as a spatial analysis tool. 
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· [bookmark: _Toc11760174]
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[bookmark: _Toc13241178][bookmark: _Toc13245324][bookmark: _Toc13246875][bookmark: _Toc13425785]CHAPTER FOUR: 
[bookmark: _Toc11760175][bookmark: _Toc13425786]METHODOLOGY
4.1.  Introduction 
This chapter discusses about how to answer research questions and address objectives of the study. The methodology of the study includes study area selection criteria, research approach, data type and source, data collection techniques, data analysis and presentation technique. The study area selection criteria are listed why the study is undertaken in the selected city and its periphery part. In the research approach what type of research method should be used is discussed. The data type  and source method describes the type of data collected from what type of data where should be collected. governmental and non-governmental offices .The data collection technique describes how the data was collected. Data analysis technique stated the type of method adapted used to analyze the collected data.
4.2. [bookmark: _Toc11760177][bookmark: _Toc13425788] 4.3. Study area selection Criteria  
The study is was done in Addis Ababa city related with condominium areas which emphasized more on suburb part of Addis Ababa. The reason behind the study area is was undertaken in Addis Ababa ist that:;
· The city has more number of condominiums at the periphery part
· The condominium areas have few job options
· Periphery condominium areas are located long distance to the city center
· There is high number of residents in condominium neighborhoods which demands high of public transit service and still the residents are increasing in this area
· There is limited infrastructure provision and service distribution across the city
· Condominium is built for low income, who are heavily dependent on public transportation 


[bookmark: _Toc13246194]Figure 52: Addis Ababa city periphery condominium sites 
Source: Addis Ababa city Transport Authority, 2019. 	
 

4.3. [bookmark: _Toc13425789] Research design
The outline of the research design has been illustrated in Figure below. The research problem and the objectives stated above are followed by the literature review. Next, identification of data required to deal with and solve the problem was indicated. Secondary data were acquired from different documents available at the government offices. For the collected data spatial and statistical analysis has been undertaken. After analysis the result has been discussed and based on the result conclusion and recommendation were formulated. Problem identification
Objectives and research questions
Identification of data
Secondary data 
Spatial analysis 
Statistical analysis 
Result and discussion
Conclusion and recommendation
Literature review











[bookmark: _Toc13246195]Figure 6: Research design
4.4. [bookmark: _Toc11760178][bookmark: _Toc13425790]Research approach 
The study is was based on quantitative type of research. It quantifies the availability of public transit service by using caring capacity, route coverage, service frequency, number of bus and LRT, number of routes and number of transit stops. It also quantifies neighborhood characteristics in terms of number of population, number of labor force, income level of Woreda communities and area coverage. 
4.5. [bookmark: _Toc11760179][bookmark: _Toc13425791] Data Type and Source
The study used secondary data type. The secondary data are were spatial and non-spatial. Spatial data types are were maps of Woreda boundaries, cCondominium site, transit network (Anbessa, Sheger and LRT routes) and transit stops are  collected from various sources. Whereas non-spatial data are were demographic and socio-economic characteristics of the Woreda are collected from CSA. Detail data types and sources are listed below.
[bookmark: _Toc11654691]Table 1: Data type and sources

	Types of data
	sources

	Woreda boundaries map (AutoCAD or GIS)
	AA. city planning commission, 2007

	Number of woredas boundary
	From AutoCAD or GIS, 2007

	Area coverage of each woreda
	From AutoCAD or GIS, 2007

	Number of populations in each Woreda
	CSA, 2007

	Number of labor force in each Woreda
	CSA, 2016

	Public transit routes (GIS file)
	From LRT, Anbessa and Sheger administrative office and Addis Ababa city government transport authority office,2019

	Public transit routes covers each Woreda
	From public transit routes (GIS file), 2019

	Public transit route length in each Woreda
	From public transit routes (GIS file), 2019

	Number of public transit stops in each Woreda
	From public transit routes (GIS file), 2019

	Number of Anbessa , Sheger and LRT services in each transit route of the city per day
	From Anbessa , Sheger and LRT administrative office or Addis Ababa city transport authority office, 2019

	Number of seats per Anbessa , Sheger and LRT transit services 
	From Anbessa, Sheger and LRT administrative offices or Addis Ababa city transport authority office, 2019




As it is listed on the above table the baseline data is was prepared to calculate transit availability indexes. In order to calculate the indexes; transit vehicles per day per route (total buses arriving at a typical stop per day), design capacity, population, Woreda area, route length and the number of transit stops per Woreda wereare used. The correlation and regression analysis will were be done using variables such as income level, gender, age, and percentage of labor force participants of each Woreda in relation with transit availability indexes. The method helps to identify public transit service availability impact on the socio-economic and demographic characteristics of the Woreda. For the purpose of this study the 2007 of Addis Ababa lowest administrative units which were 99 Woredas are taken as traffic analysis zone with census data. The baseline data are were collected accordingly.
Bus and LRT frequency and capacity baseline data: number of buses and LRT per day per route (total buses and LRT arriving at a given stop per day) and design capacity (allowable number of passengers). Once the database for the total buses arriving at a stop per day is prepared, the capacity of the bus and LRT line is calculated using the following formula:
Total daily seats = Buses or LRT per day at a given stop x buses’ or LRTs’ number of seats (design capacity)
Route length = [length of route completely within the Woreda] + [1/2 x (length of route bordering the Woreda)]
Bus or LRT stops: the bus or LRT stops in each analysis Woreda are counted in such a way that bus or LRT stops laying in the Woreda are were counted as ‘one’. In addition to this, stops falling along a boundary are  counted as a half stop in each of the bordering Woredas or it is was counted as one fourth if the bus or LRT stop is located at the cross intersection of Woredas.
Number of stops = [Number of bus or LRT stops completely within tract] + [1/2 x (Number of bus or LRT stop bordering the Woredas)] + [1/4 x (Number of bus or LRT stops touching 4 Woredas)]
Population and Woreda area (population density) baseline data: the 2007 Census demographic data is collected from CSA 2007 Census at Woreda level, and then the population is projected to 2019 without changing the 2007 administrative Woreda boundaries in order to identify the current public transit demand. 
Socio-demographic data (such as gender, age, incomeage, expenditure and labor force participation): the 2016  socio-economic data in of 2007 censusthe city were collected at sub-city level. In this study each sub-city socio-economic character is was distributed to its smallest administrative units (Woreda) based on the current projected population proportion.  Simple Regression and correlation analysis will be was done in relation with transit availability index. The spatial representation of socio-economic variables (incomeexpenditure level and labor force) and demographic variables (age and gender) will be included in the analysis using GIS.

4.6.   
4.7. [bookmark: _Toc11760181][bookmark: _Toc13425793]Data Collection Techniques 
The study will was depended on secondary data. The techniques that will be used to collect the data are
 Identifyingwere: identifying and organizing the variables what should be collected from where; the researcher will  go went to the sources of data which are were governmental and non-governmental offices to collect hard copies and soft copies that will behas been related with the research variables.
In the process of data collection the researcher will check or evaluated the suitability (contextually), reliability (level of accuracy), adequacy (availability in the desired quality and quantity) of secondary data.
4.8. [bookmark: _Toc11760182][bookmark: _Toc13425794]  Data Analysis and Presentation Technique
The study will adaptused local index of transit availability (LITA) analysis method which was introduced by the Local Government Commission of the United States to understand the spatial distribution of transit in small communities (Woldeamanuel & Covington, 20140). This method will be used to show public transit service intensity or spatial distribution of transit service in Addis Ababa city specifically in the periphery part of condominium neighborhoods. The reason behind to use this method for this research was first it helps to analyze public transit  quantitative data and next it helps to present the analyzed data in maps using GIS software.  The method was used for Addis Ababa city Anbessa, Sheger and LRT transit services. Each of transit service route length, number of stops, frequency and number of buses or LRT were studied at Woreda level and encode in excel to produce transit availability index. For the case of this study the public transit availability in each Woreda of the city is was represented as WITA  (woreda index of transitAddis Ababa bus and LRT service index availability(ABLSI)). The analysis will covered all parts of the city in Woreda unit level. For each part of the city Woreda units the WITA ABLSI components that of public transit capacity (design capacity), frequency and coverage of the service will be analyzed by using census and transit data. 
1. Capacity score 
Capacity can be defined in different terms such as vehicle capacity; person capacity, maximum capacity, and design capacity (Gebeyehu & Takano, 2008). In this study, the design capacity of the transit vehicle is was used for the analysis. The total amount of daily bus or LRT seats is was calculated as a product of the total number of bus or LRT arrivals at a specific stop in the Woreda, and the number of seats on the bus or LRT.

Where,   = Capacity score in the ith Woreda (W); BS or LRT = Total daily bus or LRT seat (the design capacity); lWi = Route length in Wi; and PopWi = Population in Wi 

2. Frequency score 
This component is referrreferreding to the headway between two consecutive buses (the waiting time for the travelers). Frequency measure is was based on the total daily number of buses on all the routes that have at least one stop in the Woreda (W).
FWi = TB or TL, if lWi has at least one stop in Wi; 0, otherwise  
Where, FWi = Frequency score in the ith woreda (W); and TB = Total number of buses, TL=Total number of LRT
3. Coverage score 
The bus or LRT coverage component of the transit availability analysis focuseds on the spatial distributions of the existing bus or LRT service, and is was calculated based on the density of transit stops or stations. 

COWi = Coverage score in the ith W; SWi = Number of bus or LRT stops in Wi; and AWi = Area of the Wi
After calculating each transit availability components the next step is was standardizing the scores. Since the units of measurement for each of the three scores are were different, the mean and the standard deviation are were calculated for every attribute (capacity, frequency and coverage) in to standardize/normalize the scores order to standardize/normalize the scores.
Standardized score for capacity = ([capacity score] - [mean of distribution])/ [standard deviation]  
Standardized score for frequency = ([frequency score] - [mean of distribution])/ [standard deviation]  
Standardized score for coverage = ([coverage score] - [mean of distribution])/ [standard deviation]
After standardizing the calculated values it will bewas added together to give each Woreda transit availability index. The result will be converted to a spatial map using GIS to visually display the distribution of high , medium and low serviced areas by the existing bus or LRT services. The three components of transit availability are were equally weighted by considering the relative importance they have to each other. 
Overall score/index = standardized capacity score+ standardized frequency score + standardized coverage score
The result of each Woreda transit availability index will be correlated with Woredas demographic and socio-economic characteristics spatially using GIS. The strength of relation between transit availability and socio-economic charactersticscharacteristics of Woredas with condominium residential neighborhoods identified based on simple regression analysis method.














[bookmark: _Toc11760183][bookmark: _Toc11916406][bookmark: _Toc11922773][bookmark: _Toc13125162][bookmark: _Toc13245334][bookmark: _Toc13246885][bookmark: _Toc13425795]CHAPTER FIVE: 
[bookmark: _Toc11760184][bookmark: _Toc13425796]RESULT AND DISCUSSION
5.1. [bookmark: _Toc11760185][bookmark: _Toc13425797]5.1. Introduction 
5.1.1. 
The data used for this research was secondary data and it was quantitative. The collected quantitative public transit and socio-economic data were analyzed using excel, SPSS and GIS. This chapter discusses about data description descriptionand the result of it, result and discussion. It shows the evaluation of each public transit services (Anbessa, Sheger and LRT) capacity, frequency and coverage analysis (result and discussion) .The evaluation of total result of each of the transit service availability and the standardized score has been discussed calculated at  Woreda level all over the city. Finally it has been evaluated the relationship between socio-economic characteristics of periphery woredas with condominium residential neighborhoods and the standardized transit availability index of the city. As result, tables, percentages, graphs and maps were intensively utilized in presenting the findings.
5.2. [bookmark: _Toc11760186][bookmark: _Toc13425798] 5.1. Data description 
Used for the AnalysisIn this chapter the base line data used for the analysis were public transit service, socio-economic and demographic data. For public transit service each transit services (Anbessa, sheger and LRT) route length, stops and number of transit services assigned in the provided routes with their frequency have been collected at Woreda level. These transit data were collected from GIS line map by measuring route length and counting stops from each transit route within Woredas but the number of bus assigned  and its frequency were collected from each public transit offices and Addis Ababa city transport authority. For socio-economic and demographic data expenditure, labor force, age and gender have been collected and analyzed. These data are collected from 2007 CSA census and 2016 CSA socio-economic of Addis Ababa city. The 2007 census data of Addis Ababa population at Woreda level were projected using geometric increase projection method to 2019 with 3.8 annual growth rates.
5.1.1. Statistics data description 
Table 1: Description statistics for the 99 Woreda of the city
	Description statistics for the 99 woredas of the city

	Characteristics of the woreda
	Average 
	Minimum
	Maximum
	Standard deviation

	Area 
	5.240
	0.36
	47.87
	8.328

	Population 
	43,292
	6,106
	127,356
	20,127

	Density 
	25,081
	172
	117,957
	21,593

	Labor force participation 15+ age group
	39,816
	4042
	206,550
	31,694









Table 2: Baseline data of Anbessa bus capacity and frequency
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	


[bookmark: _Toc11916410][bookmark: _Toc13245338][bookmark: _Toc13246889][bookmark: _Toc13425799]5.2.1. 
[bookmark: _Toc11760187]Baseline data for capacity and frequency


	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	


Table 2: Baseline data of Anbessa bus capacity and frequency
	Baseline data of Anbessa bus capacity and frequency

	
	Route1
	Route2
	Route3
	
	Route122
	Route123
	Route124

	Buses per day(frequency)(B)
	20
	18
	40
	...
	21
	16
	16

	No. of seats per bus(S)
	70
	70
	70
	...
	70
	70
	70

	Total daily seats (BxS)
	1400
	1260
	2800
	...
	1470
	1120
	1120



Source: Addis Ababa city transport Authority, 2019











[bookmark: _Toc13246196]Figure 73: Number of buses assigned and total bus seat in the provided route
The above figure shows that highest number routes have 03 to 5 bus distributiondistributions whereas lowest numbers of routes have 6 to 108 bus distribution. The figure also shows the total number of bus seat per route; as it is shown most 120 routes have low 0 to 4000 total bus seat and 4few routes have high number4001 to 8000 of total bus seattotal bus seats.
.
[bookmark: _Toc11654692]Table 33: Baseline data of Sheger bus capacity and frequency
	Baseline data of Sheger bus capacity and frequency

	
	Route1
	Route2
	Route3
	
	Route51
	Route52
	Route53

	Buses per day(frequency)(B)
	6
	6
	36
	...
	40
	18
	20

	No. of seats per bus(S)
	70
	70
	70
	...
	70
	70
	70

	Total daily seats(BxS)
	420
	420
	2520
	...
	2800
	1260
	1400


Source: Addis Ababa city transport Authority, 2019







[bookmark: _Toc13246197]Figure 84: Number of bus assigned and total bus seat in the provided
Table 33 and figure 82 shows that 01 up-to 58 numbers of Sheger buses are assigned for 3947 numbers of routes but few numbers of routes have high number of buses distribution. Again 47 routes have between 0 to 4000 total Sheger bus seat and the rest of routes have relatively high number of total bus seat. 


[bookmark: _Toc11654693]Table 44: Baseline data for LRT capacity and frequency
	
	Route1(E-W)
	Route2(N-S)

	LRT per day(frequency)(L)
	64
	63

	No. of seats per  LRT tram(S)
	572
	572

	Total daily seats(LxS)
	36608
	36036






                                                          
 
[bookmark: _Toc13246198]Figure 9: number of LRT trams assigned in each route
 Source: Addis Ababa Light railways and railways corporation office, 2019                                                               Figure 5: number of LRT trams assigned in each route

The data presented in table 44 shows that the east – west direction of the route has relatively high number of frequency than north - south direction and figure 53 displays the east – west direction of the route has 9 numbers trams whereas the north – south is 8.




[bookmark: _Toc13246200]  Figure 10: Total LRT trams seat in each route



Figure 6: Total LRT trams seat in each route
Figure 10for presents that total seat of the trams for east – west direction is 36608 and north – south direction is 36036.


[bookmark: _Toc11760188][bookmark: _Toc13425801]5.2.2. 5.1.3. Baseline data for bus and LRT route length, stops and frequency within Woredas
 
	Baseline data of Anbessa bus route length, stop and frequency

	Woreda ID
	population
	Area (sq.km)
	Density (pop/area)
	Route length within woreda
	No. of bus stop within woreda
	Total frequency within woreda

	01
	37120
	5.26
	7057
	2.62
	5.75
	99.5

	02
	38322
	4.42
	8670
	2.76
	3.5
	48.5

	03
	40869
	3.23
	12653
	0
	0
	0

	…
	…
	…
	…
	…
	…
	…

	97
	39844
	6.11
	6521
	6.1
	6.3
	102.5

	98
	21860
	13.47
	1623
	3.08
	2.3
	104

	99
	8013
	29.09
	275
	3.18
	2
	24


Table 55: Baseline data of Anbessa bus route length, stop and frequency
Source: computed by the researcher, 2019
The above table 55 illustrates sample of the 99 woredas data; mainly it shows Anbessa bus route lengthroute length, stops and frequency. 









[bookmark: _Toc13246201]Figure 117: Anbessa bus route length and coverage in woredas
The above figure 115 data shows that 78 numbers of Woredas which is the highest proportion have route length within 0 to 3.75 range whereas the remaining woredas have relatively high route coverage. Related with number of stops the figure shows that 47 woredas have 0 to 3.75 numbers of stops which is relatively low than the remaining few woredas number of stops coverage.
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


	Baseline data of Sheger bus route length, stop and frequency

	Woreda ID
	population
	Area (sq.km)
	Density (pop/area)
	Route length within woreda
	No. of bus stop within woreda
	Total frequency within woreda

	01
	37120
	5.26
	7057
	0.62
	1.3
	665

	02
	38322
	4.42
	8670
	0.34
	1.5
	19.5

	03
	40869
	3.23
	12653
	0
	0
	0

	…
	…
	…
	…
	…
	…
	…

	97
	39844
	6.11
	6521
	4.67
	3.5
	69

	98
	21860
	13.47
	1623
	0.32
	0.5
	34.5

	99
	8013
	29.09
	275
	5.66
	4
	58


[bookmark: _Toc11654694] Table 66: Baseline data of Sheger bus route length, stops and frequency
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


Source: computed by the researcher, 2019









[bookmark: _Toc13246202]Figure 128: sheger bus route length and bus stops within Woredas
Table 66 describes about mainly the 99 woredas of Sheger bus route length and bus stops coverage. Based on figure 126 around 86 woredas have route length between 0 and 3.75 range, 10 woredas have route length between 3.76 up-to 7.50 range whereas the remaining woredas have relatively high route length. Related with Woredas bus stop coverage; 79 woredas have 0 to 3.75 stops and 17 woredas have between 3.76 up-to 7.50 range stops coverage. The rest woredas have relatively high number of stops coverage.


[bookmark: _Toc11654695]Table 77: Baseline data of LRT route length, stop and frequency
	Baseline data of LRT route length, stop and frequency

	Woreda ID
	population
	Area (sq.km)
	Density (pop/area)
	Route length within woreda
	No. of LRT stops within woreda
	Total frequency within woreda

	01
	37120
	5.26
	7057
	0
	0
	0

	…
	…
	…
	…
	…
	…
	…

	25
	38322
	4.42
	8670
	1.71
	1
	32

	26
	40869
	3.23
	12653
	0.59
	1.5
	32

	…
	…
	…
	…
	…
	…
	…

	83
	39844
	6.11
	6521
	0.77
	0.5
	32

	84
	21860
	13.47
	1623
	1.58
	1.5
	32

	…
	…
	…
	…
	…
	…
	…

	99
	8013
	29.09
	275
	0
	0
	0


Source: computed by the researcher, 2019








[bookmark: _Toc13246203]Figure 139: Total LRT route length and stops within woredas
Table 77 describes mainly LRT route length and stops data within 99 woredas. The figure 137 shows that 85 Woredas have between 0 and 0.75 route length, 9 Woredas have between 0.76 and 1.50 route length; whereas the remaining Woredas have relatively high route length. The figure also shows total LRT stops within Woredas; 78 woredas have between 0 – 0.75 number of stops, 16 Woredas have between 0.76 – 1.50 stops and the remaining woredas have relatively high number of stops coverage.

[bookmark: _Toc11760189][bookmark: _Toc13425802]5.2.3. 1.2. Baseline data of statistical analysis


 
[bookmark: _Toc13246204]           Figure 1410: Gender (female) distribution in woredas
The map and bar graph (figure 814) shows that 56 woredas have 18682 - 34555 female distribution which is presented on the map with light grey color, 33 woredas have 2807 - 18681 female, 6 Woredas have 34556 - 50428 female and 4 Woredas have 504229 - 66302 number of female distribution which is indicated on the map with dens black color. The map color intensity shows that some periphery woredas have medium and high gender (female) distribution whereas the remaining part of the city indicated on the map have low and very low female distribution intensity. In the other way low and very low female distribution intensity indicates that there is high male distribution.
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[bookmark: _Toc13246205]   Figure 1511: Age distribution within Woredas
The map shows distribution and intensity of each age category in all Woredas. The bar graph (figure 159) presents that age between 25 to 54 category populations covers highest proportion, age between 0 to 14 and age between 15 to 54 categories takes the next proportion; the rest age categories takes small proportion relatively.
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[bookmark: _Toc13246206]                                                        Figure 12: Expenditure distribution in Woredas[bookmark: _Toc13246207]Figure 16: Expenditure distribution in Woredas

The map describes about intensity of each expenditure category distribution across the Woredas and the bar graph shows expenditure proportion of the population in each Woredas. According to the bar graph (figure 1610) expenditure (5) takes the largest proportion and expenditure (4) takes the second proportion which indicates high income population whereas the rest expenditures which indicate medium and low income group are small in proportion. 

		
[bookmark: _Toc13246208]                             Figure 1713: Labor force distribution in Woredas
In Figure 11 17 the bar graph shows that 87 woredas have 4042 to 54669 labor forces, 6 Woredas have 54670 to 105296 labors force, 5 Woredas have 105297 to 15 5923 labor force and one woreda has the maximum labor force distribution. The map also displays intensity of labor force distribution across woredas. According to the map west and east direction of the city Woredas have low, medium and high intensity of labor force whereas the rest part of the city woredas have very low labor force intensity. 


5.3. [bookmark: _Toc11760190][bookmark: _Toc13425803]5.2. Result on capacity, frequency and coverage
The spatial analysis includes the three public transit services frequency, capacity and coverage within the city of Addis Ababa at Woredas level. In the spatial analysis maps were produced Using GIS to show the service distribution across the city woredas. The maps were displayed in four equal interval quantities of graduate colors to show the public transit service intensity. The graduate colors starting from dense black to light gray represents high service intensity, intermediate service intensity, low service intensity and almost no service in the traffic analysis zone (woreda). The spatial analysis also presented by graphs in addition to maps.
The result of transit availability index is compared with socio economic and demographic characteristics of woredas using graphs with simple regression equations to show the relationships of each two variables. In addition to that periphery woredas with condominium residential neighborhoods are identified and this Woredas are analyzed in-terms of transit availability index and socio-economic characteristics of Woredas. The result of relationship between socio-economic characteristics of periphery woredas with condominium residential neighborhoods and public transit availability index of the city are compared and contrasted each other. Therefore, the result of relationship shows the positive and negative impact of the index over the Woreda demographic and socio-economic characteristics.
The analysis clearly responds the three objectives of the study. The first objective was to evaluate public transit availability; the second objective was evaluating the intensity of public transit availability difference between the city center and periphery city areas and the last objective was about the socio-economic impact of the public transit availability at the suburb condominium neighborhoods of Addis Ababa. The result of the objective are presented and discussed as follows.
5.3.1. [bookmark: _Toc11760191][bookmark: _Toc13425804]5.2.1. Anbessa bus frequency, capacity and coverage score 


[bookmark: _Toc13246209]Figure 1814: Anbessa Bus Frequency Score Distribution across Addis Ababa city Woredas









[bookmark: _Toc13246210]            Figure 13: Anbessa Bus Frequency Score Distribution across Addis Ababa City WoredasFigure 19: Anbessa Bus Frequency Score Distribution across Addis Ababa City Woredas
According to figure 182 and 193 Anbessa bus frequency map and bar graph shows large part of the city woredas as presented on the graph (70 woredas) has less or almost no transit frequency. Low frequency of the bus service availability is dispersed in 25 woredas of the city. These low frequency of the service showed in south part of the city around Saris and Kality, in the North - East part of the city around Yeka Abado, in North - West part of the city around Torhayloch and Asco , in the North part of the city around Addisu Gebeya, the rest low frequency service are visible in inner part of the city. Moderate frequency of the service showed around Shiromeda and Karalo. High frequency service is showed around Piassa. 
Most Woredas of the city with condominium residential neighborhood as shown on the map have almost no Anbessa bus service frequency. However few Woredas with condominium residential neighborhood around North – East, North - West and south direction of the city have low Anbessa bus service frequency.


	
[bookmark: _Toc13246211]	Figure 2015: Anbessa bus capacity score distribution in the city Woredas

[bookmark: _Toc13246212]Figure 2116: Anbessa bus capacity score distribution in Addis Ababa city Woredas
The bus capacity score is the amount of relationship between public transit service and population in woredas. According to the map (figure 2013) and bar graph (figure2114) 85 Woredas have almost no capacity score which is presented on the map with light grey color , 12 Woredas have low capacity score , one1 Woreda has moderate capacity score and one1 Woreda has high capacity score with dense black color which is located around Piassa on the map. 
Periphery woredas with condominium residential areas have almost no Anbessa bus capacity score except Woredas around Jemo and Yeka Abado condominium residential neighborhoods.
The result indicates that most Woredas of the city including periphery residential neighborhoods have high population proportion with low total number of anbessa bus distribution. Hence the existing quantities of Anbessa buses are less in providing the transit service for the available population size in most woredas.



[bookmark: _Toc13246213]Figure 2217: Anbessa bus capacity score distribution in Addis Ababa city Woredas

[bookmark: _Toc13246214]Figure 2318: Anbessa bus Capacity coverage score distribution in Addis Ababa city Woredas
Bus coverage score shows density of transit services in each woredas or it explains how much numbers of stops are available in square kilometer within transit analysis zone (Woreda). Based on this fact the map (figure 2215) and the bar graph (figure 2316) shows that 49 Woredas have almost no Anbessa bus coverage, 33 Woredas have low coverage and 14 Woredas have high coverage.
The map clearly presents the inner part of the city Woredas have low to high Anbessa bus coverage score whereas the rest of the city Woredas have almost no service coverage. Therefor there is no periphery woredas with condominium residential neighborhoods lays in low to high Anbessa bus coverage score.
The result of Anbessa bus coverage indicates that the numbers of stops within periphery woredas are low. These periphery Woredas are not well covered in number of stops in relation with its size. However, the inner city’s Woredas relatively have better Anbessa bus service distribution in-terms of density of stops.
5.3.2. [bookmark: _Toc11760192][bookmark: _Toc13425805]5.2.2. Sheger bus frequency, capacity and coverage score


[bookmark: _Toc13246215]Figure 2419: Sheger bus frequency distribution in Addis Ababa city Woredas








[bookmark: _Toc13246216]Figure 2520: Sheger bus frequency score distribution in Addis Ababa city Woredas
According to the bar graph (figure 2518) 71 Woredas presented almost no frequency, 13 Woredas have low frequency and moderate frequency and two Woredas have high frequency. The bar graph results are also shown on the map (figure 1724); according to the map most Woredas are displayed in light grey color which represents almost no Sheger bus frequency. However few Woredas in North – East and South – West direction of the city Woredas have Moderate bus frequency distribution.
Sheger bus has better frequency distribution in Jemo and Yeka Abado condominium residential neighborhoods which are located in the city Periphery Woredas. Nevertheless, the rest condominium residential neighborhoods are almost not covered by the bus frequency distribution as presented on the map (figure 1724). 
Sheger bus frequency score result indicates that, the number of buses arriving in Woredas where Yeka Abado and Jemo condominium residential neighborhoods located are Moderate. However, Sheger bus in the remaining woredas has less movement.  



[bookmark: _Toc13246217]	Figure 2621: Sheger bus capacity score distribution in Addis Ababa city Woredas

[bookmark: _Toc13246218]Figure 2722: Sheger bus capacity score distribution in Addis Ababa city Woredas
The figure 270 shows that 87 Woredas are identified with almost no capacity score, 9 Woredas have low capacity, two Woredas have moderate capacity and one Woredas has high capacity score of Sheger bus service. The result is also presented by the map (figure2619); it shows most Woredas are within light grey colors which are high in proportion, the East and south - west direction of periphery Woredas are within low bus capacity score. Moderate capacity score distribution is observed on the map in the south direction of the city.
According to the map (figure2619) most periphery condominium sites are covered with low capacity score and one condominium residential neighborhood have moderate capacity score. The remaining Woredas with condominium residential neighborhoods lay with almost no capacity score distribution.
Therefor Sheger bus capacity score result indicates that relatively better numbers of bus are available in periphery Woredas than in the inner city woredas. Nevertheless, these Woredas are still has low capacity score. 


[bookmark: _Toc13246219]	Figure 2823: Sheger bus capacity score distribution in Addis Ababa city Woredas









[bookmark: _Toc13246220]Figure 2924: Sheger bus coverage score distribution in Addis Ababa city Woredas
The coverage score of sheger bus as it is shown on the graph (figure 292) 63 woredas lay in almost no frequency, 25 Woredas have low frequency score, three Woredas have moderate frequency score and 8 Woredas have high frequency score. 
The map (figure 281) presents the coverage score distribution in graduate color from light grey to dense black. According this map better coverage score is shown in inner city Woredas whereas the rest of the city woredas including the periphery woredas lay in light grey color which represents almost no coverage score. As a result, condominium residential neighborhoods within these Woredas have very low coverage score. 
The result of Sheger bus coverage score indicates that the density of bus stops in relative with the sizes of Woredas is very low in periphery Woredas of the city. Nevertheless, the bus service coverage in inner city Woredas has better intensity.



5.3.3. [bookmark: _Toc11760193][bookmark: _Toc13425806]5.2.3. LRT frequency, capacity and coverage score



[bookmark: _Toc13246221]Figure  Figure 3025: LRT frequency score distribution in Addis Ababa Woredas

 







[bookmark: _Toc13246222]Figure 3126: LRT frequency score distribution in Addis Ababa Woredas
According to figure 3124 the LRT frequency score result indicates that 92 Woredas are represented in very low or almost no frequency score, 4 Woredas have low frequency score, one Woreda has moderate frequency score and two Woredas have high frequency score. The bar graph (figure 3124) LRT frequency result is also displayed in the map (figure 3023) except few Woredas in the inner city all Woredas lays in light grey color which represents almost no LRT service frequency. The LRT frequency score which are represented in high and low values in the inner city Woredas are observed. These observable frequency score distribution is found in the overlapped route from Stadium to Lideta.
The East – West LRT route is a bit close to periphery Woredas residential condominium neighborhoods than North – South route. However, the LRT frequency score is very low in these Woredas like most Woredas of the city.
The LRT frequency score distribution result indicates that the number of LRT trams with its headway time arrived in each station is not sufficient.



[bookmark: _Toc13246223]Figure 3227: LRT capacity score distribution in Addis Ababa city Woredas










[bookmark: _Toc13246224]Figure 3328: LRT capacity score distribution In Addis Ababa Woredas
	The capacity score of LRT transit service as shown in the bar graph (figure 2633) almost 94 woredas have very low or no capacity score, three Woredas have low capacity score and two Woredas have high capacity score. The LRT capacity score which are indicted in high and low capacity score (figure 32 25) are easily observed in inner city Woredas around the overlapped route. Specifically high capacity score of LRT displayed on the map (figure 2326) are around Stadium and and Lideta junctions.
The LRT capacity score from high to low value is not observed in other Woredas except few Woredas in the inner city. As a result all periphery Woredas with condominium residential neighborhoods are not accessed by the LRT service.
The result of LRT capacity score distribution indicates that the number of LRT trams assigned and route length is not proportional with available population density of Woredas.




[bookmark: _Toc13246225]Figure 3429: LRT coverage score distribution in Addis Ababa city Woredas










[bookmark: _Toc13246226]Figure 3530: LRT coverage score distribution in Addis Ababa city Woredas
According to bar graph (figure 3528) 81 Woredas are under very low or no coverage score, 11 Woredas have low coverage, 5 Woredas have moderate and two Woredas have high coverage score. The result is also presented in the map (figure 3428); except few woredas that the LRT route passes through other Woredas touched by the route have low to high coverage score. The intensity of coverage score of Woredas with LRT route increases towards the inner city.
According to the map (figure 3427) periphery Woredas with condominium residential neighborhood have very low or no coverage at all.
The result indicates that LRT service coverage in the inner city is relatively proportional with Woredas boundary area than Woredas to the periphery.


5.3.4. [bookmark: _Toc11760194][bookmark: _Toc11922785][bookmark: _Toc13425807]5.2.4. Total frequency, capacity and coverage score of the three public transit services


[bookmark: _Toc13246227]Figure 3631: Public transit total capacity score distribution in Addis Ababa city Woredas








[bookmark: _Toc13246228]Figure 3732: Public transit total frequency score distribution in Addis Ababa city Woredas
The total frequency score according to the bar graph (figure 370) shows that 63 Woredas represented in very low or almost no frequency, 22 woredas have low frequency, 12 Woredas have moderate frequency and two Woredas have high frequency score. According to the map (figure 3629) Woredas with high frequency score are located in inner city and Woredas with moderate frequency are located in North – East direction of the city and low frequency score are shown in the South – West as well as in inner city Woredas. The remaining Woredas with highest proportion lay under very low or almost no frequency score.
The frequency score in Woredas with periphery condominium residential neighborhoods as shown on the map (figure 3629); North – East direction of the city Woredas have moderate frequency score whereas South – West and North direction of the city Woredas have low frequency score distribution.
The total frequency score distribution result indicates that high number of total daily buses arrived from Stadium to Piassa transit corridor Woredas. There is moderate total daily number of buses arrived in North – East direction of the city Woredas and low number of total daily buses in South – West direction of the city Woredas. Nevertheless, the remaining Woredas of the city have very low or almost no total number of daily bus arrived.


[bookmark: _Toc13246229]Figure 3833: Public transit total capacity score distribution in Addis Ababa Woredas











[bookmark: _Toc13246230]Figure 3934: Public transit total capacity score distribution in Addis Ababa city Woredas
The total capacity score as shown on bar graph (figure 392) 85 Woredas of the city lies in very low capacity score, 10 woredas have low capacity score, three Woredas have moderate capacity and one Woreda has high capacity score. These result presented on the map (figure 381) also shows high capacity score in inner city woredas around Stadium and Beherawi  and Moderate capacity score distribution is shown around Mekanisa. The map shows low capacity score around South – West and North – West part of the city Woredas. The rest part of the city Woredas are within very low or almost no capacity score. 
The capacity score in periphery woredas with condominium residential neighborhoods is low in the North – East and South – East part of the city Woredas whereas the rest periphery woredas with condominium residential neighborhoods of the city are very low. 
The result shows that in most part of the city Woredas the number of population and the number of total daily buses availability is not balanced. As a result, the number of total daily bus assigned in each route is low. It also shows that there is limited route length in Woredas.


[bookmark: _Toc13246231]Figure 4035: Public transit total coverage score distribution in Addis Ababa city Woredas

[bookmark: _Toc13246232]Figure 4136: Public transit total coverage score distribution in Addis Ababa city Woredas
The total coverage score of the city Woredas are shown in the map (figure 4033) and the bar graph (figure 4134). According to the bar graph 50 Woredas capacity score distribution lay in very low or almost no coverage, 32 Woredas have low coverage score, 14 Woredas have moderate coverage and three Woredas have high capacity score. Based on the map high to low transit coverage sore is shown in inner city Woredas. Periphery woredas transit coverage score is very low or almost no coverage.
The periphery Woredas with condominium residential neighborhood lies in very low or almost no coverage score.
The result of total transit coverage score shows that in the inner city Woredas; there is well coverage in number of transit stops in relative with the periphery Woredas transit coverage. The periphery Woredas boundary size and distribution of transit stops are not balanced. As a result, low transit coverage score shown in the map. 


5.3.5. [bookmark: _Toc11760195][bookmark: _Toc13425808]5.2.5. Standardized overall public transit availability index of Addis Ababa city 


[bookmark: _Toc13246233]Figure 4237: standardized overall transit availability index of Addis Ababa city Woredas









Figure 4338: Standardized overall public transit availability score of Addis Ababa city Woredas
The standardized public transit availability score of the city Woredas is the final sum output of each public transit standardized frequency, capacity and coverage score of the transit services. As it is presented on the graph (figure 3643) 64 Woredas of the city lies in almost no transit availability range, 24 Woredas have low transit availability, 8 Woredas have moderate transit availability and three Woredas have high transit availability. The map (figure 4235) shows that Woredas with high transit availability is displayed in inner part of the city around Stadium, Legehar, Bherawi, Piassa and Awtobs Tera. Moderate transit availability is displayed around Megenagna, Torhayloch,  Arat killo and Mekanisa. Low transit availability is shown in the North part of the city around Mikilily land condominium, North – East around Yeka Abado and South – West around Jemo. The remaining low transit availability index is shown on the map in inner part of the city Woredas. However, most part of the city Woredas lies in very low or almost no transit availability index.
The result indicates that public transit availability is low or almost not available in all periphery Woredas with condominium residential neighborhoods whereas relatively inner part of the city Woredas have low to high transit availability.


                   
[bookmark: _Toc13246234]Figure 4439: comparison between population density and public transit availability index








[bookmark: _Toc13246235]	Figure 4540: Intensity of public transit availability in Woredas                                          Figure 4641 Population density in Woredas
Based on four equal interval population density ranges, Woredas with very low population density are 38 and Woredas with high population density are 12 (figure 4639).  The population density distribution is mapped as shown in figure 4437. Based on the  map low to high population density is displayed in the inner part of the city Woredas whereas the rest part of the city Woredas lies in very low population category. When the population density is compared with transit availability index as shown on the map (figure 4437); inner part of the city Woredas as well as South –East and North – East part of the city Woredas have low to high public transit service. The remaining Woredas including the peripheries have almost no transit service and very low population density. Low population and low transit service shows that there is no or limited number of public transport service provision for less number of population at the periphery and other part of the city Woredas.



[bookmark: _Toc13246236]Figure 4742: Periphery woredas condominium residential neighborhoods in comparison with public transit availability index





	


[bookmark: _Toc13246237]Figure 4843: periphery Woredas with condominium residential neighborhood
The map (figure 4737) and the graph (figure 4838) show that 11 periphery woredas with condominium residential neighborhoods such as Bole Ayat, Bole Arabse, kilinto, etc. lies in almost no transit availability index, three Woredas with Yeka Abado, Yeka Ayat, and Jemo condominiums have low transit service intensity and one Woreda around Mekanisa has moderate service intensity. According to the Woreda population and public transit index graph, Woredas with high and low population density lies in almost no service intensity but Woredas with high service intensity have average population density. 
Therefore, the result indicates that periphery condominium residential neighborhoods have low transit coverage.
5.3.6. [bookmark: _Toc11760196][bookmark: _Toc13425809]5.2.6. Public transit availability index and Socio – economic characteristics of periphery Woredas with condominium residential neighborhood simple regression analysis result
     	Periphery woredas with condominium residential  neighborhoods sSocio-economic and demographic variables are compared with public transit availability index as dependent variables whereas transit availability is independent variable in the result and discussion below.                  
    
[bookmark: _Toc13246238]Figure 4944: Transit availability index and gender relationship in periphery Woredas with condominium
The figure 490 shows that the relation between female and public transit index is positive. Based on the figure gender distribution is affected in the change that occurs in public transit availability by 56% as R square shows.







[bookmark: _Toc13246239]Figure 5045: Age (0 - 14) and public transit availability index relation
The result shows Age (0 – 14) is affected in public transit availability by 57%.








[bookmark: _Toc13246240]Figure 5146: Age (15 - 24) and public transit availability index relation
The result (figure 5141) shows that age (15 -24) is affected by transit availability index in 54 percent. This age category is active working age which demands transit service to get and to actively engage in their jobs.
	






[bookmark: _Toc13246241]Figure 5247: Age (25 -24) and public transit index relation
The age (25 – 54) has positivestrong relation with transit availability index. The change in 1 unit in the transit index affectsThe transit availability affects the age group the age group by 61 percent. It also shows there is a likelihood of this working age to exist around public transit serviced area. This age group according to CSA (2016) categorized as matured wWorking age. As a result, to engage in their job they demand high transit availability.





	




[bookmark: _Toc13246242]Figure 5348 : Age (55 - 64) and public transit availability relation
This age group has strong positive relation with the public transit availability index. It is also matured working age which demands public transit serviceshows that there is a likelihood of existing age 55 to 64 around public transit serviced area.







[bookmark: _Toc13246243]Figure 5449 : Age 65 and public transit availability relation
The figure shows that the age 65 and above has strong positive relation with public transit availability. As the figure shows the change in one unit in public transit availability has 62 percent positive impact on age 65 and above.







     
[bookmark: _Toc13246244]  Figure 5550: Labor force and public transit index relation
The labor force variable has strong positive relation with public transit index. As a result, the increase in public transit service in one unit will change the labor force in 62 percent.






[bookmark: _Toc13246245]Figure 5651: Very low expenditure and public transit availability index
Based on CSA 2016 socio-economic data document, income data is replaced by expenditure. CSA categorized the community based on annual expenditure into five. Very poor (<=5379.48birr), poor (5379.81 birr – 7688.06birr), medium income (7688.11 – 10121.95), high income (10123.36 – 15109.21), very high income (>=15110.22). According to figure 5649, very low expenditure has positive relationship with public transit availability. Therefore, expenditure is 52 percent positively affected by the change in public transit availability.



	


	


 
[bookmark: _Toc13246246]Figure 5752: very high expenditure and public transit relation
Very high expenditure has positive relation with public transit availability. Hence the change in public transit service in Woredas brings 53 percent change in expenditure.The public transit availability affects high expenditure by 53 percent. 
[bookmark: _Toc11760197][bookmark: _Toc13425810]5.4. Discussion
The findings from this study suggest that socio-economic characteristics of periphery Woredas condominium residential neighborhoods are influenced by the intensity of public transit availability. 
The result indicates that public transit availability is low or almost not available in all periphery Woredas with condominium residential neighborhoods whereas relatively inner part of the city Woredas have low to high transit availability. As McKenzie (2013) study shows compared to compact urban centers or inner cities, transit availability in suburb communities is relatively poor in most metropolitan areas. The reason behind is that peripheries condominium residential developments are not well integrated by public transportation with inner cities in terms of availability of adequate public transit route , number of stops and number of transit service. The other reason for low intensity of transit availability is that a number of transit services are using the same route and this affects the spatial distribution of the service in terms of transit stops and route coverage through the Woredas. Which means communities who are far away from the transit route cannot access the service in walking distance. According to Abreha (2007) study, the higher the spatial coverage of the service the shorter will be the walking distance to the service. The unbalanced periphery Woredas boundary and population size with the distribution of transit stops route coverage and number of transit can also contribute for low coverage of transit at the periphery residential neighborhoods. But in the other way condominium residential neighborhoods are dense settlements which are easy to provide transport infrastructures from the perspective of getting riders in a specific point. 
The result of total transit coverage score shows that the inner city Woredas has well coverage of transit availability. This is because of adequate number of transit stops, route and number of bus availability in relative with the periphery Woredas transit coverage. According to Scott (2014) spatial mismatch research has found that transportation access has a positive relationship with employment outcomes whereas housing and employment discrimination have a negative relationship with the spatial mismatch of jobs and housing. This literature proves the result of transit availability and socio-economic characteristics of the periphery woredas with condominium residential neighborhoods correlation. As the results show socio-economic and public transit availability have strong positive relationships. This result is analyzed and presented by simple regression analysis and the strength of the relation is presented using R2. According to Etenesh (2007) study in periphery condominium areas female headed households compared to their male counterparts prone to economic challenges. 
Therefore, less transit availability has negative impact on the residents of periphery condominiums. Based on Woldeamanuel and Covington (2014) study a portion of Americans relies on various modes of public transit for commuting. As they discussed great portion of members in low-income, elderly and minority households are depend on public transit. As a result, the intensity (high and low) of transit availability in periphery area has positive or negative impact on the socio-economic characteristics of the neighborhoods.














[bookmark: _Toc11760198][bookmark: _Toc11916422][bookmark: _Toc11922789][bookmark: _Toc13125178][bookmark: _Toc13241204][bookmark: _Toc13245350][bookmark: _Toc13246901][bookmark: _Toc13425811]CHAPTER SIXSIX: 
[bookmark: _Toc11760199][bookmark: _Toc13425812]CONCLUSION AND RECOMMENDATION
[bookmark: _Toc11760200][bookmark: _Toc13425813]6.1. 6.1. Conclusion 
The research condominium boom in Addis Ababa and public transit mismatch evaluation is done based on the problems that are observed in the city. It is more of emphasized on its periphery condominium residential neighborhoods socio – economic and demographic characteristics in relation with public transit availability.
For the problems identified in the research problem statement three objectives and research questions were formulated. Then after, the methodology is designed to achieve objectives and to answer research questions. The analysis method developed to answer objective research questions one and two was ABLSIIA (Addis Ababa bus and LRT service index availability) whereas objective three was answered using simple regression method.
ABLSIA was developed by calculating the capacity, frequency and coverage of Anbessa , Sheger and LRT public transit services within 99 traffic analysis zones (Woredas).The calculated and standardized result of each transit service capacity, frequency and coverage were added  to give overall transit availability index of the city Woredas. Then after the overall transit availability index were joined in GIS to produce the result of the first two objectives in the form of spatial analysis or maps.
The result of the first objective is that transit service availability in the periphery suburban condominium residential neighborhoods is low. This result is shown in Anbessa , Sheger and LRT public transit services capacity , frequency and coverage score. It is also shown in the total score of three transit services capacity, frequency and coverage scores. Finally low availability of public transit service is shown in the standardized sum of three transit services availability scores.
According to the overall transit availability index (figure 4235) the second objective result shows that there is a difference in the intensity of public transit service availability between the city center and periphery Woredas with condominium residential neighborhoods. Periphery woredas with condominium residential neighborhoods lies between low and almost no transit availability scores whereas the inner part of the city Woredas lies in between low and high transit availability index.
 Simple regression analysis method is used to answer the third objective research question of the study. In the simple regression analysis method scatter plot graph type and trend line is used to identify the relationship between the socio-economic and demographic impact of public transit availability at the periphery condominium residential areas. The result of simple regression analysis interpreted based on R2 value which lies between 0 - 1 and the independent variable coefficient. If the independent variable coefficient is negative then the two variables have negative relationship. This is to mean when independent variable increase, the dependent variable decrease and the reverse is true. The R2 value has to be greater than or equal to 0.5 in order to have the two variables strong positive relationship. Therefore, the result of the study regression analysis R2 shows that public transit availability and periphery Woredas socio-economic and demographic characteristics have strong positive relationship. Periphery Woredas socio-economic and demographic characteristics that are compared with public transit index are gender, age, labor force and expenditure. Each of these periphery Woredas characteristics has R2 greater than 0.5 values which indicates strong positive relationship between variables in the study.

[bookmark: _Toc11760201][bookmark: _Toc13425814]6.2. Recommendation 
In this study, analysis and discussions have been carried out to evaluate transit availability in the periphery Woredas condominium residential neighborhoods. As seen from the evaluation, it is clearly identified the neighborhoods low intensity of public transit service availability. Based on the evaluation carried out in the previous chapter, recommendations are proposed to improve the public transit availability in periphery residential condominium neighborhoods of Addis Ababa city. 
There should be possible solutions by state/municipal government in short and medium term to improve the availability of public transit service. According to the public transit availability in the peripheral condominium residential neighborhoods, the study area needs the following recommendations which were outlined based on the evaluated findings.
1. Providing additional and extending the existing public transit routes
Based on the result Woredas with low and almost no transit service availability are because of limited or overlapped number of public transit routes. The presence of limited or overlapped routes influences the transit service provision in the negative way. The reason behind is that it limits the service availability across woredas or the riders cannot access the service easily in proximity with their residence. Therefore, in order to get the service they have to walk long distance. As a result, the route has to be provided with walking distance of the riders to increase the transit availability in the area. The increase in transit service availability of periphery Woredas would benefit the socio-economic and demographic characteristics. The route helps to connect woredas community with inner part of the city in terms of social, economic and recreational purpose.  

1. Increasing density or number of stops in the provided public transit routes
Stops density is one factor for the result of low or no transit service availability in periphery Woredas with condominium residential neighborhoods. When the number of stops in an area exists in walking distance then riders have the chance to get the transit service frequently.
1. Increasing the number of Anbessa bus, Sheger bus and LRT trams in the route.
According to the result discussed in chapter five the numbers of bus and LRT transit services are the leading factor that affect the transit availability of Woredas. As the result shows the number of transit availability and Woredas population density is not balanced. The current transit service even is not available in low population density as it is shown in the result and discussion part of the study. Therefore, the number of transit services should be provided by considering the number of population, the standard carrying capacity and headway or frequency of buses and LRT transit services. 

Future studies related with spatial analysis of public transit availability for cities should include primary socio-economic data in addition to secondary data to triangulate the result of relation between intensity of transit availability and socio-economic characteristics.
Further studies are recommended for Woredas that have low and almost no public transit availability index route design in order to alleviate the spatial distribution and proximity of the transit service by considering primary socio-economic data.
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	 route No.
	



Origin-Destination
	No. of buses 
	Frequency per bus 
	Total daily bus frequency within route
	Total daily bus seats
	Trip Time (Min.)
	km

	1
	Megenagna     -    Karalo
	4
	5
	20
	1400
	33
	7.7

	2
	Kore  Mekanissa     -     Addis Ketema
	3
	6
	18
	1260
	54
	11.1

	3
	Ayer  Tena     -     Menelik   Squar
	8
	5
	40
	2800
	60
	10.8

	4
	Kaliti        -   Addis  Ketema
	4
	3
	12
	840
	80
	19.4

	5
	Kore Mekanissa    - Menelik Squar
	2
	2
	4
	280
	53
	12.7

	6
	Kera       - Semen  Gebeya  Squar
	8
	5
	40
	2800
	52
	9.9

	7
	Megenagna  -   Aleltu  
	3
	7
	21
	1470
	100
	49

	8
	Kechene   -   Addis  Ketema
	2
	8
	16
	1120
	38
	9.4

	9
	Bole Brass Clinic - Piassa
	2
	2
	4
	280
	49
	10.5

	10
	Kotebe  College -  Piassa
	5
	14
	70
	4900
	53
	12.7

	11
	Kolfe  Efoyeta  -   Menelik Hospital
	2
	4
	8
	560
	49
	10

	12
	Gurara Ferensay Kela - Addis Ketema
	6
	7
	42
	2940
	44
	9.9

	13
	Italy   Embassy  -   Addis Ketema
	3
	2
	6
	420
	48
	9.9

	14
	Saris Abo  -   Menelik   Squar
	3
	3
	9
	630
	60
	12.3

	15
	Megenagna     -   Addis Ketema
	4
	5
	20
	1400
	53
	10.4

	16
	Kidanimihret   -  Addis  Ketema
	6
	3
	18
	1260
	42
	7.9

	17
	Kusqum     -    Addis Ketema
	4
	4
	16
	1120
	49
	9.1

	18
	Keraniyo    -    Addis Ketema
	6
	9
	54
	3780
	48
	7.3

	19
	Sansusi     -   Piassa 
	5
	9
	45
	3150
	48
	12.8

	20
	Dil Ber    -   Addis Ketema
	2
	6
	12
	840
	41
	8.6

	21
	Felidoro    - Addis Ketema
	6
	3
	18
	1260
	52
	8.6

	22
	Summit     -   Legehar
	6
	4
	24
	1680
	58
	14.3

	23
	Lamberet   -   Addis  Ketema
	5
	6
	30
	2100
	53
	12

	24
	Dire  Sololiya  -Addis Ketema
	4
	5
	20
	1400
	70
	15.9

	25
	Legehar     -     Akaki
	3
	4
	12
	840
	80
	19

	26
	Addis Ketema  -   Sebeta
	4
	9
	36
	2520
	74
	25.5

	27
	Legehar   -  Kaliti
	3
	2
	6
	420
	65
	14.9

	28
	Asko Sansuzi  -Addis  Ketema
	3
	7
	21
	1470
	51
	11.1

	29
	Saris  Addisu Sefer  - Addis Ketema
	4
	5
	20
	1400
	58
	12.7

	30
	Sululta    -Addis Ketema
	2
	10
	20
	1400
	70
	25.8

	31
	Legehar   -Shiro  Meda
	5
	10
	50
	3500
	35
	7.4

	32
	Hana Mariam  -Legehar
	6
	2
	12
	840
	51
	10.6

	33
	Kotebe Gebriel  -   Arat Kilo
	5
	6
	30
	2100
	40
	11.4

	34
	German  Squar         -      Addis Ketema
	2
	4
	8
	560
	52
	9.8

	35
	 Lebu Muziqa  Sefer-  Addis Ketema
	2
	2
	4
	280
	60
	15

	36
	Kara Kore  -   Legehar
	3
	5
	15
	1050
	55
	11.7

	37
	Keraniyo    -   Menelik  Squar
	3
	3
	9
	630
	60
	12

	38
	German  Squar   -   Sidist  Kilo
	3
	3
	9
	630
	60
	11

	39
	Bole School -  Addis  Ketema
	3
	2
	6
	420
	52
	9.6

	40
	Karalo    -      Addis  Ketema
	4
	2
	8
	560
	70
	17.9

	41
	Eyesus      -  Addis Ketema
	4
	2
	8
	560
	46
	8.5

	42
	Megenagna   -    Legehar
	2
	2
	4
	280
	50
	9.8

	43
	Menagesha  -  Addis Ketema
	2
	4
	8
	560
	85
	30.2

	44
	Legedadi    -    Addis  Ketema
	2
	16
	32
	2240
	91
	30.4

	45
	Legehar    -    Dil Ber
	4
	4
	16
	1120
	46
	8.6

	46
	Gerji       -    Arat  Kilo
	4
	2
	8
	560
	55
	11.2

	47
	Yenegew  Fire School  -  Addis Ketema
	2
	5
	10
	700
	41
	6

	48
	Bole Michael - Menelik Sq;
	3
	3
	9
	630
	49
	10.9

	49
	Chefe Ayate;   -    Megenagna
	4
	10
	40
	2800
	40
	11

	50
	Ayer  Tena       -     Megenagna
	3
	20
	60
	4200
	62
	14.9

	51
	Bethel  Hospital  -  Addis Ketema
	2
	3
	6
	420
	51
	10.9

	52
	Gerji     -      Addis  Ketema
	3
	3
	9
	630
	70
	14.1

	53
	Bole  Michael   -  Shiro  Meda
	4
	3
	12
	840
	52
	11.5

	54
	Lafto      -     Legehar 
	2
	3
	6
	420
	57
	9.5

	55
	Legehar  -  Gurara  Ferensay  Kella
	4
	6
	24
	1680
	45
	9.5

	56
	Saris  Abo  -  Shiro Meda
	4
	2
	8
	560
	51
	14.2

	57
	Kara   -   Legehar
	4
	3
	12
	840
	60
	14.4

	58
	Legehalr  - Alem  Bank
	4
	3
	12
	840
	52
	12

	59
	Bethel Hospital - Menelik  Squar
	5
	5
	25
	1750
	54
	11.5

	60
	Debr Zeit -  Legehar
	4
	7
	28
	1960
	100
	47.2

	61
	Chefe Ayate  -  Legehar
	4
	6
	24
	1680
	65
	18

	62
	Sebeta  -  Legehar
	3
	7
	21
	1470
	80
	23.8

	63
	Addis Ketema  - Mikililand
	5
	3
	15
	1050
	47
	9.1

	64
	Sidist Kilo - Megenagna Gorf Aswegaj
	2
	19
	38
	2660
	46
	9.5

	65
	Addis Ketema -  Alem  Bank
	4
	3
	12
	840
	48
	11

	66
	Addis Ketema  -  Kara Qorre
	4
	3
	12
	840
	50
	10.5

	67
	Legehar  -   Jemmo  Mekanissa
	6
	7
	42
	2940
	48
	10.6

	68
	Menelik Hospital - Tore Hailoch
	2
	5
	10
	700
	46
	10.2

	69
	Lome  Meda      -       Merkato
	4
	1
	4
	280
	41
	5.9

	70
	Aware  Square  - Ayer Tena
	3
	3
	9
	630
	52
	12

	71
	Gerji  -  Balcha  Hospital
	3
	8
	24
	1680
	60
	10.9

	72
	Hana Mariam  - Sari  Abo
	4
	4
	16
	1120
	24
	4.9

	73
	Legehar  -  Ring  Road  Vis  Winget  
	4
	6
	24
	1680
	60
	10.2

	74
	Cmc Square -  Addis  Ketema
	4
	2
	8
	560
	60
	14.2

	75
	Sidist Kilo -  Qera
	2
	3
	6
	420
	47
	10.4

	76
	Megenagna -  Kaliti
	3
	4
	12
	840
	70
	18.2

	77
	Ayer Tena -  Kera
	3
	12
	36
	2520
	35
	5

	78
	Megenagna  -  Gofa  Condiminium
	4
	2
	8
	560
	60
	12.4

	79
	Arat Kilo  - Semit Condiminium
	4
	5
	20
	1400
	53
	14.7

	80
	Semen Gebeya  Squar -  Megenagna
	3
	2
	6
	420
	59
	12.4

	81
	Sidist Kilo -Sansusi
	2
	5
	10
	700
	54
	11.1

	82
	Goro Adebabay - Balcha Hospital
	3
	4
	12
	840
	59
	14.6

	83
	Chefe Ayate - Sidist Kilo
	2
	13
	26
	1820
	60
	18

	84
	Kolfe  Efoyta  - Legehar
	2
	1
	2
	140
	54
	9.5

	85
	Addis Ketema - Holeta
	3
	2
	6
	420
	90
	45

	86
	Ayer Tena    -    Korki
	3
	4
	12
	840
	55
	12.3

	87
	Winget Vis Ring Road- Ayer Tena
	2
	20
	40
	2800
	42
	10.5

	88
	Addis Ketema -Chancho
	4
	5
	20
	1400
	90
	40

	89
	Addis Ketema -Sendafa
	5
	3
	15
	1050
	110
	44

	90
	Betel Hospital - Legehar
	4
	4
	16
	1120
	55
	10

	91
	Addis Ketema - Teji
	2
	4
	8
	560
	125
	52

	92
	Hana Mariam Ring Road- Balcha
	3
	7
	21
	1470
	41
	9.6

	93
	Bole Bulbula -  Megenanga
	3
	3
	9
	630
	55
	15.2

	94
	Piassa      -      Mikililand
	6
	5
	30
	2100
	44
	9.9

	95
	Addis Ketema -  Addis  Alem
	3
	3
	9
	630
	100
	47

	96
	Megenagna  -  Goro Sefera
	2
	2
	4
	280
	31
	9.2

	97
	Megenagna -   Legetafo Mission
	3
	7
	21
	1470
	58
	15.8

	98
	Dukem  -   Saris  Abo
	4
	6
	24
	1680
	70
	26.3

	99
	Ayer Tena -  Alem  Gena Michael
	2
	8
	16
	1120
	36
	9.4

	100
	Addis Ketema - Jemo
	4
	5
	20
	1400
	51
	14.5

	101
	Megenagna -  Aba Kirros  Sq.
	3
	13
	39
	2730
	43
	12

	102
	Kara          -     Legehar
	4
	3
	12
	840
	52
	13.7

	103
	Jemo         -        Piassa
	5
	6
	30
	2100
	59
	12.2

	104
	Werku  Sefer   - Kera
	2
	5
	10
	700
	35
	8.3

	105
	Anfo Meda  -     Legehar
	4
	4
	16
	1120
	55
	12

	106
	Goro Adebabay -  Sammit Megenagna
	3
	20
	60
	4200
	50
	10.8

	107
	Saris Abo  -   Akaki  Qorqoro
	3
	7
	21
	1470
	50
	11.4

	108
	Asko Addisu Sefer - 18  Sq . Menelik Sq.
	4
	2
	8
	560
	50
	9.3

	109
	Saris Abo  -   Tulu Dimetu Square
	4
	6
	24
	1680
	45
	12

	110
	Sidist  Kilo  -Tulu Dimetu Square
	4
	3
	12
	840
	85
	24.9

	111
	Dire  Sololiya  -  Piassa
	6
	8
	48
	3360
	72
	16.6

	112
	Circular Route With In Ring Road 4 Turning Points
	6
	14
	84
	5880
	161
	9.4

	113
	Kaliti Total        -         Feche  Koye
	2
	3
	6
	420
	45
	8.1

	114
	Gelan  Condiminium  -  Saris  Abo
	5
	7
	35
	2450
	35
	7.9

	115
	Lebu Muziqa Bet  -   Mexico Square
	2
	1
	2
	140
	45
	9.4

	116
	Mekanissa Michael Sq -    Jemo  No_ 2
	3
	10
	30
	2100
	25
	5.6

	117
	Kotari Condiminnium - Mexico Square
	3
	3
	9
	630
	35
	9.2

	118
	Merkato    -   Tateq  Kella
	2
	9
	18
	1260
	70
	18

	119
	Megenagna      -   Summit Condiminnium
	4
	7
	28
	1960
	35
	9.2

	120
	Burayu Keta       -     Tore Hiloch
	2
	11
	22
	1540
	45
	12.1

	121
	Jemo Qedus Gebreal - Mexico Square
	4
	5
	20
	1400
	45
	10

	122
	Arat Kilo  -Entoto Mariam
	3
	7
	21
	1470
	31
	16.6

	123
	Megenagna - Yeka Abado
	4
	4
	16
	1120
	 
	 

	124
	Megenagna - Tulu Dimtu
	4
	4
	16
	1120
	 
	 

	 
	Total
	443
	687
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[bookmark: _Toc13425817]Appendix2: Sheger Bus Route Information
	
route No.
	

Origin -Destination
	No. of buses
	Frequency per bus
	Total daily bus frequency within the route
	Total daily bus seats (70)

	1
	Addisu Gebeya -- Bole
	1
	6
	6
	420

	2
	Adissu Gebeya -- Kera
	1
	6
	6
	420

	3
	Piassa -- Addisu Gebeya
	4
	9
	36
	2520

	4
	Piassa -- Bole
	5
	6
	30
	2100

	5
	Piassa -- Asko/wingate
	12
	9
	108
	7560

	6
	Piassa -- Kera Mebrathail
	8
	7
	56
	3920

	7
	Piassa -- Saris
	111
	6
	66
	46200

	8
	Piassa -- Betel
	4
	5
	20
	1400

	9
	Piassa -- Megenagna
	2
	6
	12
	840

	10
	Piassa -- Jemo2
	6
	6
	36
	2520

	11
	Piassa -- Ferensay
	5
	9
	45
	3150

	12
	Awtobs Tera --Alembank
	6
	7
	42
	2940

	13
	Awtobs Tera --Asko
	3
	8
	24
	1680

	14
	Awtobs Tera -- Saris Abo
	2
	6
	12
	840

	15
	Awtobs Tera - Jemo 1
	2
	6
	12
	840

	16
	Awtobs Tera -- Ashewa Meda
	3
	6
	18
	1260

	17
	Awtobs Tera -- Karakore
	3
	6
	18
	1260

	18
	Awtobs Tera -- Spain Embassy
	1
	9
	9
	630

	19
	Awtobs Tera -- Ayer Tena
	6
	8
	48
	3360

	20
	Awtobs Tera -- Kela
	3
	5
	15
	1050

	21
	Mrab Hotel -- Alem Bank
	2
	7
	14
	980

	22
	Ayer Tena -- Stadium
	2
	7
	14
	980

	23
	Ayer Tena -- Saris ABO
	2
	6
	12
	840

	24
	Ayer Tena -- Mexico
	3
	9
	27
	1890

	25
	Mexico -- Jemo2
	27
	7
	189
	13230

	26
	Mexico -- Haile Garment
	6
	9
	54
	3780

	27
	Mexico -- Hanna Mariyam
	2
	7
	14
	980

	28
	Mexico -- Sefera
	3
	7
	21
	1470

	29
	Mexico -- Alem Bank
	3
	7
	21
	1470

	30
	Mexico -- Gelan
	3
	9
	27
	1890

	31
	Mexico -- Tulu Dimtu
	4
	4
	16
	1120

	32
	Mexico -- Shiromeda
	12
	8
	96
	6720

	33
	Mexico -- Lafto
	3
	8
	24
	1680

	34
	4Killo -- Bole
	3
	6
	18
	1260

	35
	4Killo -- Ferensay
	2
	9
	18
	1260

	36
	6Killo -- Ksanchis
	1
	9
	9
	630

	37
	Shiromeda -- Saris
	2
	5
	10
	700

	38
	Shiromeda -- Bole
	3
	5
	15
	1050

	39
	Megenagna -- Yekabado
	24
	7
	168
	11760

	40
	Megenagna -- Semmit
	3
	6
	18
	1260

	41
	Megenagna -- Goro
	3
	8
	24
	1680

	42
	Megenagna -- Koye Fiche
	1
	5
	5
	350

	43
	Megenagna -- Tulu Dimtu
	7
	5
	35
	2450

	44
	Megenagna -- Saris
	4
	8
	32
	2240

	45
	Megenagna -- Tafo
	4
	5
	20
	1400

	46
	Megenagna -- Shiromeda
	2
	8
	16
	1120

	47
	Megenagna -- Pissa
	4
	5
	20
	1400

	48
	Megenagna -- Mexico
	2
	9
	18
	1260

	49
	Megenagna -- Bole Arabsa
	8
	5
	40
	2800

	50
	Goro -- Tulu Dimtu
	3
	6
	18
	1260

	51
	Yekabado -- Piassa
	4
	5
	20
	1400



[bookmark: _Toc13425818]Appendix 3: Woreda Labor force and population density distribution

	Subcity
	woreda
	Woreda
ID
	Both geneder
	Labor force 
	Area (sq.km)
	Density

	Gulele-Sub City
	KEBELE 13/14
	1
	37,120
	26,464
	5.26
	7,057

	Gulele-Sub City
	KEBELE 16/17
	2
	38,322
	27,320
	4.42
	8,670

	Gulele-Sub City
	KEBELE 18
	3
	40,869
	29,136
	3.23
	12,653

	Gulele-Sub City
	KEBELE 19/20/21
	4
	45,737
	32,607
	7.94
	5,760

	Gulele-Sub City
	KEBELE 01/02
	5
	32,748
	23,346
	2.2
	14,885

	Gulele-Sub City
	KEBELE 03/04/05
	6
	43,999
	31,368
	1.37
	32,116

	Gulele-Sub City
	KEBELE 09/15
	7
	49,991
	35,640
	1.66
	30,115

	Gulele-Sub City
	KEBELE 07/08
	8
	57,989
	41,341
	3.13
	18,527

	Gulele-Sub City
	KEBELE 10/11/12
	9
	51,165
	36,476
	1.95
	26,238

	Arada-Sub City
	KEBELE 07/08
	10
	39,586
	31,165
	1.13
	35,032

	Arada-Sub City
	KEBELE 06
	11
	21,385
	16,836
	0.63
	33,944

	Arada-Sub City
	KEBELE 03/09
	12
	38,682
	30,453
	0.95
	40,717

	Arada-Sub City
	KEBELE 04/05
	13
	34,434
	27,109
	0.56
	61,489

	Arada-Sub City
	KEBELE 11/12
	14
	31,072
	24,462
	0.92
	33,774

	Arada-Sub City
	KEBELE 10
	15
	21,153
	16,653
	0.38
	55,666

	Arada-Sub City
	KEBELE 17
	16
	28,461
	22,406
	1
	28,461

	Arada-Sub City
	KEBELE 15/16
	17
	38,528
	30,332
	1.08
	35,674

	Arada-Sub City
	KEBELE 13/14
	18
	44,051
	34,680
	1.35
	32,630

	Arada-Sub City
	KEBELE 01/02
	19
	33,536
	26,402
	1.47
	22,814

	Yeka-Sub City
	KEBELE 01/02
	20
	42,496
	32,282
	3.92
	10,841

	Yeka-Sub City
	KEBELE 03/04
	21
	50,604
	38,442
	6.27
	8,071

	Yeka-Sub City
	KEBELE 05
	22
	21,429
	16,278
	1.02
	21,008

	Yeka-Sub City
	KEBELE 06/07
	23
	29,479
	22,394
	3.58
	8,234

	Yeka-Sub City
	KEBELE 18/19
	24
	49,835
	37,857
	21.36
	2,333

	Yeka-Sub City
	KEBELE 20/21
	25
	101,889
	77,401
	29.79
	3,420

	Yeka-Sub City
	KEBELE 15/17
	26
	86,101
	65,407
	4.9
	17,572

	Yeka-Sub City
	KEBELE 08/15
	27
	47,594
	36,155
	6.78
	7,020

	Yeka-Sub City
	KEBELE 11/12
	28
	33,311
	25,305
	1.72
	19,367

	Yeka-Sub City
	KEBELE 13/14
	29
	37,328
	28,357
	1.5
	24,886

	Yeka-Sub City
	KEBELE 09/10
	30
	42,280
	32,118
	0.98
	43,143

	Addis Ketema-Sub City
	KEBELE 19/20
	31
	30,977
	24,648
	1.23
	25,184

	Addis Ketema-Sub City
	KEBELE 14/21
	32
	44,805
	35,651
	0.62
	72,266

	Addis Ketema-Sub City
	KEBELE 16/17
	33
	44,653
	35,530
	0.77
	57,991

	Addis Ketema-Sub City
	KEBELE 10/11/12
	34
	51,089
	40,652
	1.19
	42,932

	Addis Ketema-Sub City
	KEBELE 08/09/18
	35
	51,747
	41,174
	0.98
	52,803

	Addis ketema 
	KEBELE 13/15
	36
	36,294
	28,879
	0.48
	75,613

	Addis Ketema-Sub City
	KEBELE 01/02/03
	37
	52,033
	41,402
	0.79
	65,864

	Addis Ketema-Sub City
	KEBELE 04/05
	38
	42,465
	33,789
	0.36
	117,957

	Addis Ketema-Sub City
	KEBELE 06/07
	39
	45,460
	36,173
	0.89
	51,079

	Kolfe Keraniyo-Sub City
	KEBELE 13/14
	40
	59,391
	103,069
	2.12
	28,014

	Kolfe Keraniyo-Sub City
	KEBELE 15/16
	41
	68,835
	119,460
	7.97
	8,637

	Kolfe Keraniyo-Sub City
	KEBELE 12
	42
	20,391
	35,388
	1.27
	16,056

	Kolfe Keraniyo-Sub City
	KEBELE 10/11
	43
	80,567
	139,820
	4.87
	16,544

	Kolfe Keraniyo-Sub City
	KEBELE 07
	44
	55,728
	96,713
	7.77
	7,172

	Kolfe Keraniyo-Sub City
	KEBELE 08/09
	45
	63,696
	110,541
	2.51
	25,377

	Kolfe Keraniyo-Sub City
	KEBELE 06
	46
	65,318
	113,356
	6.29
	10,384

	Kolfe Keraniyo-Sub City
	KEBELE 05
	47
	20,751
	36,012
	6.86
	3,025

	Kolfe Keraniyo-Sub City
	KEBELE 01/02
	48
	119,019
	206,550
	1.88
	63,308

	Kolfe Keraniyo-Sub City
	KEBELE 03
	49
	51,418
	89,233
	1.46
	35,218

	Kolfe Keraniyo-Sub City
	KEBELE 04
	50
	86,631
	150,343
	19.52
	4,438

	Lideta-Sub City
	KEBELE 02/03
	51
	38,450
	30,792
	2.92
	13,168

	Lideta-Sub City
	KEBELE 04/06
	52
	41,944
	33,590
	0.58
	72,316

	Lideta-Sub City
	KEBELE 05/07
	53
	44,065
	35,288
	1.03
	42,782

	Lideta-Sub City
	KEBELE 08/10
	54
	45,637
	36,548
	0.64
	71,308

	Lideta-Sub City
	KEBELE 09/11
	55
	20,909
	16,745
	0.5
	41,818

	Lideta-Sub City
	KEBELE 12
	56
	27,308
	21,869
	0.37
	73,805

	Lideta-Sub City
	KEBELE 13/14
	57
	41,282
	33,060
	1.14
	36,212

	Lideta-Sub City
	KEBELE 15/16/17
	58
	22,458
	17,985
	1.01
	22,236

	Lideta-Sub City
	KEBELE 01/18
	59
	33,522
	26,845
	2.72
	12,324

	Kirkos-Sub City
	KEBELE 17/18
	60
	33,646
	27,149
	1.69
	19,909

	Kirkos-Sub City
	KEBELE 15/16
	61
	26,803
	21,627
	1.88
	14,257

	Kirkos-Sub City
	KEBELE 01/19
	62
	28,530
	23,021
	1.43
	19,951

	Kirkos-Sub City
	KEBELE 20/21
	63
	32,162
	25,952
	1.05
	30,631

	Kirkos-Sub City
	KEBELE 02/03
	64
	39,107
	31,556
	1.91
	20,475

	Kirkos-Sub City
	KEBELE 04
	65
	20,013
	16,149
	1.35
	14,824

	Kirkos-Sub City
	KEBELE 05/06/07
	66
	44,536
	35,936
	1.6
	27,835

	Kirkos-Sub City
	KEBELE 13/14
	67
	35,504
	28,649
	0.68
	52,212

	Kirkos-Sub City
	KEBELE 11/12
	68
	35,780
	28,871
	0.71
	50,394

	Kirkos-Sub City
	KEBELE 08/09
	69
	32,752
	26,428
	1.19
	27,523

	Kirkos-Sub City
	KEBELE 10
	70
	17,283
	13,946
	1.14
	15,160

	Bole-Sub City
	KEBELE 02
	71
	12,758
	9,922
	1.15
	11,094

	Bole-Sub City
	KEBELE 04/06/07
	72
	45,415
	35,318
	1.89
	24,029

	Bole-Sub City
	KEBELE 08/09
	73
	31,646
	24,610
	1.55
	20,417

	Bole-Sub City
	KEBELE 03/05
	74
	49,683
	38,637
	5.32
	9,339

	Bole-Sub City
	KEBELE 12/13
	75
	38,112
	29,639
	3.19
	11,947

	Bole-Sub City
	KEBELE 11/14
	76
	28,850
	22,436
	5.35
	5,393

	Bole-Sub City
	KEBELE 10
	77
	50,473
	39,252
	2.92
	17,285

	Bole-Sub City
	KEBELE 15
	78
	127,356
	99,042
	11.63
	10,951

	Bole-Sub City
	KEBELE 16/18/21/22
	79
	21,169
	16,463
	47.87
	442

	Bole-Sub City
	KEBELE 01
	80
	44,123
	34,313
	8.15
	5,414

	Bole-Sub City
	KEBELE 17/19/20
	81
	33,829
	26,308
	29.53
	1,146

	Nefas Silk-
	KEBELE 12/13
	82
	43,841
	32,921
	1.2
	36,534

	Nefas Silk-Lafto-Sub 
	KEBELE 11
	83
	25,047
	18,808
	1.06
	23,629

	Nefas Silk-Lafto-Sub City
	KEBELE 10/18
	84
	64,611
	48,517
	3.65
	17,702

	Nefas Silk-Lafto-Sub City
	KEBELE 09/14
	85
	52,455
	39,389
	3.52
	14,902

	Nefas Silk-Lafto-Sub City
	KEBELE 03/04/05
	86
	54,516
	40,936
	4.3
	12,678

	Nefas Silk-Lafto-Sub City
	KEBELE 06/07/08
	87
	63,148
	47,418
	2.72
	23,216

	Nefas Silk-Lafto-Sub City
	KEBELE 02
	88
	50,414
	37,856
	6.58
	7,662

	Nefas Silk-Lafto-Sub City
	KEBELE 01(HANA,LEBU,DERTU)
	89
	49,480
	37,155
	25.68
	1,927

	Nefas Silk-Lafto-Sub City
	KEBELE 16/17
	90
	56,448
	42,387
	2.64
	21,382

	Nefas Silk-Lafto-Sub City
	KEBELE 15
	91
	34,856
	26,174
	6.59
	5,289

	Akaki Kality-Sub City
	KEBELE 12/13
	92
	42,369
	28,047
	3.62
	11,704

	Akaki Kality-Sub City
	GELANGORA
	93
	6,106
	4,042
	35.46
	172

	Akaki Kality-Sub City
	KEBELE 10/11
	94
	71,701
	47,464
	15.03
	4,771

	Akaki Kality-Sub City
	KEBELE 07/08/09
	95
	66,194
	43,818
	19.16
	3,455

	Akaki Kality-Sub
	KEBELE 05/06
	96
	27,503
	18,206
	2.49
	11,046

	Akaki Kality-Sub City
	KEBELE 01/03
	97
	39,844
	26,375
	6.11
	6,521

	Akaki Kality-Sub City
	KEBELE 02/04
	98
	21,860
	14,471
	13.47
	1,623

	Akaki Kality-Sub City
	KILINITO,FECHE KOYE(17/18/19)
	99
	8,013
	5,304
	29.09
	275
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	Woreda ID
	2007 CSA Population
	Projected population(2019)

	
	Both genders
	Male
	Female
	Both genders
	Male
	Female

	1
	23,727
	11,335
	12,392
	         37,120.27 
	   17,733.31 
	   19,386.96 

	2
	24,495
	12,208
	12,287
	         38,321.78 
	   19,099.09 
	   19,222.69 

	3
	26,123
	14,131
	11,992
	         40,868.74 
	   22,107.58 
	   18,761.17 

	4
	29,235
	14,045
	15,190
	         45,737.39 
	   21,973.03 
	   23,764.35 

	5
	20,932
	10,361
	10,571
	         32,747.56 
	   16,209.51 
	   16,538.05 

	6
	28,124
	13,247
	14,877
	         43,999.26 
	   20,724.58 
	   23,274.67 

	7
	31,954
	14,877
	17,077
	         49,991.19 
	   23,274.67 
	   26,716.52 

	8
	37,066
	17,605
	19,461
	         57,988.78 
	   27,542.56 
	   30,446.22 

	9
	32,704
	15,481
	17,223
	         51,164.54 
	   24,219.62 
	   26,944.93 

	10
	25,303
	11,524
	13,779
	         39,585.88 
	   18,028.99 
	   21,556.88 

	11
	13,669
	6,373
	7,296
	         21,384.79 
	     9,970.39 
	   11,414.40 

	12
	24,725
	11,571
	13,154
	         38,681.61 
	   18,102.52 
	   20,579.09 

	13
	22,010
	10,709
	11,301
	         34,434.06 
	   16,753.95 
	   17,680.12 

	14
	19,861
	9,238
	10,623
	         31,072.01 
	   14,452.61 
	   16,619.40 

	15
	13,521
	6,337
	7,184
	         21,153.25 
	     9,914.07 
	   11,239.18 

	16
	18,192
	8,671
	9,521
	         28,460.90 
	   13,565.55 
	   14,895.35 

	17
	24,627
	11,601
	13,026
	         38,528.29 
	   18,149.46 
	   20,378.83 

	18
	28,157
	12,852
	15,305
	         44,050.88 
	   20,106.61 
	   23,944.27 

	19
	21,436
	10,289
	11,147
	         33,536.06 
	   16,096.87 
	   17,439.19 

	20
	27,163
	12,519
	14,644
	         42,495.80 
	   19,585.65 
	   22,910.15 

	21
	32,346
	15,110
	17,236
	         50,604.46 
	   23,639.20 
	   26,965.27 

	22
	13,697
	6,025
	7,672
	         21,428.60 
	     9,425.95 
	   12,002.64 

	23
	18,843
	8,542
	10,301
	         29,479.38 
	   13,363.73 
	   16,115.64 

	24
	31,854
	14,864
	16,990
	         49,834.74 
	   23,254.34 
	   26,580.41 

	25
	65,127
	31,515
	33,612
	      101,889.47 
	   49,304.39 
	   52,585.09 

	26
	55,035
	26,241
	28,794
	         86,100.81 
	   41,053.35 
	   45,047.45 

	27
	30,422
	14,247
	16,175
	         47,594.42 
	   22,289.06 
	   25,305.36 

	28
	21,292
	9,582
	11,710
	         33,310.77 
	   14,990.79 
	   18,319.99 

	29
	23,860
	10,837
	13,023
	         37,328.34 
	   16,954.20 
	   20,374.14 

	30
	27,025
	12,110
	14,915
	         42,279.90 
	   18,945.78 
	   23,334.12 

	31
	19,800
	9,541
	10,259
	         30,976.58 
	   14,926.64 
	   16,049.93 

	32
	28,639
	14,039
	14,600
	         44,804.96 
	   21,963.65 
	   22,841.31 

	33
	28,542
	13,524
	15,018
	         44,653.21 
	   21,157.94 
	   23,495.26 

	34
	32,656
	15,742
	16,914
	         51,089.45 
	   24,627.94 
	   26,461.51 

	35
	33,076
	16,834
	16,242
	         51,746.53 
	   26,336.35 
	   25,410.18 

	36
	23,199
	11,062
	12,137
	         36,294.22 
	   17,306.21 
	   18,988.02 

	37
	33,259
	16,574
	16,685
	         52,032.83 
	   25,929.59 
	   26,103.24 

	38
	27,143
	13,047
	14,096
	         42,464.51 
	   20,411.69 
	   22,052.82 

	39
	29,058
	14,535
	14,523
	         45,460.47 
	   22,739.62 
	   22,720.85 

	40
	37,962
	18,557
	19,405
	         59,390.55 
	   29,031.94 
	   30,358.61 

	41
	43,999
	20,983
	23,016
	         68,835.27 
	   32,827.35 
	   36,007.92 

	42
	13,034
	6,497
	6,537
	         20,391.35 
	   10,164.39 
	   10,226.96 

	43
	51,498
	26,246
	25,252
	         80,567.26 
	   41,061.17 
	   39,506.09 

	44
	35,621
	17,844
	17,777
	         55,728.11 
	   27,916.47 
	   27,811.65 

	45
	40,714
	20,752
	19,962
	         63,695.98 
	   32,465.96 
	   31,230.02 

	46
	41,751
	19,000
	22,751
	         65,318.34 
	   29,725.00 
	   35,593.34 

	47
	13,264
	6,106
	7,158
	         20,751.18 
	     9,552.68 
	   11,198.50 

	48
	76,076
	35,088
	40,988
	      119,018.89 
	   54,894.25 
	   64,124.64 

	49
	32,866
	15,731
	17,135
	         51,417.99 
	   24,610.73 
	   26,807.26 

	50
	55,374
	26,943
	28,431
	         86,631.16 
	   42,151.61 
	   44,479.55 

	51
	24,577
	11,760
	12,817
	         38,450.07 
	   18,398.21 
	   20,051.86 

	52
	26,810
	13,088
	13,722
	         41,943.54 
	   20,475.83 
	   21,467.71 

	53
	28,166
	13,315
	14,851
	         44,064.96 
	   20,830.97 
	   23,234.00 

	54
	29,171
	14,283
	14,888
	         45,637.26 
	   22,345.38 
	   23,291.88 

	55
	13,365
	6,364
	7,001
	         20,909.19 
	     9,956.31 
	   10,952.88 

	56
	17,455
	8,234
	9,221
	         27,307.89 
	   12,881.88 
	   14,426.01 

	57
	26,387
	12,465
	13,922
	         41,281.77 
	   19,501.16 
	   21,780.60 

	58
	14,355
	6,794
	7,561
	         22,458.02 
	   10,629.03 
	   11,828.98 

	59
	21,427
	9,969
	11,458
	         33,521.98 
	   15,596.24 
	   17,925.74 

	60
	21,506
	9,762
	11,744
	         33,645.57 
	   15,272.39 
	   18,373.18 

	61
	17,132
	8,498
	8,634
	         26,802.56 
	   13,294.90 
	   13,507.67 

	62
	18,236
	8,495
	9,741
	         28,529.74 
	   13,290.20 
	   15,239.54 

	63
	20,558
	9,462
	11,096
	         32,162.45 
	   14,803.05 
	   17,359.40 

	64
	24,997
	11,478
	13,519
	         39,107.15 
	   17,957.03 
	   21,150.12 

	65
	12,792
	6,269
	6,523
	         20,012.75 
	     9,807.69 
	   10,205.06 

	66
	28,467
	13,065
	15,402
	         44,535.87 
	   20,439.85 
	   24,096.02 

	67
	22,694
	10,745
	11,949
	         35,504.16 
	   16,810.27 
	   18,693.90 

	68
	22,870
	10,636
	12,234
	         35,779.51 
	   16,639.74 
	   19,139.77 

	69
	20,935
	9,873
	11,062
	         32,752.26 
	   15,446.05 
	   17,306.21 

	70
	11,047
	5,217
	5,830
	         17,282.74 
	     8,161.86 
	     9,120.88 

	71
	8,155
	3,699
	4,456
	         12,758.28 
	     5,786.99 
	     6,971.29 

	72
	29,029
	13,339
	15,690
	         45,415.10 
	   20,868.51 
	   24,546.59 

	73
	20,228
	9,645
	10,583
	         31,646.17 
	   15,089.35 
	   16,556.82 

	74
	31,757
	14,849
	16,908
	         49,682.99 
	   23,230.87 
	   26,452.12 

	75
	24,361
	11,129
	13,232
	         38,112.14 
	   17,411.03 
	   20,701.11 

	76
	18,441
	7,959
	10,482
	         28,850.46 
	   12,451.65 
	   16,398.81 

	77
	32,262
	14,822
	17,440
	         50,473.05 
	   23,188.63 
	   27,284.42 

	78
	81,405
	39,025
	42,380
	      127,355.97 
	   61,053.58 
	   66,302.39 

	79
	13,531
	6,846
	6,685
	         21,168.89 
	   10,710.39 
	   10,458.51 

	80
	28,203
	13,120
	15,083
	         44,122.85 
	   20,525.89 
	   23,596.96 

	81
	21,623
	10,792
	10,831
	         33,828.61 
	   16,883.80 
	   16,944.81 

	82
	28,023
	12,806
	15,217
	         43,841.24 
	   20,034.65 
	   23,806.59 

	83
	16,010
	7,722
	8,288
	         25,047.22 
	   12,080.87 
	   12,966.36 

	84
	41,299
	19,560
	21,739
	         64,611.20 
	   30,601.10 
	   34,010.09 

	85
	33,529
	15,698
	17,831
	         52,455.24 
	   24,559.11 
	   27,896.13 

	86
	34,846
	16,089
	18,757
	         54,515.65 
	   25,170.82 
	   29,344.83 

	87
	40,364
	19,140
	21,224
	         63,148.41 
	   29,944.02 
	   33,204.39 

	88
	32,224
	15,096
	17,128
	         50,413.60 
	   23,617.29 
	   26,796.30 

	89
	31,627
	15,323
	16,304
	         49,479.61 
	   23,972.43 
	   25,507.18 

	90
	36,081
	17,447
	18,634
	         56,447.77 
	   27,295.37 
	   29,152.40 

	91
	22,280
	10,103
	12,177
	         34,856.47 
	   15,805.88 
	   19,050.60 

	92
	27,082
	13,027
	14,055
	         42,369.07 
	   20,380.40 
	   21,988.68 

	93
	3,903
	2,109
	1,794
	           6,106.14 
	     3,299.47 
	     2,806.67 

	94
	45,831
	22,931
	22,900
	         71,701.39 
	   35,874.94 
	   35,826.45 

	95
	42,311
	20,263
	22,048
	         66,194.44 
	   31,700.93 
	   34,493.51 

	96
	17,580
	8,376
	9,204
	         27,503.45 
	   13,104.03 
	   14,399.42 

	97
	25,468
	12,555
	12,913
	         39,844.01 
	   19,641.97 
	   20,202.05 

	98
	13,973
	6,838
	7,135
	         21,860.39 
	   10,697.87 
	   11,162.52 

	99
	5,122
	2,615
	2,507
	           8,013.23 
	     4,091.10 
	     3,922.14 


[bookmark: _Toc13425820]Appendix 5: Age distribution in all Woredas
	Woreda ID
	age(0 - 14)
	age(15 - 24 )
	age(25 - 54)
	age(55 - 64)
	age(65 & above)

	1
	8,377
	8,734
	16,055
	1,674
	2,277

	2
	8,648
	9,017
	16,575
	1,729
	2,351

	3
	9,223
	9,616
	17,676
	1,844
	2,507

	4
	10,321
	10,762
	19,782
	2,063
	2,805

	5
	7,390
	7,706
	14,164
	1,477
	2,009

	6
	9,929
	10,353
	19,030
	1,985
	2,699

	7
	11,281
	11,763
	21,622
	2,255
	3,066

	8
	13,086
	13,645
	25,081
	2,616
	3,557

	9
	11,546
	12,039
	22,129
	2,308
	3,138

	10
	8,420
	9,566
	17,039
	2,378
	2,182

	11
	4,549
	5,168
	9,205
	1,285
	1,179

	12
	8,228
	9,347
	16,650
	2,324
	2,132

	13
	7,324
	8,321
	14,821
	2,069
	1,898

	14
	6,609
	7,509
	13,374
	1,867
	1,712

	15
	4,499
	5,112
	9,105
	1,271
	1,166

	16
	6,054
	6,878
	12,250
	1,710
	1,568

	17
	8,195
	9,310
	16,584
	2,315
	2,123

	18
	9,370
	10,645
	18,961
	2,647
	2,428

	19
	7,133
	8,104
	14,435
	2,015
	1,848

	20
	10,213
	10,432
	17,587
	2,384
	1,879

	21
	12,162
	12,422
	20,943
	2,839
	2,238

	22
	5,150
	5,260
	8,868
	1,202
	948

	23
	7,085
	7,236
	12,200
	1,654
	1,303

	24
	11,977
	12,233
	20,624
	2,796
	2,204

	25
	24,488
	25,011
	42,167
	5,717
	4,505

	26
	20,694
	21,136
	35,633
	4,831
	3,807

	27
	11,439
	11,683
	19,697
	2,670
	2,104

	28
	8,006
	8,177
	13,786
	1,869
	1,473

	29
	8,972
	9,163
	15,449
	2,094
	1,651

	30
	10,162
	10,379
	17,498
	2,372
	1,869

	31
	6,329
	8,565
	12,652
	1,487
	1,943

	32
	9,154
	12,389
	18,300
	2,151
	2,810

	33
	9,123
	12,347
	18,238
	2,144
	2,801

	34
	10,438
	14,127
	20,867
	2,453
	3,204

	35
	10,572
	14,308
	21,136
	2,485
	3,246

	36
	7,415
	10,036
	14,824
	1,743
	2,276

	37
	10,631
	14,388
	21,253
	2,498
	3,264

	38
	8,676
	11,742
	17,345
	2,039
	2,663

	39
	9,288
	12,570
	18,568
	2,183
	2,851

	40
	17,826
	14,717
	23,201
	2,702
	1,635

	41
	20,660
	17,057
	26,890
	3,132
	1,896

	42
	6,120
	5,053
	7,966
	928
	562

	43
	24,182
	19,964
	31,473
	3,666
	2,219

	44
	16,726
	13,809
	21,770
	2,535
	1,535

	45
	19,118
	15,784
	24,882
	2,898
	1,754

	46
	19,605
	16,186
	25,516
	2,972
	1,799

	47
	6,228
	5,142
	8,106
	944
	571

	48
	35,723
	29,492
	46,494
	5,415
	3,277

	49
	15,433
	12,741
	20,086
	2,339
	1,416

	50
	26,002
	21,467
	33,842
	3,941
	2,386

	51
	7,657
	9,381
	16,022
	2,525
	2,863

	52
	8,353
	10,234
	17,478
	2,755
	3,123

	53
	8,776
	10,751
	18,362
	2,894
	3,281

	54
	9,089
	11,135
	19,017
	2,997
	3,398

	55
	4,164
	5,101
	8,713
	1,373
	1,557

	56
	5,438
	6,663
	11,379
	1,793
	2,033

	57
	8,221
	10,072
	17,202
	2,711
	3,074

	58
	4,473
	5,479
	9,358
	1,475
	1,672

	59
	6,676
	8,179
	13,969
	2,202
	2,496

	60
	6,493
	6,493
	14,437
	2,065
	2,315

	61
	5,172
	5,172
	11,501
	1,645
	1,844

	62
	5,506
	5,506
	12,242
	1,751
	1,963

	63
	6,207
	6,207
	13,801
	1,974
	2,213

	64
	7,547
	7,547
	16,781
	2,400
	2,691

	65
	3,862
	3,862
	8,587
	1,228
	1,377

	66
	8,594
	8,594
	19,110
	2,734
	3,065

	67
	6,851
	6,851
	15,235
	2,179
	2,443

	68
	6,905
	6,905
	15,353
	2,196
	2,462

	69
	6,320
	6,320
	14,054
	2,010
	2,254

	70
	3,335
	3,335
	7,416
	1,061
	1,189

	71
	2,837
	3,471
	5,211
	634
	606

	72
	10,098
	12,356
	18,549
	2,256
	2,157

	73
	7,037
	8,610
	12,926
	1,572
	1,503

	74
	11,047
	13,518
	20,293
	2,468
	2,360

	75
	8,475
	10,369
	15,567
	1,893
	1,810

	76
	6,415
	7,850
	11,784
	1,433
	1,370

	77
	11,223
	13,733
	20,615
	2,507
	2,397

	78
	28,319
	34,651
	52,017
	6,325
	6,049

	79
	4,707
	5,760
	8,646
	1,051
	1,005

	80
	9,811
	12,005
	18,022
	2,191
	2,096

	81
	7,522
	9,204
	13,817
	1,680
	1,607

	82
	10,922
	11,299
	18,612
	1,544
	1,465

	83
	6,240
	6,456
	10,633
	882
	837

	84
	16,096
	16,653
	27,429
	2,276
	2,159

	85
	13,068
	13,520
	22,269
	1,848
	1,753

	86
	13,581
	14,051
	23,144
	1,920
	1,821

	87
	15,732
	16,276
	26,808
	2,225
	2,110

	88
	12,559
	12,993
	21,402
	1,776
	1,684

	89
	12,326
	12,753
	21,006
	1,743
	1,653

	90
	14,062
	14,549
	23,964
	1,988
	1,886

	91
	8,683
	8,984
	14,798
	1,228
	1,165

	92
	11,562
	10,822
	14,186
	1,390
	1,648

	93
	1,666
	1,560
	2,044
	200
	238

	94
	19,566
	18,314
	24,006
	2,353
	2,790

	95
	18,063
	16,908
	22,163
	2,172
	2,575

	96
	7,505
	7,025
	9,208
	903
	1,070

	97
	10,873
	10,177
	13,340
	1,308
	1,550

	98
	5,965
	5,584
	7,319
	717
	851

	99
	2,187
	2,047
	2,683
	263
	312



[bookmark: _Toc13425821]Appendix 6: Expenditure distribution in all Woredas

	expenditure(1)
	expenditure(2)
	expenditure(3)
	expenditure(4)
	expenditure(5)

	253
	518
	660
	2,378
	6,406

	262
	535
	681
	2,455
	6,613

	279
	571
	726
	2,618
	7,053

	312
	639
	813
	2,929
	7,893

	224
	457
	582
	2,097
	5,651

	300
	614
	782
	2,818
	7,593

	341
	698
	888
	3,202
	8,627

	396
	810
	1,030
	3,714
	10,007

	349
	714
	909
	3,277
	8,829

	108
	550
	973
	2,143
	6,183

	58
	297
	526
	1,158
	3,340

	105
	537
	951
	2,094
	6,042

	94
	478
	846
	1,864
	5,378

	84
	431
	764
	1,682
	4,853

	57
	294
	520
	1,145
	3,304

	77
	395
	700
	1,541
	4,445

	105
	535
	947
	2,086
	6,018

	120
	612
	1,083
	2,385
	6,880

	91
	466
	824
	1,816
	5,238

	145
	218
	789
	1,932
	8,367

	173
	260
	940
	2,301
	9,963

	73
	110
	398
	974
	4,219

	101
	152
	547
	1,340
	5,804

	170
	256
	925
	2,266
	9,812

	348
	524
	1,892
	4,632
	20,061

	294
	443
	1,599
	3,914
	16,952

	162
	245
	884
	2,164
	9,371

	114
	171
	618
	1,514
	6,558

	127
	192
	693
	1,697
	7,349

	144
	217
	785
	1,922
	8,324

	95
	603
	876
	1,241
	3,689

	138
	872
	1,267
	1,796
	5,336

	138
	869
	1,263
	1,789
	5,318

	157
	994
	1,445
	2,047
	6,084

	159
	1,007
	1,464
	2,074
	6,162

	112
	706
	1,027
	1,455
	4,322

	160
	1,013
	1,472
	2,085
	6,197

	131
	827
	1,201
	1,702
	5,057

	140
	885
	1,286
	1,822
	5,414

	177
	1,663
	1,122
	2,225
	8,324

	205
	1,928
	1,300
	2,579
	9,648

	61
	571
	385
	764
	2,858

	240
	2,257
	1,522
	3,019
	11,292

	166
	1,561
	1,053
	2,088
	7,811

	190
	1,784
	1,203
	2,386
	8,928

	195
	1,829
	1,234
	2,447
	9,155

	62
	581
	392
	777
	2,908

	355
	3,334
	2,248
	4,459
	16,682

	153
	1,440
	971
	1,926
	7,207

	258
	2,426
	1,636
	3,246
	12,142

	581
	2,361
	1,592
	3,158
	11,813

	633
	2,575
	1,737
	3,445
	12,886

	665
	2,705
	1,824
	3,619
	13,538

	689
	2,802
	1,890
	3,748
	14,021

	316
	1,284
	866
	1,717
	6,424

	412
	1,677
	1,131
	2,243
	8,390

	623
	2,535
	1,709
	3,390
	12,683

	339
	1,379
	930
	1,844
	6,900

	506
	2,058
	1,388
	2,753
	10,299

	204
	340
	703
	1,725
	5,744

	163
	271
	560
	1,374
	4,576

	173
	289
	596
	1,463
	4,870

	195
	325
	672
	1,649
	5,491

	237
	396
	818
	2,005
	6,676

	121
	202
	418
	1,026
	3,416

	270
	450
	931
	2,284
	7,603

	216
	359
	742
	1,821
	6,061

	217
	362
	748
	1,835
	6,108

	199
	331
	685
	1,679
	5,591

	105
	175
	361
	886
	2,950

	53
	197
	366
	84
	1,997

	190
	702
	1,303
	300
	7,108

	133
	489
	908
	209
	4,953

	208
	768
	1,426
	328
	7,776

	160
	589
	1,094
	252
	5,965

	121
	446
	828
	191
	4,515

	211
	780
	1,448
	334
	7,900

	533
	1,969
	3,654
	842
	19,932

	89
	327
	607
	140
	3,313

	185
	682
	1,266
	292
	6,906

	142
	523
	971
	224
	5,294

	290
	459
	489
	3,068
	7,773

	165
	262
	280
	1,753
	4,441

	427
	677
	721
	4,522
	11,455

	347
	549
	585
	3,671
	9,300

	360
	571
	608
	3,816
	9,666

	417
	661
	705
	4,420
	11,196

	333
	528
	563
	3,528
	8,938

	327
	518
	552
	3,463
	8,773

	373
	591
	630
	3,951
	10,008

	230
	365
	389
	2,440
	6,180

	134
	682
	1,423
	3,414
	5,916

	19
	98
	205
	492
	853

	227
	1,155
	2,409
	5,777
	10,011

	210
	1,066
	2,224
	5,334
	9,243

	87
	443
	924
	2,216
	3,840

	126
	642
	1,339
	3,211
	5,563

	69
	352
	734
	1,761
	3,052

	25
	129
	269
	646
	1,119



[bookmark: _Toc13425822]Appendix 7: Anbessa bus capacity, frequency and coverage score
	Woreda ID
	Route length
	No. of Stops
	Total daily bus frequency  
	Total daily seats
	Capacity score
	Coverage score

	1
	2.62
	5.75
	99.5
	6965
	0.492
	1.093

	2
	2.76
	3.5
	48.5
	3395
	0.245
	0.792

	3
	0
	0
	0
	0
	0.000
	0.000

	4
	4.06
	3.5
	16
	1120
	0.099
	0.441

	5
	5.69
	8.35
	245.5
	17185
	2.986
	3.795

	6
	2.27
	6.6
	16
	1120
	0.058
	4.818

	7
	1.19
	3
	71.5
	5005
	0.119
	1.807

	8
	4.17
	6.5
	50.5
	3535
	0.254
	2.077

	9
	1.7
	3.6
	123
	8610
	0.286
	1.846

	10
	2.16
	4.6
	223.5
	15645
	0.854
	4.071

	11
	1.34
	1.8
	85.5
	5985
	0.375
	2.857

	12
	3.53
	7.1
	265.5
	18585
	1.696
	7.474

	13
	1.21
	2
	127.5
	8925
	0.314
	3.571

	14
	3.14
	4.1
	501.5
	35105
	3.548
	4.457

	15
	1.09
	1.5
	362
	25340
	1.306
	3.947

	16
	2.53
	5
	487
	34090
	3.030
	5.000

	17
	2.76
	4
	202
	14140
	1.013
	3.704

	18
	2.52
	1.8
	230
	16100
	0.921
	1.333

	19
	4.1
	9.3
	751.5
	52605
	6.431
	6.327

	20
	1.65
	4.3
	96
	6720
	0.261
	1.097

	21
	2.64
	5
	66
	4620
	0.241
	0.797

	22
	1.23
	2.05
	56
	3920
	0.225
	2.010

	23
	1.42
	1.25
	9
	630
	0.030
	0.349

	24
	1.52
	6
	260
	18200
	0.555
	0.281

	25
	14.69
	14.3
	255
	17850
	2.574
	0.480

	26
	2.89
	6
	383
	26810
	0.900
	1.224

	27
	1.66
	2
	115
	8050
	0.281
	0.295

	28
	3.3
	6
	342
	23940
	2.372
	3.488

	29
	3.65
	4
	282
	19740
	1.930
	2.667

	30
	2.01
	5
	136
	9520
	0.453
	5.102

	31
	2.04
	4.6
	164
	11480
	0.756
	3.740

	32
	1.81
	3.3
	57
	3990
	0.161
	5.323

	33
	1.02
	2.6
	135.5
	9485
	0.217
	3.377

	34
	2.99
	3.8
	236
	16520
	0.967
	3.193

	35
	2.88
	2.6
	204
	14280
	0.795
	2.653

	36
	1.69
	2.1
	238
	16660
	0.776
	4.375

	37
	2.78
	2.8
	250.5
	17535
	0.937
	3.544

	38
	0.32
	1.3
	60
	4200
	0.032
	3.611

	39
	1.52
	4
	2
	140
	0.005
	4.494

	40
	1.51
	3.5
	132
	9240
	0.235
	1.651

	41
	3.5
	10
	258
	18060
	0.918
	1.255

	42
	2.13
	4.5
	148
	10360
	1.082
	3.543

	43
	1.5
	4
	54.5
	3815
	0.071
	0.821

	44
	9.82
	8
	56.5
	3955
	0.697
	1.030

	45
	1.9
	5
	199.5
	13965
	0.417
	1.992

	46
	3.55
	4
	41
	2870
	0.156
	0.636

	47
	4.7
	7
	65.5
	4585
	1.038
	1.020

	48
	1.07
	2.55
	95
	6650
	0.060
	1.356

	49
	2.8
	1.5
	6
	420
	0.023
	1.027

	50
	3.46
	4.25
	60
	4200
	0.168
	0.218

	51
	4.66
	8.3
	235.5
	16485
	1.998
	2.842

	52
	1.12
	1.3
	65.5
	4585
	0.122
	2.241

	53
	3.4
	5.3
	203.5
	14245
	1.099
	5.146

	54
	1.3
	2
	30.5
	2135
	0.061
	3.125

	55
	1.49
	1.3
	35
	2450
	0.175
	2.600

	56
	0.66
	1.3
	41
	2870
	0.069
	3.514

	57
	5.03
	6.4
	194.5
	13615
	1.659
	5.614

	58
	1.18
	2.5
	198.5
	13895
	0.730
	2.475

	59
	2.34
	4.5
	180
	12600
	0.880
	1.654

	60
	5.05
	6.6
	194.5
	13615
	2.044
	3.905

	61
	4.1
	6.1
	298.5
	20895
	3.196
	3.245

	62
	2.69
	5.3
	97
	6790
	0.640
	3.706

	63
	1.82
	2.5
	101.5
	7105
	0.402
	2.381

	64
	3.59
	4.5
	141.5
	9905
	0.909
	2.356

	65
	2.58
	3
	92.5
	6475
	0.835
	2.222

	66
	1.76
	1.5
	74
	5180
	0.205
	0.938

	67
	0.39
	1.5
	78
	5460
	0.060
	2.206

	68
	1.23
	2
	40.5
	2835
	0.097
	2.817

	69
	1.58
	3
	123.5
	8645
	0.417
	2.521

	70
	2.72
	4.3
	96
	6720
	1.058
	3.772

	71
	2.74
	3.3
	35.5
	2485
	0.534
	2.870

	72
	3.29
	5.3
	133
	9310
	0.674
	2.804

	73
	2.26
	1.8
	71
	4970
	0.355
	1.161

	74
	7.69
	8.8
	92.5
	6475
	1.002
	1.654

	75
	3.54
	5.8
	302
	21140
	1.964
	1.818

	76
	2.89
	7.5
	39
	2730
	0.273
	1.402

	77
	1.13
	2
	8.5
	595
	0.013
	0.685

	78
	1.18
	5.1
	113
	7910
	0.073
	0.439

	79
	0.47
	7.6
	109
	7630
	0.169
	0.159

	80
	2.57
	1.8
	27
	1890
	0.110
	0.221

	81
	7.92
	2.8
	11
	770
	0.180
	0.095

	82
	1.23
	1.6
	124.5
	8715
	0.245
	1.333

	83
	1.81
	3
	130.5
	9135
	0.660
	2.830

	84
	3.84
	7.6
	121.5
	8505
	0.505
	2.082

	85
	3.04
	3
	23
	1610
	0.093
	0.852

	86
	5.13
	9.3
	162
	11340
	1.067
	2.163

	87
	1.41
	2.3
	82
	5740
	0.128
	0.846

	88
	8.86
	7.8
	131
	9170
	1.612
	1.185

	89
	5.8
	7
	101
	7070
	0.829
	0.273

	90
	0
	0
	0
	0
	0.000
	0.000

	91
	4.32
	2.5
	27
	1890
	0.234
	0.379

	92
	4.26
	6.5
	212
	14840
	1.492
	1.796

	93
	3.55
	0
	0
	0
	0.000
	0.000

	94
	4.65
	7
	159
	11130
	0.722
	0.466

	95
	3.23
	7.5
	352
	24640
	1.202
	0.391

	96
	0.86
	1.5
	16.5
	1155
	0.036
	0.602

	97
	6.1
	6.3
	102.5
	7175
	1.098
	1.031

	98
	3.08
	2.3
	104
	7280
	1.026
	0.171

	99
	3.18
	2
	24
	1680
	0.667
	0.069



[bookmark: _Toc13425823]Appendix 8: Sheger bus capacity, frequency and coverage score
	Woreda
ID
	Route Length
	No. of Stops
	Total daily bus frequency
	Total daily seat
	capacity score
	coverage score

	1
	0.62
	1.3
	66
	4620
	0.077
	0.247

	2
	0.34
	1.5
	19.5
	1365
	0.012
	0.339

	3
	0
	0
	0
	0
	0.000
	0.000

	4
	0.19
	0.5
	73
	5110
	0.021
	0.063

	5
	4.09
	9
	173
	12110
	1.512
	4.091

	6
	0.95
	2.33
	4.5
	315
	0.007
	1.701

	7
	0.42
	1.5
	39
	2730
	0.023
	0.904

	8
	0.77
	3
	39
	2730
	0.036
	0.958

	9
	1.15
	2.33
	54
	3780
	0.085
	1.195

	10
	1.97
	5.5
	132
	9240
	0.460
	4.867

	11
	0.76
	1.5
	54
	3780
	0.134
	2.381

	12
	2.42
	5
	320
	22400
	1.401
	5.263

	13
	0.33
	0.5
	4.5
	315
	0.003
	0.893

	14
	1.88
	2.16
	204.5
	14315
	0.866
	2.348

	15
	0.61
	1
	187
	13090
	0.377
	2.632

	16
	2.08
	4.5
	200
	14000
	1.023
	4.500

	17
	1.41
	2
	100
	7000
	0.256
	1.852

	18
	1.87
	1
	56
	3920
	0.166
	0.741

	19
	2.91
	7.5
	164.5
	11515
	0.999
	5.102

	20
	0.71
	1.5
	31.5
	2205
	0.037
	0.383

	21
	2.05
	3.5
	94.5
	6615
	0.268
	0.558

	22
	1.23
	2.33
	39.5
	2765
	0.159
	2.284

	23
	0.06
	0
	0
	0
	0.000
	0.000

	24
	2.31
	3.5
	227
	15890
	0.737
	0.164

	25
	12.3
	13.16
	228
	15960
	1.927
	0.442

	26
	2.68
	3.5
	282
	19740
	0.614
	0.714

	27
	1.69
	2
	112
	7840
	0.278
	0.295

	28
	1.2
	1.5
	43
	3010
	0.108
	0.872

	29
	1.91
	2.5
	82
	5740
	0.294
	1.667

	30
	0
	0
	0
	0
	0.000
	0.000

	31
	0.77
	1.66
	54
	3780
	0.094
	1.350

	32
	0.22
	0.33
	54
	3780
	0.019
	0.532

	33
	0.2
	0.33
	28.5
	1995
	0.009
	0.429

	34
	0.98
	1
	57
	3990
	0.077
	0.840

	35
	1.73
	1.66
	179
	12530
	0.419
	1.694

	36
	0.73
	1.33
	33
	2310
	0.046
	2.771

	37
	1.27
	3.33
	99.5
	6965
	0.170
	4.215

	38
	0.32
	0.83
	89.5
	6265
	0.047
	2.306

	39
	0
	0
	0
	0
	0.000
	0.000

	40
	1.5
	3
	66
	4620
	0.117
	1.415

	41
	1.41
	4.5
	198
	13860
	0.284
	0.565

	42
	1.87
	3.5
	66
	4620
	0.424
	2.756

	43
	3.3
	3.33
	28.5
	1995
	0.082
	0.684

	44
	3.8
	2.83
	54.5
	3815
	0.260
	0.364

	45
	0.67
	1
	16.5
	1155
	0.012
	0.398

	46
	3.14
	2
	56
	3920
	0.188
	0.318

	47
	4.92
	7.33
	59.5
	4165
	0.988
	1.069

	48
	1.03
	1.5
	64.5
	4515
	0.039
	0.798

	49
	2.91
	2.16
	15
	1050
	0.059
	1.479

	50
	1.24
	2.25
	18
	1260
	0.018
	0.115

	51
	2.56
	3.5
	98.5
	6895
	0.459
	1.199

	52
	0.71
	1.3
	83
	5810
	0.098
	2.241

	53
	2.64
	4.8
	122.5
	8575
	0.514
	4.660

	54
	0.38
	0.5
	10
	700
	0.006
	0.781

	55
	0.18
	0.5
	10
	700
	0.006
	1.000

	56
	0.16
	0.5
	10
	700
	0.004
	1.351

	57
	1.61
	3.5
	82.5
	5775
	0.225
	3.070

	58
	1.19
	2
	217
	15190
	0.805
	1.980

	59
	3.28
	5.5
	256
	17920
	1.753
	2.022

	60
	3.26
	3.5
	21
	1470
	0.142
	2.071

	61
	2.95
	4.8
	219
	15330
	1.687
	2.553

	62
	2.81
	3.5
	43.5
	3045
	0.300
	2.448

	63
	1.44
	2
	42.5
	2975
	0.133
	1.905

	64
	1.48
	2
	42.5
	2975
	0.113
	1.047

	65
	0.48
	0.5
	8
	560
	0.013
	0.370

	66
	1.75
	1.5
	14
	980
	0.039
	0.938

	67
	0.24
	0.5
	8
	560
	0.004
	0.735

	68
	0.1
	1
	24.5
	1715
	0.005
	1.408

	69
	1.27
	2.5
	49
	3430
	0.133
	2.101

	70
	2.67
	4.8
	203
	14210
	2.195
	4.211

	71
	1.58
	1.3
	53.5
	3745
	0.464
	1.130

	72
	1.3
	1.8
	15
	1050
	0.030
	0.952

	73
	1.32
	0.5
	63
	4410
	0.184
	0.323

	74
	2.49
	1.3
	50.5
	3535
	0.177
	0.244

	75
	5
	5.3
	204
	14280
	1.873
	1.661

	76
	3.08
	3.5
	103
	7210
	0.770
	0.654

	77
	0.4
	0
	0
	0
	0.000
	0.000

	78
	4.78
	5.1
	121
	8470
	0.318
	0.439

	79
	8.9
	6.8
	59
	4130
	1.736
	0.142

	80
	2.58
	2.3
	66.5
	4655
	0.272
	0.282

	81
	6
	0
	0
	0
	0.000
	0.000

	82
	1.2
	2
	46
	3220
	0.088
	1.667

	83
	1.66
	2
	46
	3220
	0.213
	1.887

	84
	2
	2.5
	30
	2100
	0.065
	0.685

	85
	3.17
	3
	86
	6020
	0.364
	0.852

	86
	3.69
	4.8
	227.5
	15925
	1.078
	1.116

	87
	1.29
	1.8
	151.5
	10605
	0.217
	0.662

	88
	7.86
	8.1
	381
	26670
	4.158
	1.231

	89
	2.99
	2.5
	261
	18270
	1.104
	0.097

	90
	0.82
	0.5
	12
	840
	0.012
	0.189

	91
	4.44
	2.5
	84
	5880
	0.749
	0.379

	92
	3.34
	3.3
	42
	2940
	0.232
	0.912

	93
	3.55
	0
	0
	0
	0.000
	0.000

	94
	5.82
	7
	49
	3430
	0.278
	0.466

	95
	3.18
	4.5
	43
	3010
	0.145
	0.235

	96
	0.9
	0
	0
	0
	0.000
	0.000

	97
	4.67
	3.5
	69
	4830
	0.566
	0.573

	98
	0.32
	0.5
	34.5
	2415
	0.035
	0.037

	99
	5.66
	4
	58
	4060
	2.868
	0.138



[bookmark: _Toc13425824]Appendix 9: LRT capacity, frequency and coverage score
	Woreda ID
	Route Length
	No. of Stops
	Total daily tram car frequency
	Total daily seat
	capacity score
	coverage score

	1
	0
	0
	0
	0
	0.000
	0.000

	2
	0
	0
	0
	0
	0.000
	0.000

	3
	0
	0
	0
	0
	0.000
	0.000

	4
	0
	0
	0
	0
	0.000
	0.000

	5
	0
	0
	0
	0
	0.000
	0.000

	6
	0
	0
	0
	0
	0.000
	0.000

	7
	0
	0
	0
	0
	0.000
	0.000

	8
	0
	0
	0
	0
	0.000
	0.000

	9
	0
	0
	0
	0
	0.000
	0.000

	10
	0
	0
	0
	0
	0.000
	0.000

	11
	0
	0
	0
	0
	0.000
	0.000

	12
	0
	0
	0
	0
	0.000
	0.000

	13
	0.32
	0.5
	32
	18304
	0.170
	0.893

	14
	0
	0
	0
	0
	0.000
	0.000

	15
	0.1
	0.5
	32
	18304
	0.087
	1.316

	16
	0
	0
	0
	0
	0.000
	0.000

	17
	0
	0
	0
	0
	0.000
	0.000

	18
	0
	0
	0
	0
	0.000
	0.000

	19
	0.5
	0.5
	32
	18304
	0.273
	0.340

	20
	0
	0
	0
	0
	0.000
	0.000

	21
	0
	0
	0
	0
	0.000
	0.000

	22
	0
	0
	0
	0
	0.000
	0.000

	23
	0
	0
	0
	0
	0.000
	0.000

	24
	0.72
	1
	32
	18304
	0.264
	0.047

	25
	1.71
	1.5
	32
	18304
	0.307
	0.050

	26
	0.59
	0.5
	32
	18304
	0.125
	0.102

	27
	0.07
	0.3
	32
	18304
	0.027
	0.044

	28
	0.47
	0.5
	32
	18304
	0.258
	0.291

	29
	0.92
	1.3
	32
	18304
	0.451
	0.867

	30
	0
	0
	0
	0
	0.000
	0.000

	31
	0
	0
	0
	0
	0.000
	0.000

	32
	0
	0
	0
	0
	0.000
	0.000

	33
	0
	0
	0
	0
	0.000
	0.000

	34
	0
	0
	0
	0
	0.000
	0.000

	35
	1.1
	1.3
	32
	18304
	0.389
	1.327

	36
	0.51
	1
	32
	18304
	0.257
	2.083

	37
	0.32
	0.3
	32
	18304
	0.113
	0.380

	38
	0.32
	0.3
	32
	18304
	0.138
	0.833

	39
	0
	0
	0
	0
	0.000
	0.000

	40
	0
	0
	0
	0
	0.000
	0.000

	41
	0
	0
	0
	0
	0.000
	0.000

	42
	0
	0
	0
	0
	0.000
	0.000

	43
	0
	0
	0
	0
	0.000
	0.000

	44
	0
	0
	0
	0
	0.000
	0.000

	45
	0
	0
	0
	0
	0.000
	0.000

	46
	0
	0
	0
	0
	0.000
	0.000

	47
	0
	0
	0
	0
	0.000
	0.000

	48
	0
	0
	0
	0
	0.000
	0.000

	49
	0
	0
	0
	0
	0.000
	0.000

	50
	0
	0
	0
	0
	0.000
	0.000

	51
	0.07
	0.5
	32
	18304
	0.033
	0.171

	52
	0.26
	0.8
	32
	18304
	0.113
	1.379

	53
	1.74
	2.1
	223.5
	127842
	5.048
	2.039

	54
	0.04
	0
	0
	0
	0.000
	0.000

	55
	0
	0
	0
	0
	0.000
	0.000

	56
	0
	0
	0
	0
	0.000
	0.000

	57
	0.29
	0.5
	127.5
	72930
	0.512
	0.439

	58
	0.47
	0.8
	127.5
	72930
	1.526
	0.792

	59
	1.04
	1.1
	159.5
	91234
	2.830
	0.404

	60
	0.68
	0.8
	32
	18304
	0.370
	0.473

	61
	1.18
	2.5
	255
	145860
	6.422
	1.330

	62
	0.69
	1.3
	32
	18304
	0.443
	0.909

	63
	1.01
	1.3
	127.5
	72930
	2.290
	1.238

	64
	0.64
	1.1
	32
	18304
	0.300
	0.576

	65
	0.49
	0.3
	32
	18304
	0.448
	0.222

	66
	1.24
	1.1
	32
	18304
	0.510
	0.688

	67
	0.24
	0.5
	32
	18304
	0.124
	0.735

	68
	0
	0
	0
	0
	0.000
	0.000

	69
	0
	0
	0
	0
	0.000
	0.000

	70
	0.55
	0.5
	127.5
	72930
	2.321
	0.439

	71
	0
	0
	0
	0
	0.000
	0.000

	72
	1.28
	1.6
	32
	18304
	0.516
	0.847

	73
	0.25
	0
	0
	0
	0.000
	0.000

	74
	0
	0
	0
	0
	0.000
	0.000

	75
	1.92
	1.8
	32
	18304
	0.922
	0.564

	76
	0.64
	1
	32
	18304
	0.406
	0.187

	77
	0
	0
	0
	0
	0.000
	0.000

	78
	1.18
	1.5
	32
	18304
	0.170
	0.129

	79
	0
	0
	0
	0
	0.000
	0.000

	80
	0
	0
	0
	0
	0.000
	0.000

	81
	0
	0
	0
	0
	0.000
	0.000

	82
	0
	0
	0
	0
	0.000
	0.000

	83
	0.77
	0.5
	32
	18304
	0.563
	0.472

	84
	1.58
	1.5
	32
	18304
	0.448
	0.411

	85
	0
	0
	0
	0
	0.000
	0.000

	86
	0
	0
	0
	0
	0.000
	0.000

	87
	0
	0
	0
	0
	0.000
	0.000

	88
	0
	0
	0
	0
	0.000
	0.000

	89
	0
	0
	0
	0
	0.000
	0.000

	90
	0
	0
	0
	0
	0.000
	0.000

	91
	0
	0
	0
	0
	0.000
	0.000

	92
	2.35
	3
	32
	18304
	1.015
	0.829

	93
	0
	0
	0
	0
	0.000
	0.000

	94
	0
	0
	0
	0
	0.000
	0.000

	95
	0
	0
	0
	0
	0.000
	0.000

	96
	0
	0
	0
	0
	0.000
	0.000

	97
	0
	0
	0
	0
	0.000
	0.000

	98
	0
	0
	0
	0
	0.000
	0.000

	99
	0
	0
	0
	0
	0.000
	0.000



[bookmark: _Toc13425825]Appendix 10: Total capacity, frequency and coverage score
	Woreda ID
	Total capacity score
	Total frequency score 
	Total coverage score

	1
	0.5688
	165.500
	1.340

	2
	0.2566
	68.000
	1.131

	3
	0.0000
	0.000
	0.000

	4
	0.1206
	89.000
	0.504

	5
	4.4984
	418.500
	7.886

	6
	0.0646
	20.500
	6.518

	7
	0.1421
	110.500
	2.711

	8
	0.2905
	89.500
	3.035

	9
	0.3710
	177.000
	3.041

	10
	1.3135
	355.500
	8.938

	11
	0.5094
	139.500
	5.238

	12
	3.0974
	585.500
	12.737

	13
	0.4867
	164.000
	5.357

	14
	4.4137
	706.000
	6.804

	15
	1.7697
	581.000
	7.895

	16
	4.0536
	687.000
	9.500

	17
	1.2691
	302.000
	5.556

	18
	1.0874
	286.000
	2.074

	19
	7.7034
	948.000
	11.769

	20
	0.2978
	127.500
	1.480

	21
	0.5090
	160.500
	1.356

	22
	0.3837
	95.500
	4.294

	23
	0.0303
	9.000
	0.349

	24
	1.5561
	519.000
	0.492

	25
	4.8074
	515.000
	0.972

	26
	1.6397
	697.000
	2.041

	27
	0.5861
	259.000
	0.634

	28
	2.7384
	417.000
	4.651

	29
	2.6750
	396.000
	5.200

	30
	0.4526
	136.000
	5.102

	31
	0.8500
	218.000
	5.089

	32
	0.1797
	111.000
	5.855

	33
	0.2256
	164.000
	3.805

	34
	1.0434
	293.000
	4.034

	35
	1.6028
	415.000
	5.673

	36
	1.0794
	303.000
	9.229

	37
	1.2194
	382.000
	8.139

	38
	0.2168
	181.500
	6.750

	39
	0.0047
	2.000
	4.494

	40
	0.3516
	198.000
	3.066

	41
	1.2022
	456.000
	1.819

	42
	1.5058
	214.000
	6.299

	43
	0.1527
	83.000
	1.505

	44
	0.9571
	111.000
	1.394

	45
	0.4287
	216.000
	2.390

	46
	0.3444
	97.000
	0.954

	47
	2.0260
	125.000
	2.089

	48
	0.0989
	159.500
	2.154

	49
	0.0823
	21.000
	2.507

	50
	0.1858
	78.000
	0.333

	51
	2.4903
	366.000
	4.212

	52
	0.3342
	180.500
	5.862

	53
	6.6610
	549.500
	11.845

	54
	0.0666
	40.500
	3.906

	55
	0.1806
	45.000
	3.600

	56
	0.0735
	51.000
	4.865

	57
	2.3965
	404.500
	9.123

	58
	3.0612
	543.000
	5.248

	59
	5.4634
	595.500
	4.081

	60
	2.5559
	247.500
	6.450

	61
	11.3052
	772.500
	7.128

	62
	1.3828
	172.500
	7.063

	63
	2.8255
	271.500
	5.524

	64
	1.3214
	216.000
	3.979

	65
	1.2963
	132.500
	2.815

	66
	0.7528
	120.000
	2.563

	67
	0.1875
	118.000
	3.676

	68
	0.1023
	65.000
	4.225

	69
	0.5500
	172.500
	4.622

	70
	5.5738
	426.500
	8.421

	71
	0.9975
	89.000
	4.000

	72
	1.2204
	180.000
	4.603

	73
	0.5389
	134.000
	1.484

	74
	1.1794
	143.000
	1.898

	75
	4.7591
	538.000
	4.044

	76
	1.4492
	174.000
	2.243

	77
	0.0133
	8.500
	0.685

	78
	0.5608
	266.000
	1.006

	79
	1.9058
	168.000
	0.301

	80
	0.3823
	93.500
	0.503

	81
	0.1803
	11.000
	0.095

	82
	0.3326
	170.500
	3.000

	83
	1.4362
	208.500
	5.189

	84
	1.0181
	183.500
	3.178

	85
	0.4571
	109.000
	1.705

	86
	2.1450
	389.500
	3.279

	87
	0.3448
	233.500
	1.507

	88
	5.7697
	512.000
	2.416

	89
	1.9328
	362.000
	0.370

	90
	0.0122
	12.000
	0.189

	91
	0.9832
	111.000
	0.759

	92
	2.7391
	286.000
	3.536

	93
	0.0000
	0.000
	0.000

	94
	1.0002
	208.000
	0.931

	95
	1.3469
	395.000
	0.626

	96
	0.0361
	16.500
	0.602

	97
	1.6646
	171.500
	1.604

	98
	1.0611
	138.500
	0.208

	99
	3.5344
	82.000
	0.206



[bookmark: _Toc13425826]Appendix 11: Standardized capacity, frequency, coverage and overall index
	Woreda ID
	Standardized capacity score 
	Standardized frequency score 
	Standardized coverage score 
	Woreda Index
	 woreda index plus five

	1
	-0.4949
	-0.3861
	-0.4987
	-1.3797
	3.6203

	2
	-0.6598
	-0.8797
	-0.5430
	-2.0825
	2.9175

	3
	-0.7954
	-1.2239
	-0.7828
	-2.8021
	2.1979

	4
	-0.7316
	-0.7734
	-0.6760
	-2.1810
	2.8190

	5
	1.5814
	0.8945
	0.8891
	3.3650
	8.3650

	6
	-0.7612
	-1.1201
	0.5991
	-1.2823
	3.7177

	7
	-0.7203
	-0.6645
	-0.2081
	-1.5930
	3.4070

	8
	-0.6419
	-0.7708
	-0.1394
	-1.5521
	3.4479

	9
	-0.5993
	-0.3279
	-0.1381
	-1.0654
	3.9346

	10
	-0.1014
	0.5756
	1.1121
	1.5863
	6.5863

	11
	-0.5262
	-0.5177
	0.3277
	-0.7163
	4.2837

	12
	0.8411
	1.7398
	1.9175
	4.4984
	9.4984

	13
	-0.5382
	-0.3937
	0.3529
	-0.5790
	4.4210

	14
	1.5366
	2.3498
	0.6597
	4.5461
	9.5461

	15
	0.1397
	1.7171
	0.8909
	2.7476
	7.7476

	16
	1.3463
	2.2536
	1.2312
	4.8312
	9.8312

	17
	-0.1248
	0.3048
	0.3950
	0.5749
	5.5749

	18
	-0.2208
	0.2238
	-0.3431
	-0.3401
	4.6599

	19
	3.2747
	3.5748
	1.7122
	8.5617
	13.5617

	20
	-0.6381
	-0.5785
	-0.4692
	-1.6857
	3.3143

	21
	-0.5264
	-0.4114
	-0.4954
	-1.4333
	3.5667

	22
	-0.5926
	-0.7405
	0.1275
	-1.2056
	3.7944

	23
	-0.7793
	-1.1783
	-0.7088
	-2.6665
	2.3335

	24
	0.0268
	1.4032
	-0.6786
	0.7514
	5.7514

	25
	1.7446
	1.3830
	-0.5767
	2.5508
	7.5508

	26
	0.0710
	2.3042
	-0.3502
	2.0250
	7.0250

	27
	-0.4857
	0.0872
	-0.6484
	-1.0470
	3.9530

	28
	0.6514
	0.8869
	0.2032
	1.7416
	6.7416

	29
	0.6180
	0.7806
	0.3196
	1.7182
	6.7182

	30
	-0.5563
	-0.5355
	0.2988
	-0.7929
	4.2071

	31
	-0.3463
	-0.1204
	0.2962
	-0.1705
	4.8295

	32
	-0.7004
	-0.6620
	0.4584
	-0.9040
	4.0960

	33
	-0.6762
	-0.3937
	0.0239
	-1.0460
	3.9540

	34
	-0.2441
	0.2593
	0.0723
	0.0875
	5.0875

	35
	0.0514
	0.8768
	0.4200
	1.3482
	6.3482

	36
	-0.2251
	0.3099
	1.1738
	1.2586
	6.2586

	37
	-0.1511
	0.7098
	0.9427
	1.5014
	6.5014

	38
	-0.6808
	-0.3051
	0.6482
	-0.3378
	4.6622

	39
	-0.7929
	-1.2137
	0.1700
	-1.8366
	3.1634

	40
	-0.6096
	-0.2216
	-0.1328
	-0.9640
	4.0360

	41
	-0.1602
	1.0843
	-0.3971
	0.5270
	5.5270

	42
	0.0002
	-0.1406
	0.5526
	0.4122
	5.4122

	43
	-0.7147
	-0.8037
	-0.4637
	-1.9822
	3.0178

	44
	-0.2897
	-0.6620
	-0.4873
	-1.4391
	3.5609

	45
	-0.5689
	-0.1305
	-0.2761
	-0.9754
	4.0246

	46
	-0.6134
	-0.7329
	-0.5806
	-1.9269
	3.0731

	47
	0.2750
	-0.5911
	-0.3400
	-0.6561
	4.3439

	48
	-0.7431
	-0.4165
	-0.3261
	-1.4858
	3.5142

	49
	-0.7519
	-1.1176
	-0.2514
	-2.1208
	2.8792

	50
	-0.6972
	-0.8290
	-0.7122
	-2.2385
	2.7615

	51
	0.5204
	0.6288
	0.1102
	1.2593
	6.2593

	52
	-0.6188
	-0.3102
	0.4600
	-0.4690
	4.5310

	53
	2.7239
	1.5576
	1.7283
	6.0099
	11.0099

	54
	-0.7602
	-1.0189
	0.0453
	-1.7337
	3.2663

	55
	-0.6999
	-0.9961
	-0.0196
	-1.7156
	3.2844

	56
	-0.7566
	-0.9657
	0.2485
	-1.4737
	3.5263

	57
	0.4708
	0.8237
	1.1513
	2.4457
	7.4457

	58
	0.8220
	1.5247
	0.3297
	2.6764
	7.6764

	59
	2.0912
	1.7905
	0.0823
	3.9640
	8.9640

	60
	0.5550
	0.0289
	0.5845
	1.1685
	6.1685

	61
	5.1777
	2.6864
	0.7283
	8.5924
	13.5924

	62
	-0.0648
	-0.3507
	0.7146
	0.2991
	5.2991

	63
	0.6975
	0.1504
	0.3882
	1.2361
	6.2361

	64
	-0.0972
	-0.1305
	0.0607
	-0.1670
	4.8330

	65
	-0.1105
	-0.5532
	-0.1861
	-0.8497
	4.1503

	66
	-0.3976
	-0.6164
	-0.2396
	-1.2536
	3.7464

	67
	-0.6963
	-0.6266
	-0.0034
	-1.3263
	3.6737

	68
	-0.7413
	-0.8948
	0.1130
	-1.5232
	3.4768

	69
	-0.5048
	-0.3507
	0.1970
	-0.6584
	4.3416

	70
	2.1495
	0.9350
	1.0025
	4.0870
	9.0870

	71
	-0.2684
	-0.7734
	0.0652
	-0.9765
	4.0235

	72
	-0.1506
	-0.3127
	0.1931
	-0.2703
	4.7297

	73
	-0.5107
	-0.5456
	-0.4683
	-1.5245
	3.4755

	74
	-0.1723
	-0.5000
	-0.3803
	-1.0526
	3.9474

	75
	1.7191
	1.4994
	0.0745
	3.2930
	8.2930

	76
	-0.0297
	-0.3431
	-0.3073
	-0.6801
	4.3199

	77
	-0.7883
	-1.1808
	-0.6376
	-2.6068
	2.3932

	78
	-0.4991
	0.1226
	-0.5696
	-0.9461
	4.0539

	79
	0.2115
	-0.3735
	-0.7191
	-0.8810
	4.1190

	80
	-0.5934
	-0.7506
	-0.6762
	-2.0202
	2.9798

	81
	-0.7001
	-1.1682
	-0.7627
	-2.6311
	2.3689

	82
	-0.6196
	-0.3608
	-0.1468
	-1.1273
	3.8727

	83
	-0.0365
	-0.1685
	0.3172
	0.1122
	5.1122

	84
	-0.2575
	-0.2950
	-0.1091
	-0.6616
	4.3384

	85
	-0.5539
	-0.6721
	-0.4215
	-1.6475
	3.3525

	86
	0.3379
	0.7477
	-0.0877
	0.9980
	5.9980

	87
	-0.6132
	-0.0419
	-0.4633
	-1.1184
	3.8816

	88
	2.2530
	1.3678
	-0.2705
	3.3503
	8.3503

	89
	0.2258
	0.6085
	-0.7044
	0.1299
	5.1299

	90
	-0.7889
	-1.1631
	-0.7427
	-2.6947
	2.3053

	91
	-0.2759
	-0.6620
	-0.6220
	-1.5599
	3.4401

	92
	0.6518
	0.2238
	-0.0332
	0.8424
	5.8424

	93
	-0.7954
	-1.2239
	-0.7828
	-2.8021
	2.1979

	94
	-0.2669
	-0.1710
	-0.5854
	-1.0233
	3.9767

	95
	-0.0837
	0.7756
	-0.6501
	0.0418
	5.0418

	96
	-0.7763
	-1.1403
	-0.6551
	-2.5718
	2.4282

	97
	0.0841
	-0.3558
	-0.4428
	-0.7145
	4.2855

	98
	-0.2348
	-0.5228
	-0.7388
	-1.4963
	3.5037

	99
	1.0720
	-0.8088
	-0.7391
	-0.4759
	4.5241



LRT frequency score distribution
woreda	0 - 95	96 - 191	192 - 286	287 - 381	71	13	13	2	LRT frequency
No. of Woredas
No. of Woredas	65 - 128 (High frequency)	192 - 255 (Moderate frequency)	129 - 191 (Low frequency)	0 - 64 (Almost no frequency)	2	1	4	92	Frequency score
No. of Woredas
No. of Woredas	0.000 - 1.605 (Almost no capacity	1.606 - 3.211 (Low capacity)	3.212 - 4.816 (Moderate capacity)	4.817 - 6.422 (High capacity)	94	3	0	2	LRT capacity score
No. of Woredas

No. of Woredas	0.000 - 0.521 (Almost no coverage)	0.522 - 1.042 (Low coverage)	1.043 - 1.562 (Moderate coverage)	1.563 - 2.083 (High coverage)	81	11	5	2	LRT coverage score
No. of  Woredas

No. Woredas	0 - 237 (Almost no frequency)	238 - 474 (Low frequency)	475 - 711 (Moderate frequency)	712 - 948 (High frequency)	63	22	12	2	frequency score
No. of Woredas

Public transit total capacity score distribution across the city Woredas
No.of woredas	0.0000 - 2.8263 (Almost no capacity)	2.8254 - 5.6526 (Low capacity)	5.6527 - 8.4789 (Moderate capacity)	8.4790 -11.3052 (High capacity)	85	10	3	1	capacity score
No. of Woredas

No.of woredas	0.000 - 3.184 (Almost no coverage)	3.185 - 6.369 (Low coverage)	6.370 - 9.553 (Moderate coverage)	9.544 - 12.737 (High coverage)	50	32	14	3	Total coverage score
No. of Woredas

No. of Woredas	10.7439 - 13.5924 (High transit availability)	7.8952 - 10.7438 (Moderate transit availability)	5.0466 - 7.8951 (Low transit availability)	2.1979 - 5.0465 (Almost no transit availability)	3	8	24	64	Transit availability indicies
Number of Woredas

overall transit availabity score
No. of Woredas	2.1979 - 5.0465 (Almost no transit availability)	5.0466 - 7.8951 (Low transit availability)	7.8952 - 10.7438 (Moderate transit availability)	10.7439 - 13.5924 (High transit availability)	64	24	8	3	Transit availability index
Number of Woredas
overall transit availability score
No. of Woredas	2.1979 - 5.0465 (Almost no transit availability)	5.0466 - 7.8951 (Low transit availability)	7.8952 - 10.7438 (Moderate transit availability)	10.7439 - 13.5924 (High transit availability)	3	8	24	64	Transit availability indicies
Number of Woredas
No. of Woredas	10.7439 - 13.5924 (High transit availability)	7.8952 - 10.7438 (Moderate transit availability)	5.0466 - 7.8951 (Low transit availability)	2.1979 - 5.0465 (Almost no transit availability)	3	8	24	64	Transit availability indicies
Number of Woredas

woreda	172 - 14256	12257 - 30630	30631 - 55666	55667 - 11 7957	38	31	18	12	Population density
Number of Woredas
index	2.3052999999999999	2.3689	2.7614999999999998	3.3142999999999998	3.3525	3.4479000000000002	3.5036999999999998	3.9767000000000001	4.1189999999999998	4.5240999999999998	5.0418000000000003	5.1299000000000001	5.5270000000000001	7.5507999999999997	8.3503000000000007	2.3052999999999999	2.3689	2.7614999999999998	3.3142999999999998	3.3525	3.4479000000000002	3.5036999999999998	3.9767000000000001	4.1189999999999998	4.5240999999999998	5.0418000000000003	5.1299000000000001	5.5270000000000001	7.5507999999999997	8.3503000000000007	density	2.3052999999999999	2.3689	2.7614999999999998	3.3142999999999998	3.3525	3.4479000000000002	3.5036999999999998	3.9767000000000001	4.1189999999999998	4.5240999999999998	5.0418000000000003	5.1299000000000001	5.5270000000000001	7.5507999999999997	8.3503000000000007	21382	1146	4438	10841	14902	18527	1623	4771	442	276	3455	1927	8637	3420	7662	Periphery Woredas public transit index
woredas population density
woreda	2.1979 - 5.0465 (almost no service)	5.0465 - 7.8951 (low service intensity)	7.8952 - 10.7438 (medium service intensity)	10.7439 - 13.5924 (high service intensity)	11	3	1	0	index	2.1979 - 5.0465 (almost no service)	5.0465 - 7.8951 (low service intensity)	7.8952 - 10.7438 (medium service intensity)	10.7439 - 13.5924 (high service intensity)	0	0	0	0	Public transit index
Woredas with condominium sites
Gender and transit availability relation
gender(female)	2.3052999999999999	2.3689	3.3142999999999998	3.3525	3.4479000000000002	3.5036999999999998	3.9767000000000001	5.0418000000000003	5.1299000000000001	5.5270000000000001	7.5507999999999997	29152	16945	22910	27896	30446	11163	35827	34494	25507	36008	52585	Public transit vailability index
Gender (female)
Age (0 -14) and public transit availability relation
age 0 -14	3.4479000000000002	3.3142999999999998	7.5507999999999997	5.5270000000000001	2.3689	3.3525	5.1299000000000001	2.3052999999999999	3.9767000000000001	5.0418000000000003	3.5036999999999998	13086.164550626163	10213.465012975139	24488.176412768538	20660.35415898075	7522.1192101358483	13067.694763107735	12326.403479758063	14062.319029726212	19565.727430058778	18063.003061098745	5965.2180703063686	Public transit availability index
Age (0 - 14) population
Age (15 - 24)  and public transit availability index relation
age 15 - 24	3.4479000000000002	3.3142999999999998	7.5507999999999997	5.5270000000000001	2.3689	3.3525	5.1299000000000001	2.3052999999999999	3.9767000000000001	5.0418000000000003	3.5036999999999998	13644.864299931311	10431.684702277129	25011.387902853236	17057.016918944279	9203.9803076724565	13519.613597325	12752.686308646174	14548.634859527076	18314.457367626801	16907.835431949057	5583.7296327343756	Public transit availability index
Age (15 - 24) population
Age (25 - 54) and Public transit availability index relation
age(25 - 54)	3.4479000000000002	3.3142999999999998	7.5507999999999997	5.5270000000000001	2.3689	3.3525	5.1299000000000001	2.3052999999999999	3.9767000000000001	5.0418000000000003	25080.722470567704	17587.096561184742	42167.464482578449	26890.04471089158	13816.957071823788	22268.79615083649	21005.553874631074	23963.745829530591	24006.484628796956	22162.692743536631	Public transit availability index
Age(25 - 54)
Age (55 - 64) and public transit availability relation
age(55 - 64)	3.4479000000000002	3.3142999999999998	7.5507999999999997	5.5270000000000001	4.1189999999999998	2.3689	3.3525	5.1299000000000001	2.3052999999999999	3.9767000000000001	5.0418000000000003	2615.8631193992369	2384.2753772963183	5716.6256487566652	3131.7618850191311	1051.3615392981251	1680.1116372953484	1847.8529672158525	1743.02978896286	1988.4989981841143	2353.1158761475854	2172.3873761358127	Public transit availability
Age (55 -64)
Age 65 & above
65 	&	 above	3.3142999999999998	7.5507999999999997	5.5270000000000001	2.7614999999999998	2.3689	3.3525	2.3052999999999999	3.9767000000000001	5.0418000000000003	1879.0399889231655	4505.2548451422517	1895.5558003218555	2385.6111931412624	1606.6343071624765	1752.6563654970848	1886.0566770109551	2789.7583085218071	2575.493962424257	Public transit availability
age 65 and above
labor force and public transit availability relation
labor force	3.4479000000000002	3.3142999999999998	7.5507999999999997	4.1189999999999998	2.3689	3.3525	5.1299000000000001	3.9767000000000001	5.0418000000000003	3.5036999999999998	26463.83698099649	32282.096629681357	77400.732879330608	16462.528930140241	26307.683323954068	39388.919080874424	37154.503378293855	47463.563348185002	43818.176099693534	14470.737506582633	public transit availability index
Labor force
very low expenditure and public transit availability
expenditure(1)	3.3142999999999998	7.5507999999999997	5.5270000000000001	2.7614999999999998	4.1189999999999998	2.3689	8.3503000000000007	3.9767000000000001	5.0418000000000003	3.5036999999999998	145.03577913751636	347.74307653385216	205.28802646144092	258.3608531392947	88.675376612049774	141.70627954196678	333.05723893124878	227.04395151826924	209.606088295902	69.221381479015818	Public transit availability index
Very low expenditure
Very high expenditure and public transit availability 
expenditure(5)	3.4479000000000002	3.3142999999999998	7.5507999999999997	2.7614999999999998	2.3689	3.3525	5.1299000000000001	2.3052999999999999	3.9767000000000001	5.0418000000000003	10006.90414307086	8366.7857894673125	20060.510919656797	12142.208684498459	5294.4964957361299	9300.2203438613233	8772.6466287483036	10008.090018397817	10011.424663996557	9242.5081049586097	Public transit availabilit index
Very high expenditure
Total Anbessa bus seat in the provided route 
no.of route	0 - 1500	1501 -3000	3001 - 4500	4501 - 6000	87	29	6	2	bus seat	0 - 1500	1501 -3000	3001 - 4500	4501 - 6000	0	0	0	0	Total bus seat
Number of routes
Number of buses assigned in the provided route 
number of bus assigned 	0 - 2	3 - 5	6 - 8	29	83	12	Number of buses assigned
Number of routes
Number of  Anbessa buses assigned in the provided route 
number of bus assigned 	0 - 5	6 - 10	112	12	number of buses assigned
Number of routes
Total Anbessa bus seat in the provided route 
no.of route	0 - 4000	4001 - 8000	120	4	bus seat	0 - 4000	4001 - 8000	0	0	bus seat
Number of routes
Total Sheger bus seat in the provided route
no. of routes	0 - 4000	4001 - 8000	8001 - 12000	12001 - 16000	47	2	1	1	total bus seat	0 - 4000	4001 - 8000	8001 - 12000	12001 - 16000	0	0	0	0	total  bus seat
Number of routes
Number of Sheger buses assigned in the provided routes
no. of routes	0 - 5	6 - 10	11 - 15	16 - 20	21 - 25	26 -30	39	7	3	0	1	1	No.of bus assigned	0 - 5	6 - 10	11 - 15	16 - 20	21 - 25	26 -30	0	0	0	0	number of bus assigned
Number of routes
Number of Sheger buses assigned in the provided routes
no. of routes	0 - 5	6 - 10	11 - 15	16 - 20	39	7	3	0	No.of bus assigned	0 - 5	6 - 10	11 - 15	16 - 20	0	0	0	0	number of bus assigned
Number of routes
Number of buses Sheger assigned in the provided routes
no. of routes	1 - 8	9 - 16	17 - 24	25 - 32	46	3	1	1	No.of bus assigned	1 - 8	9 - 16	17 - 24	25 - 32	0	0	0	0	number of bus assigned
Number of routes
Number of LRT trams assigned in each route
Number of LRT 	R1(E-W)	R2(N-S)	9	8	route	R1(E-W)	R2(N-S)	0	0	LRT routes
Number of LRT trams
Total LRT trams seats in each route
total seat	R1(E-W)	R2(N-W)	36608	36036	route	R1(E-W)	R2(N-W)	0	0	LRT route
Number of seats
Anbessa bus route length within Woredas
No.of woredas	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	78	16	4	1	Anbessa rout length	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	0	0	0	0	Route length
Number of Woredas
Number of bus stops coverage in Woredas
No.of woredas	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	47	41	10	1	A.stops	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	0	0	0	0	Number of stops
Number of Woredas
Total Sheger bus rout length within Woredas
woreda	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	86	10	2	1	rout length	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	0	0	0	0	Route length
Number of Woredas
Total Sheger bus stops within Woredas
woredas	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	79	17	2	1	stops	0 - 3.75	3.76 - 7.50	7.51 - 11.25	11.26 - 15	0	0	0	0	Bus stops
Number of Woredas
LRT total route length within Woredas
woreda	0 - 0.75	0.76 - 1.50	1.51 - 2.25	2.26 -3.00	85	9	4	1	L.route length	0 - 0.75	0.76 - 1.50	1.51 - 2.25	2.26 -3.00	0	0	0	0	Route length
Number of Woredas
LRT total stops within Woredas
woreda	0 - 0.75	0.76 - 1.50	1.51 - 2.25	2.26 -3.00	78	16	3	2	stops	0 - 0.75	0.76 - 1.50	1.51 - 2.25	2.26 -3.00	0	0	0	0	Number of stops
Number of Woredas
Gender (female) distribution in Woredas
woredas	2807 - 18681	18682 - 34555	34556 - 50428	504229 - 66302	33	56	6	4	female	2807 - 18681	18682 - 34555	34556 - 50428	504229 - 66302	0	0	0	0	Gender (female) distribution
Number of Woredas
Woreda_ID	1	2	3	4	5	6	7	8	9	10	11	12	13	14	15	16	17	18	19	20	21	22	23	24	25	26	27	28	29	30	31	32	33	34	35	36	37	38	39	40	41	42	43	44	45	46	47	48	49	50	51	52	53	54	55	56	57	58	59	60	61	62	63	64	65	66	67	68	69	70	71	72	73	74	75	76	77	78	79	80	81	82	83	84	85	86	87	88	89	90	91	92	93	94	95	96	97	98	99	age(0 - 14)	8376.8258321023841	8647.9685066526727	9222.7344886420778	10321.427201142715	7390.0500829252387	9929.1882539742692	11281.371123150824	13086.164550626163	11546.158891266337	8420.2893300007181	4548.7465854554712	8227.9434724842013	7324.4503874368966	6609.309820303688	4499.4953970256374	6053.9028372672428	8195.3311990644452	9370.0385987760401	7133.4356431211854	10213.465012975139	12162.306789003196	5150.161259165794	7085.0907940761517	11977.311582789458	24488.176412768538	20693.518646286739	11438.870250882803	8005.9307534612026	8971.5154883329069	10161.576113671284	6328.704828109273	9153.9281602132069	9122.9238991866096	10437.888124582649	10572.133378512237	7415.1324902680299	10630.625953438705	8675.7593509782837	9287.853782585822	17825.5952313286	20660.35415898075	6120.2994638095206	24181.615911252313	16726.345496421585	19117.83584237692	19604.773892397672	6228.2992241805632	35722.564217337196	15432.696192846684	26001.646655592172	7657.3601217432342	8353.0872304974637	8775.5708666240771	9088.6948004789792	4164.0809711152024	5438.3863337684897	8221.2947687853975	4472.5314134200325	6675.9268962278675	6492.7982817311631	5172.2598420263321	5505.5644687831063	6206.5910478856722	7546.7534013035383	3861.9862187252411	8594.3684872147805	6851.4630431324749	6904.5985633400769	6320.4097474212731	3335.1596121214625	2836.9274457132606	10098.487654397333	7036.8324183798686	11047.492936053466	8474.6032501558238	6415.1782987612805	11223.170233427494	28318.832460856895	4707.1079421147924	9811.1422135439716	7522.1192101358483	10921.769523295299	6239.7862494364526	16095.998270798005	13067.694763107735	13580.986361515468	15731.588517942098	12559.080081314196	12326.403479758063	14062.319029726212	8683.4751803525414	11561.585613686186	1666.2310261508451	19565.727430058778	18063.003061098745	7505.0836381583031	10872.552337691446	5965.2180703063686	2186.6347209696714	age(15 - 24 )	8734.4654196425345	9017.1842396486663	9616.4892383074966	10762.089456874004	7705.5603390212646	10353.104288870345	11763.017154265503	13644.864299931311	12039.109751927737	9565.9166920638145	5167.6289477066057	9347.4011070338602	8320.9827448256929	7508.5433119029121	5111.6768601902859	6877.5701087627904	9310.3517517865675	10644.884649979875	8103.979378377262	10431.684702277129	12422.165201923792	5260.1989974262715	7236.4700086517651	12233.217409944984	25011.387902853236	21135.653925922088	11683.271804022927	8176.9845260422107	9163.1998305169618	10378.687150868438	8565.3253264427276	12389.00767797946	12347.046235723652	14126.730497995643	14308.419217041397	10035.706174148727	14387.583587482763	11741.849764426008	12570.26380483701	14716.66347591906	17057.016918944279	5052.8684406809189	19964.141396208834	13809.132018221189	15783.526599193105	16185.538611851236	5142.0321464778035	29492.252531321275	12741.105890088926	21466.743673029396	9381.1708207809497	10233.518725033051	10751.111093221965	11134.724905928351	5101.4911510655238	6662.6657719303212	10072.05738893872	5479.3793844777847	8178.7991690146655	6492.7982817311631	5172.2598420263321	5505.5644687831063	6206.5910478856722	7546.7534013035383	3861.9862187252411	8594.3684872147805	6851.4630431324749	6904.5985633400769	6320.4097474212731	3335.1596121214625	3471.2324566003263	12356.395706027086	8610.1888574017648	13517.587875445319	10369.429046626679	7849.5398813202482	13732.544637012843	34650.604307731403	5759.5642391488691	12004.803062354264	9203.9803076724565	11299.476030834161	6455.5761786266603	16652.64463467223	13519.613597325	14050.656309832892	16275.632534296472	12993.409542789848	12752.686308646174	14548.634859527076	8983.7749693817605	10822.19751762058	1559.6719928835805	18314.457367626801	16907.835431949057	7025.1175082996015	10177.229391431982	5583.7296327343756	2046.7947598128874	age(25 - 54)	16054.883236906056	16574.550718085469	17676.137514127236	19781.873453489636	14163.64546360339	19030.114896731404	21621.685798967257	25080.722470567704	22129.173573556527	17038.814305254	9204.582568806738	16649.594265399563	14821.337503799568	13374.220089185063	9104.9206900896861	12250.330389328567	16583.601940303135	18960.672425919329	14434.811028234782	17587.096561184742	20942.908565625359	8868.3305083587002	12200.186301307074	20624.355699296055	42167.464482578449	35633.245931774924	19697.185568028646	13785.828516023468	15448.519086620325	17497.746366970423	12652.292418623996	18300.454675604677	18238.471222846772	20867.336425383091	21135.718385778146	14824.269283821111	21252.65623995028	17344.503692864197	18568.197631332125	23200.524496349146	26890.04471089158	7965.7456478956547	31473.068081581278	21769.819374228253	24882.412790273411	25516.176656842981	8106.3104399024032	46493.943985676669	20086.097626495208	33841.89040252984	16022.374508401019	17478.124285723701	18362.135346202675	19017.320534832001	8712.9851204288407	11379.360664203925	17202.359773494638	9358.3914256457902	13968.808991801629	14437.124649802154	11500.828582740189	12241.951321203018	13800.725776556899	16780.65678745952	8587.3569478410282	19110.091481722215	15234.637161843675	15352.787163627601	14053.808450832699	7415.9265324265043	5210.9922268289774	18549.343145630704	12925.561099239307	20292.517492018131	15566.521353498558	11783.679663390947	20615.209224028997	52017.268206623288	8646.2214373050774	18021.534490896098	13816.957071823788	18611.90236913988	10633.28540591405	27429.360023662983	22268.79615083649	23143.501764802062	26808.365529313851	21402.060519686092	21005.553874631074	23963.745829530591	14797.601426843539	14185.673817221505	2044.4090136849395	24006.484628796956	22162.692743536631	9208.4833360443863	13340.253333468623	7319.1204581654265	2682.9267148588933	age(55 - 64)	1674.4883244478954	1728.6884775720152	1843.5815104965811	2063.20504763494	1477.236465096445	1984.7983157066892	2255.0933501668164	2615.8631193992369	2308.0231872020895	2378.349201943854	1284.8142608137587	2324.0202354685921	2068.8244846375615	1866.8297632615452	1270.9030375640375	1709.9525226954349	2314.808749803236	2646.6102232594194	2014.8714971690488	2384.2753772963183	2839.2214171493097	1202.2758842111573	1653.9741904205914	2796.0353373484859	5716.6256487566652	4830.784353330002	2670.3392676842977	1868.9390469901412	2094.3493171700525	2372.1622085716967	1487.3328602464953	2151.2992820504742	2144.0128533916904	2453.0475699095737	2484.5970548238929	1742.6583345888102	2498.3436161079894	2038.9230214985166	2182.7736491435689	2702.0601531647599	3131.7618850191311	927.73436690241522	3665.5258881955328	2535.4323986060244	2897.9420756532854	2971.7536867072831	944.10531245923221	5414.9393660018513	2339.3369420450185	3941.4119098399819	2525.2827642250268	2754.7231520882528	2894.0519321789525	2997.3155191930773	1373.2515825311261	1793.4984192353768	2711.2599706882775	1474.9739219778762	2201.6207750762774	2065.2098978227714	1645.1769724495362	1751.1935132844817	1974.1739551492858	2400.4487964231294	1228.4090492396956	2733.6710760402138	2179.2929145908106	2196.19410226015	2010.3770673728131	1060.8376146772139	633.64521121692474	2255.5593913447101	1571.7198445733848	2467.5255637787714	1892.8548118277749	1432.8695695955007	2506.76416974622	6325.1855817429496	1051.3615392981251	2191.3790180197338	1680.1116372953484	1544.4058486769613	882.34441841766227	2276.0738373660861	1847.8529672158525	1920.4355780251005	2224.5440415371968	1775.9317013798095	1743.02978896286	1988.4989981841143	1227.8971669172715	1390.4798969655665	200.39299305282501	2353.1158761475854	2172.3873761358127	902.61563358151761	1307.6117722442598	717.4202643933188	262.98050484667425	age(65 	&	 above)	2276.8974158235578	2350.5964597546276	2506.8230789210097	2805.4577465166985	2008.6827963087919	2698.8436347882894	3066.3792314757852	3556.9384926419689	3138.3509540647206	2181.5491799520209	1178.5004047252962	2131.7157441534096	1897.6365431270592	1712.3561736958891	1165.7402862163092	1568.4599724019747	2123.2664764920528	2427.6125463347844	1848.1479753962576	1879.0399889231655	2237.5815440749811	947.50987476643218	1303.4919011625818	2203.5467292699082	4505.2548451422517	3807.1260829211205	2104.4860487803458	1472.9050342065325	1650.5501651403276	1869.4936384290597	1942.9220739674151	2810.2699634521618	2800.751607837271	3204.4476387616123	3245.6611373003147	2276.457029998488	3263.6184473778922	2663.4714067524019	2851.3853346133919	1635.471017337173	1895.5558003218555	561.52808703368407	2218.6261643440739	1534.6165404501196	1754.0321110548882	1798.707930162908	571.43689937201054	3277.4904671761969	1415.9262013540786	2385.6111931412624	2863.0268452069713	3123.1537502542583	3281.1170656345184	3398.1916467238702	1556.9171903076524	2033.3699630991453	3073.877583288292	1672.2443895897006	2496.0766656731817	2315.2320139536337	1844.3483150308589	1963.1996190113673	2213.1749159703713	2691.0562007253316	1377.1248917741507	3064.6196289974005	2443.126351932659	2462.0736612628848	2253.7609137970485	1189.2666259716264	605.93362507098891	2156.9156593728685	1502.9828777358632	2359.6117880293564	1810.0734568184382	1370.2050251298722	2397.1343485027896	6048.5624462175183	1005.3817143881732	2095.5421248163216	1606.6343071624765	1464.8420570349492	836.88831792204746	2158.8164048633757	1752.6563654970848	1821.4997080769313	2109.9412907311385	1684.4402971093107	1653.2334060537528	1886.0566770109551	1164.6390832794016	1648.4963127880155	237.5777678462309	2789.7583085218071	2575.493962424257	1070.1043194303713	1550.2512404580598	850.54423523325238	311.77897179308087	number of Woredas
Age category
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woreda	4042 - 54669	54670 - 105296	105297 - 155923	155924 - 206550	87	6	5	1	labor force	4042 - 54669	54670 - 105296	105297 - 155923	155924 - 206550	0	0	0	0	Labor force
Woredas
No. of Woredas	0 - 188 (Almost no frequency)	189 - 376 (Low frequency)	377 - 564 (Moderate frequency)	565 - 752 (High frequency)	70	25	3	1	frequency score
Number of Woredas
bus capacity 	0 .000 - 1.608 (Almost no capacity)	1.609 - 3.216 (Low capacity)	3.217 - 4.823 (Moderate capacity)	4.824 - 6.431 (High capacity)	0	0	0	0	No. of Woredas	0 .000 - 1.608 (Almost no capacity)	1.609 - 3.216 (Low capacity)	3.217 - 4.823 (Moderate capacity)	4.824 - 6.431 (High capacity)	85	12	1	1	Bus capacity
Number of Woredas

bus coverage 	0 .000 - 1.869 (Almost no coverage)	1.870 - 3.737 (Low coverage)	3.738 - 5.606 (Moderate coverage)	5.607 - 7.474 (High coverage)	0	0	0	0	No. of Woredas	49	33	14	3	Bus coverage
No. of Woredas

Sheger bus frequency score distribution acros the city woredas
woreda	0 - 95	96 - 191	192 - 286	287 - 381	71	13	13	2	Bus frequency
No.of Woredas
Sheger bus frequency score  distribution across the city woredas
No. of Woredas	0  - 95 (Almost no frequency)	192 - 286 (Moderate frequency)	287 - 381 (High frequency	96 - 191 (Low frequency)	71	13	2	13	bus frequency 	0  - 95 (Almost no frequency)	192 - 286 (Moderate frequency)	287 - 381 (High frequency	96 - 191 (Low frequency)	0	0	0	0	Bus frequency
No.of Woredas

No. of Woredas	0.000 - 1.040 (Almost no capacity)	1.041 - 2.079 (Low capacity)	2.080 - 3.119 (Moderate capacity)	3.120 - 4.158 (High capacity)	87	9	2	1	bus capacity 	0.000 - 1.040 (Almost no capacity)	1.041 - 2.079 (Low capacity)	2.080 - 3.119 (Moderate capacity)	3.120 - 4.158 (High capacity)	0	0	0	0	Bus capacity
No. of Woredas
No. of Woredas	0.000 - 1.316 (Almost no coverage)	1.317 -2.632 (Low coverage)	2.633 - 3.947 (Moderate coverage)	3.948 - 5.263 (High coverage)	63	25	3	8	Bus Coverage
Number  of Woredas
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 Addis Ababa City Periphery Woredas with Condominium Residential Neighborhoods
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 Addis Ababa City Overall Public Transit Availability Score  
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Condominium Sites and PublicTransit Routes
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 Addis Ababa City Periphery Woredas with Condominium Residential Neighborhoods
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 Addis Ababa City Gender (Female) Distribution Map
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 Addis Ababa City Age (0 - 14) Distribution Map
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 Addis Ababa City Age (15 - 24)  Distribution Map
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 Addis Ababa City Age (25 - 54)  Distribution Map
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 Addis Ababa City Age (55 - 64)  Distribution Map
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 Addis Ababa City Age (65  and above)  Distribution Map
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 Addis Ababa City Expenditure (1st quantile)
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 Addis Ababa City Expenditure (2nd quantile)
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 Addis Ababa City Expenditure (3rd quantile)
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 Addis Ababa City Expenditure (4th quantile)
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 Addis Ababa City Expenditure (5th quantile)
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 Addis Ababa City Labor Force Map
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Addis Ababa City Anbessa Bus Frequency Score 
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Addis Ababa City Anbessa Bus Capacity Score 
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